Node:MIPS insn, Next:MIPS option stack, Previous:MIPS autoextend, Up:MIPS-Dependent

#### Directive to mark data as an instruction

The `.insn` directive tells `as` that the following data is actually instructions. This makes a difference in MIPS 16 mode: when loading the address of a label which precedes instructions, `as` automatically adds 1 to the value, so that jumping to the loaded address will do the right thing.