Node:H8/300 Directives, Next:H8/300 Opcodes, Previous:H8/300 Floating Point, Up:H8/300-Dependent

#### H8/300 Machine Directives

`as` has only one machine-dependent directive for the H8/300:

`.h8300h`
  Recognize and emit additional instructions for the H8/300H variant, and also make `.int` emit 32-bit numbers rather than the usual (16-bit) for the H8/300 family.

On the H8/300 family (including the H8/300H) `.word` directives generate 16-bit numbers.