Node:H8/300, Next:i960, Up:Machine Dependent

### `ld` and the H8/300

For the H8/300, `ld` can perform these global optimizations when you specify the `--relax` command-line option.

relaxing address modes
  `ld` finds all `jsr` and `jmp` instructions whose targets are within eight bits, and turns them into eight-bit program-counter relative `bsr` and `bra` instructions, respectively.
synthesizing instructions
  `ld` finds all `mov.b` instructions which use the sixteen-bit absolute address form, but refer to the top page of memory, and changes them to use the eight-bit address form. (That is: the linker turns `mov.b @`aa`:16` into `mov.b @`aa`:8` whenever the address aa is in the top page of memory).