##### Synopsis

    #include <__armlib.h>
    void __ARMLIB_enableFIQ(void);

##### Description

__ARMLIB_enableFIQ globally enables the ARM's FIQ interrupts by clearing the F bit of the CPSR register.

##### Portability

__ARMLIB_enableFIQ is an ARM specific extension provided by CrossWorks C.

##### See also

__ARMLIB_disableFIQ __ARMLIB_enableIRQ __ARMLIB_disableIRQ __ARMLIB_isrEnableIRQ __ARMLIB_isrDisableIRQ