CrossStudio's New Project Wizard simplifies the creation of projects for the LPD SDKLH79524-10 by creating a project with the appropriate project settings, memory map files and startup files. See Creating a New Project for more information on creating projects.

##### To create a new LPD SDKLH79524-10 project

- Select the File | New | New Project menu item.
- Select Logic Product Development | SDKLH79524-10 Projects from the Project Type list.
- Select the required project template type from the Templates list.
- Set the required project name and location directory.
- Click OK.

CrossStudio for ARM supports the LPD SDKLH79524-10 running applications from both RAM and FLASH.

Warning: Downloading to FLASH will erase the and re-program the FLASH memory thus removing the boot loader firmware shipped with the board.

##### To build and debug an application running from RAM

- Select the project to work on by using the Project | Set Active Project menu option.
- Select the RAM configuration you require by using the Build | Set Active Build Configuration menu option.
- Build the project by using the Build | Build Project menu option.
- Connect to the appropriate target in the target window.
- Download and start debugging the current project by using Debug | Start Debugging.

##### To build and debug an application running from FLASH

- Select the project to work on by using the Project | Set Active Project menu option.
- Select the FLASH configuration you require by using the Build | Set Active Build Configuration menu option.
- Build the project by using the Build | Build Project menu option.
- Connect to the appropriate target in the target window.
- Download and start debugging the current project by using Debug | Start Debugging.

The following sections describe the LPD SDKLH79524-10 support in more detail. See ARM Target Support for more information.

### Memory Map Files

The default memory map file $(StudioDir)/targets/LPD_SDKLH79524_10/SDKLH79524_10_MemoryMap.xml has been provided. This file is used to describe the memory layout of the target and is used for linking and debugging. The placement of program sections within the memory map for both RAM and FLASH configurations is described by the non-target-specific default memory maps $(StudioDir)/targets/flash_placement.xml and $(StudioDir)/targets/sram_placement.xml.

The memory segment layout for both configurations is the same and is described in the following table:

Type | Description | Start Address | End Address
RAM | External SDRAM | 0x20000000 | 0x21FFFFFF
FLASH | External FLASH | 0x44000000 | 0x44FFFFFF
RAM | Internal SRAM | 0x60000000 | 0x60003FFF

### Target Startup Code

The default startup code is in $(StudioDir)/targets/LPD_SDKLH79524_10/SDKLH79524_10_Startup.s. It contains the exception vectors and the default exception handlers. The FLASH version of the code (specified by defining __FLASH_BUILD) is also responsible for configuring memory to match the above memory map and copying the exception vectors into RAM.