int libmem_register_sst39xFx00A_16_driver | ( | libmem_driver_handle_t * | h,
|  | uint8_t * | start,
|  | size_t | size,
|  | const libmem_geometry_t * | geometry,
|  | const libmem_flash_info_t * | flash_info
| ) |
  | Register a LIBMEM driver for a 16 bit SST39xFx00A FLASH chip. Parameters:
  | h | A pointer to the LIBMEM handle structure to use for this LIBMEM driver.
  | start | The start address of the FLASH memory.
  | size | The size of the FLASH memory.
  | geometry | A NULL terminated description of the FLASH's geometry.
  | flash_info | A pointer to the FLASH information structure or NULL if not required.
Returns: The LIBMEM status result. Example:
        libmem_driver_handle_t flash1_handle;
        uint8_t *flash1_start = (uint8_t *)0x10000000;
        libmem_flash_info_t flash1_info;
        const int flash1_max_geometry_regions = 4;
        libmem_geometry_t flash1_geometry[flash1_max_geometry_regions];
        size_t size;
        int res;

        // Get CFI FLASH information and geometry
        res = libmem_cfi_get_info(flash1_start, &size, flash1_geometry, flash1_max_geometry_regions, &flash1_info);

        if (res == LIBMEM_STATUS_SUCCESS)
          {
            res = libmem_register_sst39xFx00A_16_driver(&flash1_handle, flash1_start, size, flash1_geometry, &flash1_info)

            if (res == LIBMEM_STATUS_SUCCESS)
              printf("libmem_register_sst39xFx00A_16_driver : success\n");
            else
              printf("libmem_register_sst39xFx00A_16_driver : failed (%d)\n", res);
          }
        else
          printf("libmem_cfi_get_info : failed (%d)\n", res);