#### 8.12.10 Writing 16-bit Code

While `as` normally writes only “pure” 32-bit i386 code or 64-bit x86-64 code depending on the default configuration, it also supports writing code to run in real mode or in 16-bit protected mode code segments. To do this, put a .code16 or .code16gcc directive before the assembly language instructions to be run in 16-bit mode. You can switch `as` back to writing normal 32-bit code with the .code32 directive.

.code16gcc provides experimental support for generating 16-bit code from gcc, and differs from .code16 in that call, ret, enter, leave, push, pop, pusha, popa, pushf, and popf instructions default to 32-bit size. This is so that the stack pointer is manipulated in the same way over function calls, allowing access to function parameters at the same stack offsets as in 32-bit mode. .code16gcc also automatically adds address size prefixes where necessary to use the 32-bit addressing modes that gcc generates.

The code which `as` generates in 16-bit mode will not necessarily run on a 16-bit pre-80386 processor. To write code that runs on such a processor, you must refrain from using any 32-bit constructs which require `as` to output address or operand size prefixes.

Note that writing 16-bit code instructions by explicitly specifying a prefix or an instruction mnemonic suffix within a 32-bit code section generates different machine instructions than those generated for a 16-bit code segment. In a 32-bit code section, the following code generates the machine opcode bytes 66 6a 04, which pushes the value 4 onto the stack, decrementing %esp by 2.

                 pushw $4

The same code in a 16-bit code section would generate the machine opcode bytes 6a 04 (ie. without the operand size prefix), which is correct since the processor default operand size is assumed to be 16 bits in a 16-bit code section.