int libmem_register_cfi_0001_8_driver | ( | libmem_driver_handle_t * | h,
|  | uint8_t * | start,
|  | size_t | size,
|  | const libmem_geometry_t * | geometry,
|  | const libmem_flash_info_t * | flash_info
| ) |
  | Register an 8 bit CFI command set 1 (Intel Extended) LIBMEM driver. Parameters:
  | h | A pointer to the LIBMEM handle structure to use for this LIBMEM driver.
  | start | The start address of the FLASH memory.
  | size | The size of the FLASH memory.
  | geometry | A NULL terminated description of the FLASH's geometry.
  | flash_info | A pointer to the FLASH information structure or NULL if not required.
Returns: The LIBMEM status result. Example:
        libmem_driver_handle_t flash1_handle;
        uint8_t *flash1_start = (uint8_t *)0x10000000;
        libmem_geometry_t flash1_geometry[] =
          {
            { 8,  0x00002000 }, // 8 x 8KB sectors
            { 31, 0x00010000 }, // 31 x 64KB sectors
            { 0, 0 },           // NULL terminator
          };
        int res;

        res = libmem_register_cfi_0001_8_driver(&flash1_handle,
                                                flash1_start,
                                                libmem_get_geometry_size(flash1_geometry),
                                                flash1_geometry,
                                                0);

        if (res == LIBMEM_STATUS_SUCCESS)
          printf("libmem_register_cfi_0001_8_driver : success\n");
        else
          printf("libmem_register_cfi_0001_8_driver : failed (%d)\n", res);