int libmem_register_st_m28w320cb_driver | ( | libmem_driver_handle_t * | h,
|  | uint8_t * | start
| ) |
  | Register an LIBMEM driver for an ST M28W320CB FLASH chip. Parameters:
  | h | A pointer to the LIBMEM handle structure to use for this LIBMEM driver.
  | start | The start address of the FLASH memory.
Returns: The LIBMEM status result. Example:
        libmem_driver_handle_t flash1_handle;
        uint8_t *flash1_start = (uint8_t *)0x10000000;
        int res;

        res = libmem_register_st_m28w320cb_driver(&flash1_handle, flash1_start);

        if (res == LIBMEM_STATUS_SUCCESS)
          printf("libmem_register_st_m28w320cb_driver : success\n");
        else
          printf("libmem_register_st_m28w320cb_driver : failed (%d)\n", res);