This documentation was generated automatically from the AVR Studio part description file `AT90S8515.pdf`.

## ANALOG COMPARATOR

The analog comparator compares the input values on the positive input PB2 (AIN0) and negative input PB3 (AIN1). When the voltage on the positive input PB2 (AIN0) is higher than the voltage on the negative input PB3 (AIN1), the Analog Com-parator Output, ACO is set (one). The comparator?s output can be set to trigger the Timer/Counter1 Input Capture function. In addition, the comparator can trigger a separate interrupt, exclusive to the Analog Comparator. The user can select Inter-rupt triggering on comparator output rise, fall or toggle

### ACSR - Analog Comparator Control And Status Register

`sfrb ACSR = $08;`

##### ACIS0 - Analog Comparator Interrupt Mode Select bit 0

`#define ACIS0_BIT 0`

`#define ACIS0_MASK 1`

These bits determine which comparator events that trigger the Analog Comparator interrupt.

##### ACIS1 - Analog Comparator Interrupt Mode Select bit 1

`#define ACIS1_BIT 1`

`#define ACIS1_MASK 2`

These bits determine which comparator events that trigger the Analog Comparator interrupt.

##### ACIC - Analog Comparator Input Capture Enable

`#define ACIC_BIT 2`

`#define ACIC_MASK 4`

When set (one), this bit enables the Input Capture function in Timer/Counter1 to be triggered by the analog comparator. The comparator output is in this case directly connected to the Input Capture front-end logic, making the comparator utilize the noise canceler and edge select features of the Timer/Counter1 Input Capture interrupt. When cleared (zero), no connection between the analog comparator and the Input Capture function is given. To make the comparator trigger the Timer/Counter1 Input Capture interrupt, the TICIE1 bit in the Timer Interrupt Mask Register (TIMSK) must be set (one)

##### ACIE - Analog Comparator Interrupt Enable

`#define ACIE_BIT 3`

`#define ACIE_MASK 8`

When the ACIE bit is set (one) and the I-bit in the Status Register is set (one), the analog comparator interrupt is activated. When Cleared (Zero), the interrupt is disabled.

##### ACI - Analog Comparator Interrupt Flag

`#define ACI_BIT 4`

`#define ACI_MASK 16`

This bit is set (one) when a comparator output event triggers the interrupt mode defined by ACI1 and ACI0. The Analog Comparator Interrupt routine is executed if the ACIE bit is set (one) and the I-bit in SREG is set (one). ACI is cleared by hardware when executing the corresponding interrupt handling vector. Alternatively, ACI is cleared by writing a logic one to the flag. Observe however, that if another bit in this register is modified using the SBI or CBI instruction, ACI will be cleared if it has become set before the operation

##### ACO - Analog Comparator Output

`#define ACO_BIT 5`

`#define ACO_MASK 32`

When this bit is set(one), the power to the analog comparator is switched off. This bit can be set at any time to turn off the analog comparator. This will reduce power consumption in active and idle mode. When changing the ACD bit, the Analog Comparator Interrupt must be disabled by clearing the ACIE bit in ACSR. Otherwise an interrupt can occur when the bit is changed.

##### ACD - Analog Comparator Disable

`#define ACD_BIT 7`

`#define ACD_MASK 128`

When this bit is set(one), the power to the analog comparator is switched off. This bit can be set at any time to turn off the analog comparator. This will reduce power consumption in active and idle mode. When changing the ACD bit, the Analog Comparator Interrupt must be disabled by clearing the ACIE bit in ACSR. Otherwise an interrupt can occur when the bit is changed.

## SPI

The Serial Peripheral Interface(SPI) allows high-speed synchronous data transfer between the AT90S4414/8515 and peripheral devices or between several AVR devices. The AT90S4414/8515 SPI features include the following: ? Full-duplex, 3-wire Synchronous Data Transfer ? Master or Slave Operation ? LSB First or MSB First Data Transfer ? Four Programmable Bit Rates ? End of Transmission Interrupt Flag ? Write Collision Flag Protection ? Wakeup from Idle Mode (Slave Mode Only)

### SPCR - SPI Control Register

`sfrb SPCR = $0D;`

##### SPR0 - SPI Clock Rate Select 0

`#define SPR0_BIT 0`

`#define SPR0_MASK 1`

These two bits control the SCK rate of the device configured as a master. SPR1 and SPR0 have no effect on the slave.

##### SPR1 - SPI Clock Rate Select 1

`#define SPR1_BIT 1`

`#define SPR1_MASK 2`

These two bits control the SCK rate of the device configured as a master. SPR1 and SPR0 have no effect on the slave.

##### CPHA - Clock Phase

`#define CPHA_BIT 2`

`#define CPHA_MASK 4`

Refer to Figure 36 or Figure 37 for the functionality of this bit.

##### CPOL - Clock polarity

`#define CPOL_BIT 3`

`#define CPOL_MASK 8`

When this bit is set (one), SCK is high when idle. When CPOL is cleared (zero), SCK is low when idle. Refer to Figure 36 and Figure 37 for additional information.

##### MSTR - Master/Slave Select

`#define MSTR_BIT 4`

`#define MSTR_MASK 16`

This bit selects Master SPI mode when set (one), and Slave SPI mode when cleared (zero). If SS is configured as an input and is driven low while MSTR is set, MSTR will be cleared, and SPIF in SPSR will become set. The user will then have to set MSTR to re-enable SPI master mode.

##### DORD - Data Order

`#define DORD_BIT 5`

`#define DORD_MASK 32`

When the DORD bit is set (one), the LSB of the data word is transmitted first. When the DORD bit is cleared (zero), the MSB of the data word is transmitted first.

##### SPE - SPI Enable

`#define SPE_BIT 6`

`#define SPE_MASK 64`

When the SPE bit is set (one), the SPI is enabled. This bit must be set to enable any SPI operations.

##### SPIE - SPI Interrupt Enable

`#define SPIE_BIT 7`

`#define SPIE_MASK 128`

This bit causes the SPI interrupt to be executed if SPIF bit in the SPSR register is set and the global interrupts are enabled.

### SPSR - SPI Status Register

`sfrb SPSR = $0E;`

##### WCOL - Write Collision Flag

`#define WCOL_BIT 6`

`#define WCOL_MASK 64`

The WCOL bit is set if the SPI data register (SPDR) is written during a data transfer. The WCOL bit (and the SPIF bit) are cleared (zero) by first reading the SPI Status Register when WCOL is set (one), and then accessing the SPI Data Register.

##### SPIF - SPI Interrupt Flag

`#define SPIF_BIT 7`

`#define SPIF_MASK 128`

When a serial transfer is complete, the SPIF bit is set (one) and an interrupt is generated if SPIE in SPCR is set (one) and global interrupts are enabled. If SS is an input and is driven low when the SPI is in master mode, this will also set the SPIF flag. SPIF is cleared by hardware when executing the corresponding interrupt handling vector. Alternatively, the SPIF bit is cleared by first reading the SPI status register when SPIF is set (one), then accessing the SPI Data Register (SPDR).

### SPDR - SPI Data Register

`sfrb SPDR = $0F;`

##### SPDR0 - SPI Data Register bit 0

`#define SPDR0_BIT 0`

`#define SPDR0_MASK 1`

##### SPDR1 - SPI Data Register bit 1

`#define SPDR1_BIT 1`

`#define SPDR1_MASK 2`

##### SPDR2 - SPI Data Register bit 2

`#define SPDR2_BIT 2`

`#define SPDR2_MASK 4`

##### SPDR3 - SPI Data Register bit 3

`#define SPDR3_BIT 3`

`#define SPDR3_MASK 8`

##### SPDR4 - SPI Data Register bit 4

`#define SPDR4_BIT 4`

`#define SPDR4_MASK 16`

##### SPDR5 - SPI Data Register bit 5

`#define SPDR5_BIT 5`

`#define SPDR5_MASK 32`

##### SPDR6 - SPI Data Register bit 6

`#define SPDR6_BIT 6`

`#define SPDR6_MASK 64`

##### SPDR7 - SPI Data Register bit 7

`#define SPDR7_BIT 7`

`#define SPDR7_MASK 128`

## UART

### UDR - UART I/O Data Register

`sfrb UDR = $0C;`

##### UDR0 - UART I/O Data Register bit 0

`#define UDR0_BIT 0`

`#define UDR0_MASK 1`

##### UDR1 - UART I/O Data Register bit 1

`#define UDR1_BIT 1`

`#define UDR1_MASK 2`

##### UDR2 - UART I/O Data Register bit 2

`#define UDR2_BIT 2`

`#define UDR2_MASK 4`

##### UDR3 - UART I/O Data Register bit 3

`#define UDR3_BIT 3`

`#define UDR3_MASK 8`

##### UDR4 - UART I/O Data Register bit 4

`#define UDR4_BIT 4`

`#define UDR4_MASK 16`

##### UDR5 - UART I/O Data Register bit 5

`#define UDR5_BIT 5`

`#define UDR5_MASK 32`

##### UDR6 - UART I/O Data Register bit 6

`#define UDR6_BIT 6`

`#define UDR6_MASK 64`

##### UDR7 - UART I/O Data Register bit 7

`#define UDR7_BIT 7`

`#define UDR7_MASK 128`

### USR - UART Status Register

`sfrb USR = $0B;`

##### OR - Overrun

`#define OR_BIT 3`

`#define OR_MASK 8`

This bit is set if an Overrun condition is detected, i.e. when a character already present in the UDR register is not read before the next character has been shifted into the Receiver Shift register. The OR bit is buffered, which means that it will be set once the valid data still in UDRE is read. The OR bit is cleared (zero) when data is received and transferred to UDR.

##### FE - Framing Error

`#define FE_BIT 4`

`#define FE_MASK 16`

This bit is set if a Framing Error condition is detected, i.e. when the stop bit of an incoming character is zero. The FE bit is cleared when the stop bit of received data is one.

##### UDRE - UART Data Register Empty

`#define UDRE_BIT 5`

`#define UDRE_MASK 32`

This bit is set (one) when a character written to UDR is transferred to the Transmit shift register. Setting of this bit indicates that the transmitter is ready to receive a new character for transmission. When the UDRIE bit in UCR is set, the UART Transmit Complete interrupt to be executed as long as UDRE is set. UDRE is cleared by writing UDR. When interrupt-driven data transmittal is used, the UART Data Register Empty Interrupt routine must write UDR in order to clear UDRE, otherwise a new interrupt will occur once the interrupt routine terminates. UDRE is set (one) during reset to indicate that the transmitter is ready

##### TXC - UART Transmit Complete

`#define TXC_BIT 6`

`#define TXC_MASK 64`

This bit is set (one) when the entire character (including the stop bit) in the Transmit Shift register has been shifted out and no new data has been written to UDR. This flag is especially useful in half-duplex communications interfaces, where a transmitting application must enter receive mode and free the communications bus immediately after completing the transmission. When the TXCIE bit in UCR is set, setting of TXC causes the UART Transmit Complete interrupt to be executed. TXC is cleared by hardware when executing the corresponding interrupt handling vector. Alternatively, the TXC bit is cleared (zero) by writing a logical one to the bit

##### RXC - UART Receive Complete

`#define RXC_BIT 7`

`#define RXC_MASK 128`

This bit is set (one) when a received character is transferred from the Receiver Shift register to UDR. The bit is set regard-less of any detected framing errors. When the RXCIE bit in UCR is set, the UART Receive Complete interrupt will be executed when RXC is set(one). RXC is cleared by reading UDR. When interrupt-driven data reception is used, the UART Receive Complete Interrupt routine must read UDR in order to clear RXC, otherwise a new interrupt will occur once the interrupt routine terminates.

### UCR - UART Control Register

`sfrb UCR = $0A;`

##### TXB8 - Transmit Data Bit 8

`#define TXB8_BIT 0`

`#define TXB8_MASK 1`

When CHR9 is set (one), TXB8 is the 9th data bit in the character to be transmitted.

##### RXB8 - Receive Data Bit 8

`#define RXB8_BIT 1`

`#define RXB8_MASK 2`

When CHR9 is set (one), RXB8 is the 9th data bit of the received character.

##### CHR9 - 9-bit Characters

`#define CHR9_BIT 2`

`#define CHR9_MASK 4`

When this bit is set (one) transmitted and received characters are 9 bit long plus start and stop bits. The 9th bit is read and written by using the RXB8 and TXB8 bits in UCR, respectively. The 9th data bit can be used as an extra stop bit or a parity bit.

##### TXEN - Transmitter Enable

`#define TXEN_BIT 3`

`#define TXEN_MASK 8`

This bit enables the UART transmitter when set (one). When disabling the transmitter while transmitting a character, the transmitter is not disabled before the character in the shift register plus any following character in UDR has been completely transmitted.

##### RXEN - Receiver Enable

`#define RXEN_BIT 4`

`#define RXEN_MASK 16`

This bit enables the UART receiver when set (one). When the receiver is disabled, the TXC, OR and FE status flags cannot become set. If these flags are set, turning off RXEN does not cause them to be cleared.

##### UDRIE - UART Data Register Empty Interrupt Enable

`#define UDRIE_BIT 5`

`#define UDRIE_MASK 32`

When this bit is set (one), a setting of the UDRE bit in USR will cause the UART Data Register Empty interrupt routine to be executed provided that global interrupts are enabled.

##### TXCIE - TX Complete Interrupt Enable

`#define TXCIE_BIT 6`

`#define TXCIE_MASK 64`

When this bit is set (one), a setting of the TXC bit in USR will cause the Transmit Complete interrupt routine to be executed provided that global interrupts are enabled.

##### RXCIE - RX Complete Interrupt Enable

`#define RXCIE_BIT 7`

`#define RXCIE_MASK 128`

When this bit is set (one), a setting of the RXC bit in USR will cause the Receive Complete interrupt routine to be executed provided that global interrupts are enabled.

### UBRR - UART BAUD Rate Register

`sfrb UBRR = $09;`

##### UBRR0 - UART Baud Rate Register bit 0

`#define UBRR0_BIT 0`

`#define UBRR0_MASK 1`

##### UBRR1 - UART Baud Rate Register bit 1

`#define UBRR1_BIT 1`

`#define UBRR1_MASK 2`

##### UBRR2 - UART Baud Rate Register bit 2

`#define UBRR2_BIT 2`

`#define UBRR2_MASK 4`

##### UBRR3 - UART Baud Rate Register bit 3

`#define UBRR3_BIT 3`

`#define UBRR3_MASK 8`

##### UBRR4 - UART Baud Rate Register bit 4

`#define UBRR4_BIT 4`

`#define UBRR4_MASK 16`

##### UBRR5 - UART Baud Rate Register bit 5

`#define UBRR5_BIT 5`

`#define UBRR5_MASK 32`

##### UBRR6 - UART Baud Rate Register bit 6

`#define UBRR6_BIT 6`

`#define UBRR6_MASK 64`

##### UBRR7 - UART Baud Rate Register bit 7

`#define UBRR7_BIT 7`

`#define UBRR7_MASK 128`

## EXTERNAL INTERRUPT

### GIMSK - General Interrupt Mask Register

`sfrb GIMSK = $3B;`

##### INT0 - External Interrupt Request 0 Enable

`#define INT0_BIT 6`

`#define INT0_MASK 64`

When the INT0 bit is set (one) and the I-bit in the Status Register (SREG) is set (one), the external pin interrupt is enabled. The Interrupt Sense Control0 bits 1/0 (ISC01 and ISC00) in the MCU general Control Register (MCUCR) defines whether the external interrupt is activated on rising or falling edge of the INT0 pin or level sensed. Activity on the pin will cause an interrupt request even if INT0 is configured as an output. The corresponding interrupt of External Interrupt Request 0 is executed from program memory address $001. See also ?External Interrupts.? ? Bits 5..0 - Res: Reserved bits

##### INT1 - External Interrupt Request 1 Enable

`#define INT1_BIT 7`

`#define INT1_MASK 128`

When the INT1 bit is set (one) and the I-bit in the Status Register (SREG) is set (one), the external pin interrupt is enabled. The Interrupt Sense Control1 bits 1/0 (ISC11 and ISC10) in the MCU general Control Register (MCUCR) defines whether the external interrupt is activated on rising or falling edge of the INT1 pin or level sensed. Activity on the pin will cause an interrupt request even if INT1 is configured as an output. The corresponding interrupt of External Interrupt Request 1 is executed from program memory address $002. See also ?External Interrupts?.

### GIFR - General Interrupt Flag register

`sfrb GIFR = $3A;`

##### INTF0 - External Interrupt Flag 0

`#define INTF0_BIT 6`

`#define INTF0_MASK 64`

When an event on the INT0 pin triggers an interrupt request, INTF0 becomes set (one). If the I-bit in SREG and the INT0 bit in GIMSK are set (one), the MCU will jump to the interrupt vector at address $001. The flag is cleared when the interrupt routine is executed. Alternatively, the flag can be cleared by writing a logical one to it.

##### INTF1 - External Interrupt Flag 1

`#define INTF1_BIT 7`

`#define INTF1_MASK 128`

When an event on the INT1 pin triggers an interrupt request, INTF1 becomes set (one). If the I-bit in SREG and the INT1 bit in GIMSK are set (one), the MCU will jump to the interrupt vector at address $002. The flag is cleared when the interrupt routine is executed. Alternatively, the flag can be cleared by writing a logical one to it.

## PORTA

### PORTA - Port A Data Register

`sfrb PORTA = $1B;`

##### PORTA0 - Port A Data Register bit 0

`#define PORTA0_BIT 0`

`#define PORTA0_MASK 1`

##### PORTA1 - Port A Data Register bit 1

`#define PORTA1_BIT 1`

`#define PORTA1_MASK 2`

##### PORTA2 - Port A Data Register bit 2

`#define PORTA2_BIT 2`

`#define PORTA2_MASK 4`

##### PORTA3 - Port A Data Register bit 3

`#define PORTA3_BIT 3`

`#define PORTA3_MASK 8`

##### PORTA4 - Port A Data Register bit 4

`#define PORTA4_BIT 4`

`#define PORTA4_MASK 16`

##### PORTA5 - Port A Data Register bit 5

`#define PORTA5_BIT 5`

`#define PORTA5_MASK 32`

##### PORTA6 - Port A Data Register bit 6

`#define PORTA6_BIT 6`

`#define PORTA6_MASK 64`

##### PORTA7 - Port A Data Register bit 7

`#define PORTA7_BIT 7`

`#define PORTA7_MASK 128`

### DDRA - Port A Data Direction Register

`sfrb DDRA = $1A;`

##### DDA0 - Data Direction Register, Port A, bit 0

`#define DDA0_BIT 0`

`#define DDA0_MASK 1`

##### DDA1 - Data Direction Register, Port A, bit 1

`#define DDA1_BIT 1`

`#define DDA1_MASK 2`

##### DDA2 - Data Direction Register, Port A, bit 2

`#define DDA2_BIT 2`

`#define DDA2_MASK 4`

##### DDA3 - Data Direction Register, Port A, bit 3

`#define DDA3_BIT 3`

`#define DDA3_MASK 8`

##### DDA4 - Data Direction Register, Port A, bit 4

`#define DDA4_BIT 4`

`#define DDA4_MASK 16`

##### DDA5 - Data Direction Register, Port A, bit 5

`#define DDA5_BIT 5`

`#define DDA5_MASK 32`

##### DDA6 - Data Direction Register, Port A, bit 6

`#define DDA6_BIT 6`

`#define DDA6_MASK 64`

##### DDA7 - Data Direction Register, Port A, bit 7

`#define DDA7_BIT 7`

`#define DDA7_MASK 128`

### PINA - Port A Input Pins

`sfrb PINA = $19;`

##### PINA0 - Input Pins, Port A bit 0

`#define PINA0_BIT 0`

`#define PINA0_MASK 1`

##### PINA1 - Input Pins, Port A bit 1

`#define PINA1_BIT 1`

`#define PINA1_MASK 2`

##### PINA2 - Input Pins, Port A bit 2

`#define PINA2_BIT 2`

`#define PINA2_MASK 4`

##### PINA3 - Input Pins, Port A bit 3

`#define PINA3_BIT 3`

`#define PINA3_MASK 8`

##### PINA4 - Input Pins, Port A bit 4

`#define PINA4_BIT 4`

`#define PINA4_MASK 16`

##### PINA5 - Input Pins, Port A bit 5

`#define PINA5_BIT 5`

`#define PINA5_MASK 32`

##### PINA6 - Input Pins, Port A bit 6

`#define PINA6_BIT 6`

`#define PINA6_MASK 64`

##### PINA7 - Input Pins, Port A bit 7

`#define PINA7_BIT 7`

`#define PINA7_MASK 128`

## PORTB

### PORTB - Port B Data Register

`sfrb PORTB = $18;`

##### PORTB0 - Port B Data Register bit 0

`#define PORTB0_BIT 0`

`#define PORTB0_MASK 1`

##### PORTB1 - Port B Data Register bit 1

`#define PORTB1_BIT 1`

`#define PORTB1_MASK 2`

##### PORTB2 - Port B Data Register bit 2

`#define PORTB2_BIT 2`

`#define PORTB2_MASK 4`

##### PORTB3 - Port B Data Register bit 3

`#define PORTB3_BIT 3`

`#define PORTB3_MASK 8`

##### PORTB4 - Port B Data Register bit 4

`#define PORTB4_BIT 4`

`#define PORTB4_MASK 16`

##### PORTB5 - Port B Data Register bit 5

`#define PORTB5_BIT 5`

`#define PORTB5_MASK 32`

##### PORTB6 - Port B Data Register bit 6

`#define PORTB6_BIT 6`

`#define PORTB6_MASK 64`

##### PORTB7 - Port B Data Register bit 7

`#define PORTB7_BIT 7`

`#define PORTB7_MASK 128`

### DDRB - Port B Data Direction Register

`sfrb DDRB = $17;`

##### DDB0 - Port B Data Direction Register bit 0

`#define DDB0_BIT 0`

`#define DDB0_MASK 1`

##### DDB1 - Port B Data Direction Register bit 1

`#define DDB1_BIT 1`

`#define DDB1_MASK 2`

##### DDB2 - Port B Data Direction Register bit 2

`#define DDB2_BIT 2`

`#define DDB2_MASK 4`

##### DDB3 - Port B Data Direction Register bit 3

`#define DDB3_BIT 3`

`#define DDB3_MASK 8`

##### DDB4 - Port B Data Direction Register bit 4

`#define DDB4_BIT 4`

`#define DDB4_MASK 16`

##### DDB5 - Port B Data Direction Register bit 5

`#define DDB5_BIT 5`

`#define DDB5_MASK 32`

##### DDB6 - Port B Data Direction Register bit 6

`#define DDB6_BIT 6`

`#define DDB6_MASK 64`

##### DDB7 - Port B Data Direction Register bit 7

`#define DDB7_BIT 7`

`#define DDB7_MASK 128`

### PINB - Port B Input Pins

`sfrb PINB = $16;`

##### PINB0 - Port B Input Pins bit 0

`#define PINB0_BIT 0`

`#define PINB0_MASK 1`

##### PINB1 - Port B Input Pins bit 1

`#define PINB1_BIT 1`

`#define PINB1_MASK 2`

##### PINB2 - Port B Input Pins bit 2

`#define PINB2_BIT 2`

`#define PINB2_MASK 4`

##### PINB3 - Port B Input Pins bit 3

`#define PINB3_BIT 3`

`#define PINB3_MASK 8`

##### PINB4 - Port B Input Pins bit 4

`#define PINB4_BIT 4`

`#define PINB4_MASK 16`

##### PINB5 - Port B Input Pins bit 5

`#define PINB5_BIT 5`

`#define PINB5_MASK 32`

##### PINB6 - Port B Input Pins bit 6

`#define PINB6_BIT 6`

`#define PINB6_MASK 64`

##### PINB7 - Port B Input Pins bit 7

`#define PINB7_BIT 7`

`#define PINB7_MASK 128`

## PORTC

### PORTC - Port C Data Register

`sfrb PORTC = $15;`

##### PORTC0 - Port C Data Register bit 0

`#define PORTC0_BIT 0`

`#define PORTC0_MASK 1`

##### PORTC1 - Port C Data Register bit 1

`#define PORTC1_BIT 1`

`#define PORTC1_MASK 2`

##### PORTC2 - Port C Data Register bit 2

`#define PORTC2_BIT 2`

`#define PORTC2_MASK 4`

##### PORTC3 - Port C Data Register bit 3

`#define PORTC3_BIT 3`

`#define PORTC3_MASK 8`

##### PORTC4 - Port C Data Register bit 4

`#define PORTC4_BIT 4`

`#define PORTC4_MASK 16`

##### PORTC5 - Port C Data Register bit 5

`#define PORTC5_BIT 5`

`#define PORTC5_MASK 32`

##### PORTC6 - Port C Data Register bit 6

`#define PORTC6_BIT 6`

`#define PORTC6_MASK 64`

##### PORTC7 - Port C Data Register bit 7

`#define PORTC7_BIT 7`

`#define PORTC7_MASK 128`

### DDRC - Port C Data Direction Register

`sfrb DDRC = $14;`

##### DDC0 - Port C Data Direction Register bit 0

`#define DDC0_BIT 0`

`#define DDC0_MASK 1`

##### DDC1 - Port C Data Direction Register bit 1

`#define DDC1_BIT 1`

`#define DDC1_MASK 2`

##### DDC2 - Port C Data Direction Register bit 2

`#define DDC2_BIT 2`

`#define DDC2_MASK 4`

##### DDC3 - Port C Data Direction Register bit 3

`#define DDC3_BIT 3`

`#define DDC3_MASK 8`

##### DDC4 - Port C Data Direction Register bit 4

`#define DDC4_BIT 4`

`#define DDC4_MASK 16`

##### DDC5 - Port C Data Direction Register bit 5

`#define DDC5_BIT 5`

`#define DDC5_MASK 32`

##### DDC6 - Port C Data Direction Register bit 6

`#define DDC6_BIT 6`

`#define DDC6_MASK 64`

##### DDC7 - Port C Data Direction Register bit 7

`#define DDC7_BIT 7`

`#define DDC7_MASK 128`

### PINC - Port C Input Pins

`sfrb PINC = $13;`

##### PINC0 - Port C Input Pins bit 0

`#define PINC0_BIT 0`

`#define PINC0_MASK 1`

##### PINC1 - Port C Input Pins bit 1

`#define PINC1_BIT 1`

`#define PINC1_MASK 2`

##### PINC2 - Port C Input Pins bit 2

`#define PINC2_BIT 2`

`#define PINC2_MASK 4`

##### PINC3 - Port C Input Pins bit 3

`#define PINC3_BIT 3`

`#define PINC3_MASK 8`

##### PINC4 - Port C Input Pins bit 4

`#define PINC4_BIT 4`

`#define PINC4_MASK 16`

##### PINC5 - Port C Input Pins bit 5

`#define PINC5_BIT 5`

`#define PINC5_MASK 32`

##### PINC6 - Port C Input Pins bit 6

`#define PINC6_BIT 6`

`#define PINC6_MASK 64`

##### PINC7 - Port C Input Pins bit 7

`#define PINC7_BIT 7`

`#define PINC7_MASK 128`

## PORTD

### PORTD - Port D Data Register

`sfrb PORTD = $12;`

##### PORTD0 - Port D Data Register bit 0

`#define PORTD0_BIT 0`

`#define PORTD0_MASK 1`

##### PORTD1 - Port D Data Register bit 1

`#define PORTD1_BIT 1`

`#define PORTD1_MASK 2`

##### PORTD2 - Port D Data Register bit 2

`#define PORTD2_BIT 2`

`#define PORTD2_MASK 4`

##### PORTD3 - Port D Data Register bit 3

`#define PORTD3_BIT 3`

`#define PORTD3_MASK 8`

##### PORTD4 - Port D Data Register bit 4

`#define PORTD4_BIT 4`

`#define PORTD4_MASK 16`

##### PORTD5 - Port D Data Register bit 5

`#define PORTD5_BIT 5`

`#define PORTD5_MASK 32`

##### PORTD6 - Port D Data Register bit 6

`#define PORTD6_BIT 6`

`#define PORTD6_MASK 64`

##### PORTD7 - Port D Data Register bit 7

`#define PORTD7_BIT 7`

`#define PORTD7_MASK 128`

### DDRD - Port D Data Direction Register

`sfrb DDRD = $11;`

##### DDD0 - Port D Data Direction Register bit 0

`#define DDD0_BIT 0`

`#define DDD0_MASK 1`

##### DDD1 - Port D Data Direction Register bit 1

`#define DDD1_BIT 1`

`#define DDD1_MASK 2`

##### DDD2 - Port D Data Direction Register bit 2

`#define DDD2_BIT 2`

`#define DDD2_MASK 4`

##### DDD3 - Port D Data Direction Register bit 3

`#define DDD3_BIT 3`

`#define DDD3_MASK 8`

##### DDD4 - Port D Data Direction Register bit 4

`#define DDD4_BIT 4`

`#define DDD4_MASK 16`

##### DDD5 - Port D Data Direction Register bit 5

`#define DDD5_BIT 5`

`#define DDD5_MASK 32`

##### DDD6 - Port D Data Direction Register bit 6

`#define DDD6_BIT 6`

`#define DDD6_MASK 64`

##### DDD7 - Port D Data Direction Register bit 7

`#define DDD7_BIT 7`

`#define DDD7_MASK 128`

### PIND - Port D Input Pins

`sfrb PIND = $10;`

##### PIND0 - Port D Input Pins bit 0

`#define PIND0_BIT 0`

`#define PIND0_MASK 1`

##### PIND1 - Port D Input Pins bit 1

`#define PIND1_BIT 1`

`#define PIND1_MASK 2`

##### PIND2 - Port D Input Pins bit 2

`#define PIND2_BIT 2`

`#define PIND2_MASK 4`

##### PIND3 - Port D Input Pins bit 3

`#define PIND3_BIT 3`

`#define PIND3_MASK 8`

##### PIND4 - Port D Input Pins bit 4

`#define PIND4_BIT 4`

`#define PIND4_MASK 16`

##### PIND5 - Port D Input Pins bit 5

`#define PIND5_BIT 5`

`#define PIND5_MASK 32`

##### PIND6 - Port D Input Pins bit 6

`#define PIND6_BIT 6`

`#define PIND6_MASK 64`

##### PIND7 - Port D Input Pins bit 7

`#define PIND7_BIT 7`

`#define PIND7_MASK 128`

## TIMER COUNTER 1

The 16-bit Timer/Counter1 can select clock source from CK, prescaled CK, or an external pin. In addition it can be stopped as described in the specification for the Timer/Counter1 Control Registers - TCCR1A and TCCR1B. The different status flags (overflow, compare match and capture event) are found in the Timer/Counter Interrupt Flag Register - TIFR. Control signals are found in the Timer/Counter1 Control Registers - TCCR1A and TCCR1B. The interrupt enable/disable settings for Timer/Counter1 are found in the Timer/Counter Interrupt Mask Register - TIMS

### TIMSK - Timer/Counter Interrupt Mask Register

`sfrb TIMSK = $39;`

##### TICIE1 - Timer/Counter1 Input Capture Interrupt Enable

`#define TICIE1_BIT 3`

`#define TICIE1_MASK 8`

##### OCIE1B - Timer/Counter1 Output CompareB Match Interrupt Enable

`#define OCIE1B_BIT 5`

`#define OCIE1B_MASK 32`

When the OCIE1B bit is set (one) and the I-bit in the Status Register is set (one), the Timer/Counter1 CompareB Match interrupt is enabled. The corresponding interrupt (at vector $005) is executed if a CompareB match in Timer/Counter1 occurs, i.e., when the OCF1B bit is set in the Timer/Counter Interrupt Flag Register - TIFR.

##### OCIE1A - Timer/Counter1 Output CompareA Match Interrupt Enable

`#define OCIE1A_BIT 6`

`#define OCIE1A_MASK 64`

When the OCIE1A bit is set (one) and the I-bit in the Status Register is set (one), the Timer/Counter1 CompareA Match interrupt is enabled. The corresponding interrupt (at vector $004) is executed if a CompareA match in Timer/Counter1 occurs, i.e., when the OCF1A bit is set in the Timer/Counter Interrupt Flag Register - TIFR.

##### TOIE1 - Timer/Counter1 Overflow Interrupt Enable

`#define TOIE1_BIT 7`

`#define TOIE1_MASK 128`

When the TOIE1 bit is set (one) and the I-bit in the Status Register is set (one), the Timer/Counter1 Overflow interrupt is enabled. The corresponding interrupt (at vector $006) is executed if an overflow in Timer/Counter1 occurs, i.e., when the TOV1 bit is set in the Timer/Counter Interrupt Flag Register - TIFR.

### TIFR - Timer/Counter Interrupt Flag register

`sfrb TIFR = $38;`

##### ICF1 - Input Capture Flag 1

`#define ICF1_BIT 3`

`#define ICF1_MASK 8`

The ICF1 bit is set (one) to flag an input capture event, indicating that the Timer/Counter1 value has been transferred to the input capture register - ICR1. ICF1 is cleared by hardware when executing the corresponding interrupt handling vector. Alternatively, ICF1 is cleared by writing a logic one to the flag. When the SREG I-bit, and TICIE1 (Timer/Counter1 Input Capture Interrupt Enable), and ICF1 are set (one), the Timer/Counter1 Capture Interrupt is executed.

##### OCF1B - Output Compare Flag 1B

`#define OCF1B_BIT 5`

`#define OCF1B_MASK 32`

The OCF1B bit is set (one) when compare match occurs between the Timer/Counter1 and the data in OCR1B - Output Compare Register 1B. OCF1B is cleared by hardware when executing the corresponding interrupt handling vector. Alterna-tively, OCF1B is cleared by writing a logic one to the flag. When the I-bit in SREG, and OCIE1B (Timer/Counter1 Compare match InterruptB Enable), and the OCF1B are set (one), the Timer/Counter1 Compare B match Interrupt is executed.

##### OCF1A - Output Compare Flag 1A

`#define OCF1A_BIT 6`

`#define OCF1A_MASK 64`

The OCF1A bit is set (one) when compare match occurs between the Timer/Counter1 and the data in OCR1A - Output Compare Register 1A. OCF1A is cleared by hardware when executing the corresponding interrupt handling vector. Alterna-tively, OCF1A is cleared by writing a logic one to the flag. When the I-bit in SREG, and OCIE1A (Timer/Counter1 Compare match InterruptA Enable), and the OCF1A are set (one), the Timer/Counter1 Compare A match Interrupt is executed.

##### TOV1 - Timer/Counter1 Overflow Flag

`#define TOV1_BIT 7`

`#define TOV1_MASK 128`

The TOV1 is set (one) when an overflow occurs in Timer/Counter1. TOV1 is cleared by hardware when executing the cor-responding interrupt handling vector. Alternatively, TOV1 is cleared by writing a logic one to the flag. When the I-bit in SREG, and TOIE1 (Timer/Counter1 Overflow Interrupt Enable), and TOV1 are set (one), the Timer/Counter1 Overflow Interrupt is executed. In PWM mode, this bit is set when Timer/Counter1 changes counting direction at $0000.

### TCCR1A - Timer/Counter1 Control Register A

`sfrb TCCR1A = $2F;`

##### PWM10 - Pulse Width Modulator Select Bit 0

`#define PWM10_BIT 0`

`#define PWM10_MASK 1`

##### PWM11 - Pulse Width Modulator Select Bit 1

`#define PWM11_BIT 1`

`#define PWM11_MASK 2`

##### COM1B0 - Compare Output Mode 1B, bit 0

`#define COM1B0_BIT 4`

`#define COM1B0_MASK 16`

The COM1B1 and COM1B0 control bits determine any output pin action following a compare match in Timer/Counter1. Any output pin actions affect pin OC1B - Output CompareB.

##### COM1B1 - Compare Output Mode 1B, bit 1

`#define COM1B1_BIT 5`

`#define COM1B1_MASK 32`

The COM1B1 and COM1B0 control bits determine any output pin action following a compare match in Timer/Counter1. Any output pin actions affect pin OC1B - Output CompareB.

##### COM1A0 - Compare Ouput Mode 1A, bit 0

`#define COM1A0_BIT 6`

`#define COM1A0_MASK 64`

The COM1A1 and COM1A0 control bits determine any output pin action following a compare match in Timer/Counter1. Any output pin actions affect pin OC1A - Output CompareA pin 1. This is an alternative function to an I/O port and the corresponding direction control bit must be set (one) to control the output pin. The control configuration is shown in Table 9.

##### COM1A1 - Compare Output Mode 1A, bit 1

`#define COM1A1_BIT 7`

`#define COM1A1_MASK 128`

The COM1A1 and COM1A0 control bits determine any output pin action following a compare match in Timer/Counter1. Any output pin actions affect pin OC1A - Output CompareA pin 1. This is an alternative function to an I/O port and the corresponding direction control bit must be set (one) to control the output pin. The control configuration is shown in Table 9.

### TCCR1B - Timer/Counter1 Control Register B

`sfrb TCCR1B = $2E;`

##### CS10 - Clock Select1 bit 0

`#define CS10_BIT 0`

`#define CS10_MASK 1`

##### CS11 - Clock Select1 bit 1

`#define CS11_BIT 1`

`#define CS11_MASK 2`

##### CS12 - Clock Select1 bit 2

`#define CS12_BIT 2`

`#define CS12_MASK 4`

##### CTC1 - Clear Timer/Counter1 on Compare Match

`#define CTC1_BIT 3`

`#define CTC1_MASK 8`

When the CTC1 control bit is set (one), the Timer/Counter1 is reset to $0000 in the clock cycle after a compareA match. If the CTC1 control bit is cleared, Timer/Counter1 continues counting and is unaffected by a compare match. Since the compare match is detected in the CPU clock cycle following the match, this function will behave differently when a prescal-ing higher than 1 is used for the timer. When a prescaling of 1 is used, and the compareA register is set to C, the timer will count as follows if CTC1 is set: ...|C-2 |C-1 |C |0|1 |... When the prescaler is set to divide by 8, the timer will count like this: ... | C-2, C-2, C-2, C-2, C-2, C-2, C-2, C-2 | C-1, C-1, C-1, C-1, C-1, C-1, C-1, C-1 | C, 0, 0, 0, 0, 0, 0, 0 | ... In PWM mode, this bit has no effect

##### ICES1 - Input Capture 1 Edge Select

`#define ICES1_BIT 6`

`#define ICES1_MASK 64`

While the ICES1 bit is cleared (zero), the Timer/Counter1 contents are transferred to the Input Capture Register - ICR1 - on the falling edge of the input capture pin - ICP. While the ICES1 bit is set (one), the Timer/Counter1 contents are transferred to the Input Capture Register - ICR1 - on the rising edge of the input capture pin - ICP.

##### ICNC1 - Input Capture 1 Noise Canceler

`#define ICNC1_BIT 7`

`#define ICNC1_MASK 128`

When the ICNC1 bit is cleared (zero), the input capture trigger noise canceler function is disabled. The input capture is triggered at the first rising/falling edge sampled on the ICP - input capture pin - as specified. When the ICNC1 bit is set (one), four successive samples are measures on the ICP - input capture pin, and all samples must be high/low according to the input capture trigger specification in the ICES1 bit. The actual sampling frequency is XTAL clock frequency.

### TCNT1H - Timer/Counter1 High Byte

`sfrb TCNT1H = $2D;`

##### TCNT1H0 - Timer/Counter1 High Byte bit 0

`#define TCNT1H0_BIT 0`

`#define TCNT1H0_MASK 1`

##### TCNT1H1 - Timer/Counter1 High Byte bit 1

`#define TCNT1H1_BIT 1`

`#define TCNT1H1_MASK 2`

##### TCNT1H2 - Timer/Counter1 High Byte bit 2

`#define TCNT1H2_BIT 2`

`#define TCNT1H2_MASK 4`

##### TCNT1H3 - Timer/Counter1 High Byte bit 3

`#define TCNT1H3_BIT 3`

`#define TCNT1H3_MASK 8`

##### TCNT1H4 - Timer/Counter1 High Byte bit 4

`#define TCNT1H4_BIT 4`

`#define TCNT1H4_MASK 16`

##### TCNT1H5 - Timer/Counter1 High Byte bit 5

`#define TCNT1H5_BIT 5`

`#define TCNT1H5_MASK 32`

##### TCNT1H6 - Timer/Counter1 High Byte bit 6

`#define TCNT1H6_BIT 6`

`#define TCNT1H6_MASK 64`

##### TCNT1H7 - Timer/Counter1 High Byte bit 7

`#define TCNT1H7_BIT 7`

`#define TCNT1H7_MASK 128`

### TCNT1L - Timer/Counter1 Low Byte

`sfrb TCNT1L = $2C;`

##### TCNT1L0 - Timer/Counter1 Low Byte bit 0

`#define TCNT1L0_BIT 0`

`#define TCNT1L0_MASK 1`

##### TCNT1L1 - Timer/Counter1 Low Byte bit 1

`#define TCNT1L1_BIT 1`

`#define TCNT1L1_MASK 2`

##### TCNT1L2 - Timer/Counter1 Low Byte bit 2

`#define TCNT1L2_BIT 2`

`#define TCNT1L2_MASK 4`

##### TCNT1L3 - Timer/Counter1 Low Byte bit 3

`#define TCNT1L3_BIT 3`

`#define TCNT1L3_MASK 8`

##### TCNT1L4 - Timer/Counter1 Low Byte bit 4

`#define TCNT1L4_BIT 4`

`#define TCNT1L4_MASK 16`

##### TCNT1L5 - Timer/Counter1 Low Byte bit 5

`#define TCNT1L5_BIT 5`

`#define TCNT1L5_MASK 32`

##### TCNT1L6 - Timer/Counter1 Low Byte bit 6

`#define TCNT1L6_BIT 6`

`#define TCNT1L6_MASK 64`

##### TCNT1L7 - Timer/Counter1 Low Byte bit 7

`#define TCNT1L7_BIT 7`

`#define TCNT1L7_MASK 128`

### OCR1AH - Timer/Counter1 Outbut Compare Register High Byte

`sfrb OCR1AH = $2B;`

##### OCR1AH0 - Timer/Counter1 Outbut Compare Register High Byte bit 0

`#define OCR1AH0_BIT 0`

`#define OCR1AH0_MASK 1`

##### OCR1AH1 - Timer/Counter1 Outbut Compare Register High Byte bit 1

`#define OCR1AH1_BIT 1`

`#define OCR1AH1_MASK 2`

##### OCR1AH2 - Timer/Counter1 Outbut Compare Register High Byte bit 2

`#define OCR1AH2_BIT 2`

`#define OCR1AH2_MASK 4`

##### OCR1AH3 - Timer/Counter1 Outbut Compare Register High Byte bit 3

`#define OCR1AH3_BIT 3`

`#define OCR1AH3_MASK 8`

##### OCR1AH4 - Timer/Counter1 Outbut Compare Register High Byte bit 4

`#define OCR1AH4_BIT 4`

`#define OCR1AH4_MASK 16`

##### OCR1AH5 - Timer/Counter1 Outbut Compare Register High Byte bit 5

`#define OCR1AH5_BIT 5`

`#define OCR1AH5_MASK 32`

##### OCR1AH6 - Timer/Counter1 Outbut Compare Register High Byte bit 6

`#define OCR1AH6_BIT 6`

`#define OCR1AH6_MASK 64`

##### OCR1AH7 - Timer/Counter1 Outbut Compare Register High Byte bit 7

`#define OCR1AH7_BIT 7`

`#define OCR1AH7_MASK 128`

### OCR1AL - Timer/Counter1 Output Compare Register Low Byte

`sfrb OCR1AL = $2A;`

##### OCR1AL0 - Timer/Counter1 Output Compare Register Low Byte Bit 0

`#define OCR1AL0_BIT 0`

`#define OCR1AL0_MASK 1`

##### OCR1AL1 - Timer/Counter1 Output Compare Register Low Byte Bit 1

`#define OCR1AL1_BIT 1`

`#define OCR1AL1_MASK 2`

##### OCR1AL2 - Timer/Counter1 Output Compare Register Low Byte Bit 2

`#define OCR1AL2_BIT 2`

`#define OCR1AL2_MASK 4`

##### OCR1AL3 - Timer/Counter1 Output Compare Register Low Byte Bit 3

`#define OCR1AL3_BIT 3`

`#define OCR1AL3_MASK 8`

##### OCR1AL4 - Timer/Counter1 Output Compare Register Low Byte Bit 4

`#define OCR1AL4_BIT 4`

`#define OCR1AL4_MASK 16`

##### OCR1AL5 - Timer/Counter1 Output Compare Register Low Byte Bit 5

`#define OCR1AL5_BIT 5`

`#define OCR1AL5_MASK 32`

##### OCR1AL6 - Timer/Counter1 Output Compare Register Low Byte Bit 6

`#define OCR1AL6_BIT 6`

`#define OCR1AL6_MASK 64`

##### OCR1AL7 - Timer/Counter1 Output Compare Register Low Byte Bit 7

`#define OCR1AL7_BIT 7`

`#define OCR1AL7_MASK 128`

### OCR1BH - Timer/Counter1 Output Compare Register High Byte

`sfrb OCR1BH = $29;`

##### OCR1BH0 - Timer/Counter1 Output Compare Register High Byte bit 0

`#define OCR1BH0_BIT 0`

`#define OCR1BH0_MASK 1`

##### OCR1BH1 - Timer/Counter1 Output Compare Register High Byte bit 1

`#define OCR1BH1_BIT 1`

`#define OCR1BH1_MASK 2`

##### OCR1BH2 - Timer/Counter1 Output Compare Register High Byte bit 2

`#define OCR1BH2_BIT 2`

`#define OCR1BH2_MASK 4`

##### OCR1BH3 - Timer/Counter1 Output Compare Register High Byte bit 3

`#define OCR1BH3_BIT 3`

`#define OCR1BH3_MASK 8`

##### OCR1BH4 - Timer/Counter1 Output Compare Register High Byte bit 4

`#define OCR1BH4_BIT 4`

`#define OCR1BH4_MASK 16`

##### OCR1BH5 - Timer/Counter1 Output Compare Register High Byte bit 5

`#define OCR1BH5_BIT 5`

`#define OCR1BH5_MASK 32`

##### OCR1BH6 - Timer/Counter1 Output Compare Register High Byte bit 6

`#define OCR1BH6_BIT 6`

`#define OCR1BH6_MASK 64`

##### OCR1BH7 - Timer/Counter1 Output Compare Register High Byte bit 7

`#define OCR1BH7_BIT 7`

`#define OCR1BH7_MASK 128`

### OCR1BL - Timer/Counter1 Output Compare Register Low Byte

`sfrb OCR1BL = $28;`

##### OCR1BL0 - Timer/Counter1 Output Compare Register Low Byte bit 0

`#define OCR1BL0_BIT 0`

`#define OCR1BL0_MASK 1`

##### OCR1BL1 - Timer/Counter1 Output Compare Register Low Byte bit 1

`#define OCR1BL1_BIT 1`

`#define OCR1BL1_MASK 2`

##### OCR1BL2 - Timer/Counter1 Output Compare Register Low Byte bit 2

`#define OCR1BL2_BIT 2`

`#define OCR1BL2_MASK 4`

##### OCR1BL3 - Timer/Counter1 Output Compare Register Low Byte bit 3

`#define OCR1BL3_BIT 3`

`#define OCR1BL3_MASK 8`

##### OCR1BL4 - Timer/Counter1 Output Compare Register Low Byte bit 4

`#define OCR1BL4_BIT 4`

`#define OCR1BL4_MASK 16`

##### OCR1BL5 - Timer/Counter1 Output Compare Register Low Byte bit 5

`#define OCR1BL5_BIT 5`

`#define OCR1BL5_MASK 32`

##### OCR1BL6 - Timer/Counter1 Output Compare Register Low Byte bit 6

`#define OCR1BL6_BIT 6`

`#define OCR1BL6_MASK 64`

##### OCR1BL7 - Timer/Counter1 Output Compare Register Low Byte bit 7

`#define OCR1BL7_BIT 7`

`#define OCR1BL7_MASK 128`

### ICR1H - Timer/Counter1 Input Capture Register High Byte

`sfrb ICR1H = $25;`

##### ICR1H0 - Timer/Counter1 Input Capture Register High Byte bit 0

`#define ICR1H0_BIT 0`

`#define ICR1H0_MASK 1`

##### ICR1H1 - Timer/Counter1 Input Capture Register High Byte bit 1

`#define ICR1H1_BIT 1`

`#define ICR1H1_MASK 2`

##### ICR1H2 - Timer/Counter1 Input Capture Register High Byte bit 2

`#define ICR1H2_BIT 2`

`#define ICR1H2_MASK 4`

##### ICR1H3 - Timer/Counter1 Input Capture Register High Byte bit 3

`#define ICR1H3_BIT 3`

`#define ICR1H3_MASK 8`

##### ICR1H4 - Timer/Counter1 Input Capture Register High Byte bit 4

`#define ICR1H4_BIT 4`

`#define ICR1H4_MASK 16`

##### ICR1H5 - Timer/Counter1 Input Capture Register High Byte bit 5

`#define ICR1H5_BIT 5`

`#define ICR1H5_MASK 32`

##### ICR1H6 - Timer/Counter1 Input Capture Register High Byte bit 6

`#define ICR1H6_BIT 6`

`#define ICR1H6_MASK 64`

##### ICR1H7 - Timer/Counter1 Input Capture Register High Byte bit 7

`#define ICR1H7_BIT 7`

`#define ICR1H7_MASK 128`

### ICR1L - Timer/Counter1 Input Capture Register Low Byte

`sfrb ICR1L = $24;`

##### ICR1L0 - Timer/Counter1 Input Capture Register Low Byte bit 0

`#define ICR1L0_BIT 0`

`#define ICR1L0_MASK 1`

##### ICR1L1 - Timer/Counter1 Input Capture Register Low Byte bit 1

`#define ICR1L1_BIT 1`

`#define ICR1L1_MASK 2`

##### ICR1L2 - Timer/Counter1 Input Capture Register Low Byte bit 2

`#define ICR1L2_BIT 2`

`#define ICR1L2_MASK 4`

##### ICR1L3 - Timer/Counter1 Input Capture Register Low Byte bit 3

`#define ICR1L3_BIT 3`

`#define ICR1L3_MASK 8`

##### ICR1L4 - Timer/Counter1 Input Capture Register Low Byte bit 4

`#define ICR1L4_BIT 4`

`#define ICR1L4_MASK 16`

##### ICR1L5 - Timer/Counter1 Input Capture Register Low Byte bit 5

`#define ICR1L5_BIT 5`

`#define ICR1L5_MASK 32`

##### ICR1L6 - Timer/Counter1 Input Capture Register Low Byte bit 6

`#define ICR1L6_BIT 6`

`#define ICR1L6_MASK 64`

##### ICR1L7 - Timer/Counter1 Input Capture Register Low Byte bit 7

`#define ICR1L7_BIT 7`

`#define ICR1L7_MASK 128`

## TIMER COUNTER 0

The 8-bit Timer/Counter0 can select clock source from CK, prescaled CK, or an external pin. In addition it can be stopped as described in ?Timer/Counter0 Control Register - TCCR0? on page 35. The overflow status flag is found in ?The Timer/Counter Interrupt Flag Register - TIFR? on page 29. Control signals are found in the Timer/Counter0 Control Register - TCCR0. The interrupt enable/disable settings for Timer/Counter0 are found in ?The Timer/Counter Interrupt Mask Regis-ter - TIMSK? on page 28. When Timer/Counter0 is externally clocked, the external signal is synchronized with the oscillator frequency of the CPU. To assure proper sampling of the external clock, the minimum time between two external clock transitions must be at least one internal CPU clock period. The external clock signal is sampled on the rising edge of the internal CPU clock. The 8-bit Timer/Counter0 features both a high resolution and a high accuracy usage with the lower prescaling opportuni-ties. Similarly, the high prescaling opportuni ties make the Timer/Counter0 useful for lower speed functions or exact timing functions with infrequent actions

### TIMSK - Timer/Counter Interrupt Mask Register

`sfrb TIMSK = $39;`

##### TOIE0 - Timer/Counter0 Overflow Interrupt Enable

`#define TOIE0_BIT 1`

`#define TOIE0_MASK 2`

When the TOIE0 bit is set (one) and the I-bit in the Status Register is set (one), the Timer/Counter0 Overflow interrupt is enabled. The corresponding interrupt is executed if an overflow in Timer/Counter0 occurs, i.e., when the TOV0 bit is set in the Timer/Counter Interrupt Flag Register - TIFR.

### TIFR - Timer/Counter Interrupt Flag register

`sfrb TIFR = $38;`

##### TOV0 - Timer/Counter0 Overflow Flag

`#define TOV0_BIT 1`

`#define TOV0_MASK 2`

The bit TOV0 is set (one) when an overflow occurs in Timer/Counter0. TOV0 is cleared by hardware when executing the corresponding interrupt handling vector. Alternatively, TOV0 is cleared by writing a logic one to the flag. When the SREG I-bit, and TOIE0 (Timer/Counter0 Overflow Interrupt Enable), and TOV0 are set (one), the Timer/Counter0 Overflow interrupt is executed.

### TCCR0 - Timer/Counter0 Control Register

`sfrb TCCR0 = $33;`

##### CS00 - Clock Select0 bit 0

`#define CS00_BIT 0`

`#define CS00_MASK 1`

##### CS01 - Clock Select0 bit 1

`#define CS01_BIT 1`

`#define CS01_MASK 2`

##### CS02 - Clock Select0 bit 2

`#define CS02_BIT 2`

`#define CS02_MASK 4`

### TCNT0 - Timer Counter 0

`sfrb TCNT0 = $32;`

##### TCNT00 - Timer Counter 0 bit 0

`#define TCNT00_BIT 0`

`#define TCNT00_MASK 1`

##### TCNT01 - Timer Counter 0 bit 1

`#define TCNT01_BIT 1`

`#define TCNT01_MASK 2`

##### TCNT02 - Timer Counter 0 bit 2

`#define TCNT02_BIT 2`

`#define TCNT02_MASK 4`

##### TCNT03 - Timer Counter 0 bit 3

`#define TCNT03_BIT 3`

`#define TCNT03_MASK 8`

##### TCNT04 - Timer Counter 0 bit 4

`#define TCNT04_BIT 4`

`#define TCNT04_MASK 16`

##### TCNT05 - Timer Counter 0 bit 5

`#define TCNT05_BIT 5`

`#define TCNT05_MASK 32`

##### TCNT06 - Timer Counter 0 bit 6

`#define TCNT06_BIT 6`

`#define TCNT06_MASK 64`

##### TCNT07 - Timer Counter 0 bit 7

`#define TCNT07_BIT 7`

`#define TCNT07_MASK 128`

## WATCHDOG

### WDTCR - Watchdog Timer Control Register

`sfrb WDTCR = $21;`

##### WDP0 - Watch Dog Timer Prescaler bit 0

`#define WDP0_BIT 0`

`#define WDP0_MASK 1`

##### WDP1 - Watch Dog Timer Prescaler bit 1

`#define WDP1_BIT 1`

`#define WDP1_MASK 2`

##### WDP2 - Watch Dog Timer Prescaler bit 2

`#define WDP2_BIT 2`

`#define WDP2_MASK 4`

##### WDE - Watch Dog Enable

`#define WDE_BIT 3`

`#define WDE_MASK 8`

When the WDE is set (one) the Watchdog Timer is enabled, and if the WDE is cleared (zero) the Watchdog Timer function is disabled. WDE can only be cleared if the WDTOE bit is set(one). To disable an enabled watchdog timer, the following procedure must be followed: 1. In the same operation, write a logical one to WDTOE and WDE. A logical one must be written to WDE even though it is set to one before the disable operation starts. 2. Within the next four clock cycles, write a logical 0 to WDE. This disables the watchdog

##### WDTOE - RW

`#define WDTOE_BIT 4`

`#define WDTOE_MASK 16`

This bit must be set (one) when the WDE bit is cleared. Otherwise, the watchdog will not be disabled. Once set, hardware will clear this bit to zero after four clock cycles. Refer to the description of the WDE bit for a watchdog disable procedure.

## CPU

### SREG - Status Register

`sfrb SREG = $3F;`

### SPH - Stack Pointer High

`sfrb SPH = $3E;`

##### SP8 - Stack pointer bit 8

`#define SP8_BIT 0`

`#define SP8_MASK 1`

##### SP9 - Stack pointer bit 9

`#define SP9_BIT 1`

`#define SP9_MASK 2`

##### SP10 - Stack pointer bit 10

`#define SP10_BIT 2`

`#define SP10_MASK 4`

##### SP11 - Stack pointer bit 11

`#define SP11_BIT 3`

`#define SP11_MASK 8`

##### SP12 - Stack pointer bit 12

`#define SP12_BIT 4`

`#define SP12_MASK 16`

##### SP13 - Stack pointer bit 13

`#define SP13_BIT 5`

`#define SP13_MASK 32`

##### SP14 - Stack pointer bit 14

`#define SP14_BIT 6`

`#define SP14_MASK 64`

##### SP15 - Stack pointer bit 15

`#define SP15_BIT 7`

`#define SP15_MASK 128`

### SPL - Stack Pointer Low

`sfrb SPL = $3D;`

##### SP0 - Stack pointer bit 0

`#define SP0_BIT 0`

`#define SP0_MASK 1`

##### SP1 - Stack pointer bit 1

`#define SP1_BIT 1`

`#define SP1_MASK 2`

##### SP2 - Stack pointer bit 2

`#define SP2_BIT 2`

`#define SP2_MASK 4`

##### SP3 - Stack pointer bit 3

`#define SP3_BIT 3`

`#define SP3_MASK 8`

##### SP4 - Stack pointer bit 4

`#define SP4_BIT 4`

`#define SP4_MASK 16`

##### SP5 - Stack pointer bit 5

`#define SP5_BIT 5`

`#define SP5_MASK 32`

##### SP6 - Stack pointer bit 6

`#define SP6_BIT 6`

`#define SP6_MASK 64`

##### SP7 - Stack pointer bit 7

`#define SP7_BIT 7`

`#define SP7_MASK 128`

### MCUCR - MCU Control Register

`sfrb MCUCR = $35;`

##### ISC00 - Interrupt Sense Control 0 bit 0

`#define ISC00_BIT 0`

`#define ISC00_MASK 1`

##### ISC01 - Interrupt Sense Control 0 bit 1

`#define ISC01_BIT 1`

`#define ISC01_MASK 2`

##### ISC10 - Interrupt Sense Control 1 bit 0

`#define ISC10_BIT 2`

`#define ISC10_MASK 4`

##### ISC11 - Interrupt Sense Control 1 bit 1

`#define ISC11_BIT 3`

`#define ISC11_MASK 8`

##### SM - Sleep Mode

`#define SM_BIT 4`

`#define SM_MASK 16`

When SM is set (one), Power Down mode is selected as sleep mode. For details, refer to the paragraph ?Sleep Modes? below.

##### SE - Sleep Enable

`#define SE_BIT 5`

`#define SE_MASK 32`

The SE bit must be set (one) to make the MCU enter the sleep mode when the SLEEP instruction is executed. To avoid the MCU entering the sleep mode unless it is the programmers purpose, it is recommended to set the Sleep Enable SE bit just before the execution of the SLEEP instruction.

##### SRW - External SRAM Wait State

`#define SRW_BIT 6`

`#define SRW_MASK 64`

When the SRW bit is set (one), a one cycle wait state is inserted in the external data SRAM access cycle. When the SRW bit is cleared (zero), the external data SRAM access is executed with the normal three-cycle scheme. See Figure 43: Exter-nal Data SRAM Memory Cycles without Wait State and Figure 44: External Data SRAM Memory Cycles with Wait State.

##### SRE - External SRAM Enable

`#define SRE_BIT 7`

`#define SRE_MASK 128`

When the SRE bit is set (one), the external data SRAM is enabled, and the pin functions AD0-7 (Port A), A8-15 (Port C), WR and RD (Port D) are activated as the alternate pin functions. Then the SRE bit overrides any pin direction settings in the respective data direction registers. See ?The SRAM Data Memory - Internal and External? for description of the External SRAM pin functions. When the SRE bit is cleared (zero), the external data SRAM is disabled, and the normal pin and data direction settings are used

## EEPROM

### EEARH - EEPROM Read/Write Access High Byte

`sfrb EEARH = $1F;`

##### EEAR8 - EEPROM Read/Write Access High Byte bit 0

`#define EEAR8_BIT 0`

`#define EEAR8_MASK 1`

### EEARL - EEPROM Read/Write Access Low Byte

`sfrb EEARL = $1E;`

##### EEAR0 - EEPROM Read/Write Access Low Byte bit 0

`#define EEAR0_BIT 0`

`#define EEAR0_MASK 1`

##### EEAR1 - EEPROM Read/Write Access Low Byte bit 1

`#define EEAR1_BIT 1`

`#define EEAR1_MASK 2`

##### EEAR2 - EEPROM Read/Write Access Low Byte bit 2

`#define EEAR2_BIT 2`

`#define EEAR2_MASK 4`

##### EEAR3 - EEPROM Read/Write Access Low Byte bit 3

`#define EEAR3_BIT 3`

`#define EEAR3_MASK 8`

##### EEAR4 - EEPROM Read/Write Access Low Byte bit 4

`#define EEAR4_BIT 4`

`#define EEAR4_MASK 16`

##### EEAR5 - EEPROM Read/Write Access Low Byte bit 5

`#define EEAR5_BIT 5`

`#define EEAR5_MASK 32`

##### EEAR6 - EEPROM Read/Write Access Low Byte bit 6

`#define EEAR6_BIT 6`

`#define EEAR6_MASK 64`

##### EEAR7 - EEPROM Read/Write Access Low Byte bit 7

`#define EEAR7_BIT 7`

`#define EEAR7_MASK 128`

### EEDR - EEPROM Data Register

`sfrb EEDR = $1D;`

##### EEDR0 - EEPROM Data Register bit 0

`#define EEDR0_BIT 0`

`#define EEDR0_MASK 1`

##### EEDR1 - EEPROM Data Register bit 1

`#define EEDR1_BIT 1`

`#define EEDR1_MASK 2`

##### EEDR2 - EEPROM Data Register bit 2

`#define EEDR2_BIT 2`

`#define EEDR2_MASK 4`

##### EEDR3 - EEPROM Data Register bit 3

`#define EEDR3_BIT 3`

`#define EEDR3_MASK 8`

##### EEDR4 - EEPROM Data Register bit 4

`#define EEDR4_BIT 4`

`#define EEDR4_MASK 16`

##### EEDR5 - EEPROM Data Register bit 5

`#define EEDR5_BIT 5`

`#define EEDR5_MASK 32`

##### EEDR6 - EEPROM Data Register bit 6

`#define EEDR6_BIT 6`

`#define EEDR6_MASK 64`

##### EEDR7 - EEPROM Data Register bit 7

`#define EEDR7_BIT 7`

`#define EEDR7_MASK 128`

### EECR - EEPROM Control Register

`sfrb EECR = $1C;`

##### EERE - EEPROM Read Enable

`#define EERE_BIT 0`

`#define EERE_MASK 1`

The EEPROM Read Enable Signal EERE is the read strobe to the EEPROM. When the correct address is set up in the EEAR register, the EERE bit must be set. When the EERE bit is cleared (zero) by hardware, requested data is found in the EEDR register. The EEPROM read access takes one instruction and there is no need to poll the EERE bit. When EERE has been set, the CPU is halted for four cycles before the next instruction is executed. The user should poll the EEWE bit before starting the read operation. If a write operation is in progress when new data or address is written to the EEPROM I/O registers, the write operation will be interrupted, and the result is undefined.

##### EEWE - EEPROM Write Enable

`#define EEWE_BIT 1`

`#define EEWE_MASK 2`

The EEPROM Write Enable Signal EEWE is the write strobe to the EEPROM. When address and data are correctly set up, the EEWE bit must be set to write the value into the EEPROM. The EEMWE bit must be set when the logical one is written to EEWE, otherwise no EEPROM write takes place. The following procedure should be followed when writing the EEPROM (the order of steps 2 and 3 is unessential): 1. Wait until EEWE becomes zero. 2. Write new EEPROM address to EEARL and EEARH (optional). 3. Write new EEPROM data to EEDR (optional). 4. Write a logical one to the EEMWE bit in EECR (to be able to write a logical one to the EEMWE bit, the EEWE bit mustbewritten to zero in thesamecycle). 5. Within four clock cycles after setting EEMWE, write a logical one to EEWE. When the write access time (typically 2.5 ms at V CC =5Vor 4msatV CC = 2.7V) has elapsed, the EEWE bit is cleared (zero) by hardware. The user software can poll this bit and wait for a zero before writing the next byte. When EEWE has been set, the CPU is halted or two cycles before the next instruction is executed. Caution: An interrupt between step 4 and step 5 will make the write cycle fail, since the EEPROM Master Write Enable will time-out. If an interrupt routine accessing the EEPROM is interrupting another EEPROM access, the EEAR or EEDR regis-ter will be modified, causing the interrupted EEPROM access to fail. It is recommended to have the global interrupt flag cleared during the 4 last steps to avoid these problems.

##### EEMWE - EEPROM Master Write Enable

`#define EEMWE_BIT 2`

`#define EEMWE_MASK 4`

The EEMWE bit determines whether setting EEWE to one causes the EEPROM to be written. When EEMWE is set(one) setting EEWE will write data to the EEPROM at the selected address If EEMWE is zero, setting EEWE will have no effect. When EEMWE has been set (one) by software, hardware clears the bit to zero after four clock cycles. See the description of the EEWE bit for a EEPROM write procedure.