The Atmel STK500-ISP/AVRISP target interface provides access to Atmel’s STK500 ISP programming and to Atmel’s AVRISP programmer. This target interface supports program loading and access to the fuse bits and lock bits.

###### Target window specific context menu entries

Fuse Bits.
  This displays the fuse bits editor.
Lock Bits.
  This displays the fuse bits editor.

###### Connection property group

Device Name
  The device to be programmed.
Port Name
  The name of the serial port.
Hardware Version
  The hardware version of the STK500.
Software Version
  The software version of the STK500.

###### Current property group

Device Type
  The AVR device type, identified from the signature bytes.
Fuse Bits
  The fuse bits of the device.
ISP Freq (Desired) and (Actual)
  The ISP frequency which must be less than 1/4 of the target frequency.
JTAG ID
  The JTAG id.
Lock Bits
  The lock bits of the device.
Osc Freq (Desired) and (Actual)
  The supplied oscillator frequency of the STK500.
Oscillator Callibration Bytes
  The oscillator callibration bytes of the device.
Signature Bytes
  The signature bytes of the device.
TopCard
  The name of the expansion card on the STK500.
Voltages
  The supplied VTarget and ARef voltage values of the STK500.