The Atmel AVRISP mkII target interface provides access to Atmel’s AVRISP mkII programmer. This target interface supports program loading and access to the fuse bits and lock bits.

###### Connection property group

Device Name
  The device to be programmed.
Hardware Version
  The hardware version of the AVRISP mkII.
ISP Freq (Desired)
  The ISP frequency which must be less than 1/4 of the target frequency.
Software Version
  The software version of the AVRISP mkII.
USB Serial Number
  The serial numbers of the AVRISP mkII. This is updated each time a connection is made.
Use Target As Device Name
  If this is set the Target project property of the current project in the current build configuration is used rather than the Device Name.

###### Current property group

Device Type
  The AVR device type, identified from the signature bytes.
ISP Freq (Actual)
  The actual ISP frequency in use.