    #ifndef __AT90USB646_h
    #define __AT90USB646_h

    // Interrupt vectors

    #define RESET_vect 0x0000
    #define INT0_vect 0x0004
    #define INT1_vect 0x0008
    #define INT2_vect 0x000c
    #define INT3_vect 0x0010
    #define INT4_vect 0x0014
    #define INT5_vect 0x0018
    #define INT6_vect 0x001c
    #define INT7_vect 0x0020
    #define PCINT0_vect 0x0024
    #define USB_GEN_vect 0x0028
    #define USB_COM_vect 0x002c
    #define WDT_vect 0x0030
    #define TIMER2_COMPA_vect 0x0034
    #define TIMER2_COMPB_vect 0x0038
    #define TIMER2_OVF_vect 0x003c
    #define TIMER1_CAPT_vect 0x0040
    #define TIMER1_COMPA_vect 0x0044
    #define TIMER1_COMPB_vect 0x0048
    #define TIMER1_COMPC_vect 0x004c
    #define TIMER1_OVF_vect 0x0050
    #define TIMER0_COMPA_vect 0x0054
    #define TIMER0_COMPB_vect 0x0058
    #define TIMER0_OVF_vect 0x005c
    #define SPI_STC_vect 0x0060
    #define USART1_RX_vect 0x0064
    #define USART1_UDRE_vect 0x0068
    #define USART1_TX_vect 0x006c
    #define ANALOG_COMP_vect 0x0070
    #define ADC_vect 0x0074
    #define EE_READY_vect 0x0078
    #define TIMER3_CAPT_vect 0x007c
    #define TIMER3_COMPA_vect 0x0080
    #define TIMER3_COMPB_vect 0x0084
    #define TIMER3_COMPC_vect 0x0088
    #define TIMER3_OVF_vect 0x008c
    #define TWI_vect 0x0090
    #define SPM_READY_vect 0x0094

    // I/O addresses

    sfrb PLLCSR = 0x49;
    #define PLOCK 0
    #define PLOCK_BIT 0
    #define PLOCK_MASK 1
    #define PLLE 1
    #define PLLE_BIT 1
    #define PLLE_MASK 2
    #define PLLP0 2
    #define PLLP0_BIT 2
    #define PLLP0_MASK 4
    #define PLLP1 3
    #define PLLP1_BIT 3
    #define PLLP1_MASK 8
    #define PLLP2 4
    #define PLLP2_BIT 4
    #define PLLP2_MASK 16

    sfrb TESTPADSTATUS = 0xfd;

    sfrb TESTPADPULL = 0xfe;

    sfrb TESTPADCTRL = 0xff;

    sfrb UPERRX = 0xf5;
    #define DATATGL 0
    #define DATATGL_BIT 0
    #define DATATGL_MASK 1
    #define DATAPID 1
    #define DATAPID_BIT 1
    #define DATAPID_MASK 2
    #define PID 2
    #define PID_BIT 2
    #define PID_MASK 4
    #define TIMEOUT 3
    #define TIMEOUT_BIT 3
    #define TIMEOUT_MASK 8
    #define CRC16 4
    #define CRC16_BIT 4
    #define CRC16_MASK 16
    #define COUNTER0 5
    #define COUNTER0_BIT 5
    #define COUNTER0_MASK 32
    #define COUNTER1 6
    #define COUNTER1_BIT 6
    #define COUNTER1_MASK 64

    sfrb UEINT = 0xf4;
    #define UEINT_0 0
    #define UEINT_0_BIT 0
    #define UEINT_0_MASK 1
    #define UEINT_1 1
    #define UEINT_1_BIT 1
    #define UEINT_1_MASK 2
    #define UEINT_2 2
    #define UEINT_2_BIT 2
    #define UEINT_2_MASK 4
    #define UEINT_3 3
    #define UEINT_3_BIT 3
    #define UEINT_3_MASK 8
    #define UEINT_4 4
    #define UEINT_4_BIT 4
    #define UEINT_4_MASK 16
    #define UEINT_5 5
    #define UEINT_5_BIT 5
    #define UEINT_5_MASK 32
    #define UEINT_6 6
    #define UEINT_6_BIT 6
    #define UEINT_6_MASK 64

    sfrb UPINT = 0xf8;
    #define PINT0 0
    #define PINT0_BIT 0
    #define PINT0_MASK 1
    #define PINT1 1
    #define PINT1_BIT 1
    #define PINT1_MASK 2
    #define PINT2 2
    #define PINT2_BIT 2
    #define PINT2_MASK 4
    #define PINT3 3
    #define PINT3_BIT 3
    #define PINT3_MASK 8
    #define PINT4 4
    #define PINT4_BIT 4
    #define PINT4_MASK 16
    #define PINT5 5
    #define PINT5_BIT 5
    #define PINT5_MASK 32
    #define PINT6 6
    #define PINT6_BIT 6
    #define PINT6_MASK 64

    sfrb UEBCHX = 0xf3;
    #define UEBCHX_0 0
    #define UEBCHX_0_BIT 0
    #define UEBCHX_0_MASK 1
    #define UEBCHX_1 1
    #define UEBCHX_1_BIT 1
    #define UEBCHX_1_MASK 2
    #define UEBCHX_2 2
    #define UEBCHX_2_BIT 2
    #define UEBCHX_2_MASK 4

    sfrb UPBCHX = 0xf7;
    #define PBYCT8 0
    #define PBYCT8_BIT 0
    #define PBYCT8_MASK 1
    #define PBYCT9 1
    #define PBYCT9_BIT 1
    #define PBYCT9_MASK 2
    #define PBYCT10 2
    #define PBYCT10_BIT 2
    #define PBYCT10_MASK 4

    sfrb UEBCLX = 0xf2;
    #define UEBCLX_0 0
    #define UEBCLX_0_BIT 0
    #define UEBCLX_0_MASK 1
    #define UEBCLX_1 1
    #define UEBCLX_1_BIT 1
    #define UEBCLX_1_MASK 2
    #define UEBCLX_2 2
    #define UEBCLX_2_BIT 2
    #define UEBCLX_2_MASK 4
    #define UEBCLX_3 3
    #define UEBCLX_3_BIT 3
    #define UEBCLX_3_MASK 8
    #define UEBCLX_4 4
    #define UEBCLX_4_BIT 4
    #define UEBCLX_4_MASK 16
    #define UEBCLX_5 5
    #define UEBCLX_5_BIT 5
    #define UEBCLX_5_MASK 32
    #define UEBCLX_6 6
    #define UEBCLX_6_BIT 6
    #define UEBCLX_6_MASK 64
    #define UEBCLX_7 7
    #define UEBCLX_7_BIT 7
    #define UEBCLX_7_MASK 128

    sfrb UPBCLX = 0xf6;
    #define PBYCT0 0
    #define PBYCT0_BIT 0
    #define PBYCT0_MASK 1
    #define PBYCT1 1
    #define PBYCT1_BIT 1
    #define PBYCT1_MASK 2
    #define PBYCT2 2
    #define PBYCT2_BIT 2
    #define PBYCT2_MASK 4
    #define PBYCT3 3
    #define PBYCT3_BIT 3
    #define PBYCT3_MASK 8
    #define PBYCT4 4
    #define PBYCT4_BIT 4
    #define PBYCT4_MASK 16
    #define PBYCT5 5
    #define PBYCT5_BIT 5
    #define PBYCT5_MASK 32
    #define PBYCT6 6
    #define PBYCT6_BIT 6
    #define PBYCT6_MASK 64
    #define PBYCT7 7
    #define PBYCT7_BIT 7
    #define PBYCT7_MASK 128

    sfrb UEDATX = 0xf1;
    #define UEDATX_0 0
    #define UEDATX_0_BIT 0
    #define UEDATX_0_MASK 1
    #define UEDATX_1 1
    #define UEDATX_1_BIT 1
    #define UEDATX_1_MASK 2
    #define UEDATX_2 2
    #define UEDATX_2_BIT 2
    #define UEDATX_2_MASK 4
    #define UEDATX_3 3
    #define UEDATX_3_BIT 3
    #define UEDATX_3_MASK 8
    #define UEDATX_4 4
    #define UEDATX_4_BIT 4
    #define UEDATX_4_MASK 16
    #define UEDATX_5 5
    #define UEDATX_5_BIT 5
    #define UEDATX_5_MASK 32
    #define UEDATX_6 6
    #define UEDATX_6_BIT 6
    #define UEDATX_6_MASK 64
    #define UEDATX_7 7
    #define UEDATX_7_BIT 7
    #define UEDATX_7_MASK 128

    sfrb UPDATX = 0xaf;
    #define PDAT0 0
    #define PDAT0_BIT 0
    #define PDAT0_MASK 1
    #define PDAT1 1
    #define PDAT1_BIT 1
    #define PDAT1_MASK 2
    #define PDAT2 2
    #define PDAT2_BIT 2
    #define PDAT2_MASK 4
    #define PDAT3 3
    #define PDAT3_BIT 3
    #define PDAT3_MASK 8
    #define PDAT4 4
    #define PDAT4_BIT 4
    #define PDAT4_MASK 16
    #define PDAT5 5
    #define PDAT5_BIT 5
    #define PDAT5_MASK 32
    #define PDAT6 6
    #define PDAT6_BIT 6
    #define PDAT6_MASK 64
    #define PDAT7 7
    #define PDAT7_BIT 7
    #define PDAT7_MASK 128

    sfrb UEIENX = 0xf0;
    #define TXINE 0
    #define TXINE_BIT 0
    #define TXINE_MASK 1
    #define STALLEDE 1
    #define STALLEDE_BIT 1
    #define STALLEDE_MASK 2
    #define RXOUTE 2
    #define RXOUTE_BIT 2
    #define RXOUTE_MASK 4
    #define RXSTPE 3
    #define RXSTPE_BIT 3
    #define RXSTPE_MASK 8
    #define NAKOUTE 4
    #define NAKOUTE_BIT 4
    #define NAKOUTE_MASK 16
    #define NAKINE 6
    #define NAKINE_BIT 6
    #define NAKINE_MASK 64
    #define FLERRE 7
    #define FLERRE_BIT 7
    #define FLERRE_MASK 128

    sfrb UPIENX = 0xae;
    #define RXINE 0
    #define RXINE_BIT 0
    #define RXINE_MASK 1
    #define RXSTALLE 1
    #define RXSTALLE_BIT 1
    #define RXSTALLE_MASK 2
    #define TXOUTE 2
    #define TXOUTE_BIT 2
    #define TXOUTE_MASK 4
    #define TXSTPE 3
    #define TXSTPE_BIT 3
    #define TXSTPE_MASK 8
    #define PERRE 4
    #define PERRE_BIT 4
    #define PERRE_MASK 16
    #define NAKEDE 6
    #define NAKEDE_BIT 6
    #define NAKEDE_MASK 64
    #define FLERRE 7
    #define FLERRE_BIT 7
    #define FLERRE_MASK 128

    sfrb UESTA1X = 0xef;
    #define CURRBK0 0
    #define CURRBK0_BIT 0
    #define CURRBK0_MASK 1
    #define CURRBK1 1
    #define CURRBK1_BIT 1
    #define CURRBK1_MASK 2
    #define CTRLDIR 2
    #define CTRLDIR_BIT 2
    #define CTRLDIR_MASK 4

    sfrb UPCFG2X = 0xad;
    #define UPCFG2X_0 0
    #define UPCFG2X_0_BIT 0
    #define UPCFG2X_0_MASK 1
    #define UPCFG2X_1 1
    #define UPCFG2X_1_BIT 1
    #define UPCFG2X_1_MASK 2
    #define UPCFG2X_2 2
    #define UPCFG2X_2_BIT 2
    #define UPCFG2X_2_MASK 4
    #define UPCFG2X_3 3
    #define UPCFG2X_3_BIT 3
    #define UPCFG2X_3_MASK 8
    #define UPCFG2X_4 4
    #define UPCFG2X_4_BIT 4
    #define UPCFG2X_4_MASK 16
    #define UPCFG2X_5 5
    #define UPCFG2X_5_BIT 5
    #define UPCFG2X_5_MASK 32
    #define UPCFG2X_6 6
    #define UPCFG2X_6_BIT 6
    #define UPCFG2X_6_MASK 64
    #define UPCFG2X_7 7
    #define UPCFG2X_7_BIT 7
    #define UPCFG2X_7_MASK 128

    sfrb UESTA0X = 0xee;
    #define NBUSYBK0 0
    #define NBUSYBK0_BIT 0
    #define NBUSYBK0_MASK 1
    #define NBUSYBK1 1
    #define NBUSYBK1_BIT 1
    #define NBUSYBK1_MASK 2
    #define DTSEQ0 2
    #define DTSEQ0_BIT 2
    #define DTSEQ0_MASK 4
    #define DTSEQ1 3
    #define DTSEQ1_BIT 3
    #define DTSEQ1_MASK 8
    #define ZLPSEEN 4
    #define ZLPSEEN_BIT 4
    #define ZLPSEEN_MASK 16
    #define UNDERFI 5
    #define UNDERFI_BIT 5
    #define UNDERFI_MASK 32
    #define OVERFI 6
    #define OVERFI_BIT 6
    #define OVERFI_MASK 64
    #define CFGOK 7
    #define CFGOK_BIT 7
    #define CFGOK_MASK 128

    sfrb UPSTAX = 0xac;
    #define NBUSYK0 0
    #define NBUSYK0_BIT 0
    #define NBUSYK0_MASK 1
    #define NBUSYK1 1
    #define NBUSYK1_BIT 1
    #define NBUSYK1_MASK 2
    #define DTSEQ0 2
    #define DTSEQ0_BIT 2
    #define DTSEQ0_MASK 4
    #define DTSEQ1 3
    #define DTSEQ1_BIT 3
    #define DTSEQ1_MASK 8
    #define UNDERFI 5
    #define UNDERFI_BIT 5
    #define UNDERFI_MASK 32
    #define OVERFI 6
    #define OVERFI_BIT 6
    #define OVERFI_MASK 64
    #define CFGOK 7
    #define CFGOK_BIT 7
    #define CFGOK_MASK 128

    sfrb UECFG1X = 0xed;
    #define ALLOC 1
    #define ALLOC_BIT 1
    #define ALLOC_MASK 2
    #define EPBK0 2
    #define EPBK0_BIT 2
    #define EPBK0_MASK 4
    #define EPBK1 3
    #define EPBK1_BIT 3
    #define EPBK1_MASK 8
    #define EPSIZE0 4
    #define EPSIZE0_BIT 4
    #define EPSIZE0_MASK 16
    #define EPSIZE1 5
    #define EPSIZE1_BIT 5
    #define EPSIZE1_MASK 32
    #define EPSIZE2 6
    #define EPSIZE2_BIT 6
    #define EPSIZE2_MASK 64

    sfrb UPCFG1X = 0xab;
    #define ALLOC 1
    #define ALLOC_BIT 1
    #define ALLOC_MASK 2
    #define PBK0 2
    #define PBK0_BIT 2
    #define PBK0_MASK 4
    #define PBK1 3
    #define PBK1_BIT 3
    #define PBK1_MASK 8
    #define PSIZE0 4
    #define PSIZE0_BIT 4
    #define PSIZE0_MASK 16
    #define PSIZE1 5
    #define PSIZE1_BIT 5
    #define PSIZE1_MASK 32
    #define PSIZE2 6
    #define PSIZE2_BIT 6
    #define PSIZE2_MASK 64

    sfrb UECFG0X = 0xec;
    #define EPDIR 0
    #define EPDIR_BIT 0
    #define EPDIR_MASK 1
    #define EPTYPE0 6
    #define EPTYPE0_BIT 6
    #define EPTYPE0_MASK 64
    #define EPTYPE1 7
    #define EPTYPE1_BIT 7
    #define EPTYPE1_MASK 128

    sfrb UPCFG0X = 0xaa;
    #define PEPNUM0 0
    #define PEPNUM0_BIT 0
    #define PEPNUM0_MASK 1
    #define PEPNUM1 1
    #define PEPNUM1_BIT 1
    #define PEPNUM1_MASK 2
    #define PEPNUM2 2
    #define PEPNUM2_BIT 2
    #define PEPNUM2_MASK 4
    #define PEPNUM3 3
    #define PEPNUM3_BIT 3
    #define PEPNUM3_MASK 8
    #define PTOKEN0 4
    #define PTOKEN0_BIT 4
    #define PTOKEN0_MASK 16
    #define PTOKEN1 5
    #define PTOKEN1_BIT 5
    #define PTOKEN1_MASK 32
    #define PTYPE0 6
    #define PTYPE0_BIT 6
    #define PTYPE0_MASK 64
    #define PTYPE1 7
    #define PTYPE1_BIT 7
    #define PTYPE1_MASK 128

    sfrb UECONX = 0xeb;
    #define EPEN 0
    #define EPEN_BIT 0
    #define EPEN_MASK 1
    #define RSTDT 3
    #define RSTDT_BIT 3
    #define RSTDT_MASK 8
    #define STALLRQC 4
    #define STALLRQC_BIT 4
    #define STALLRQC_MASK 16
    #define STALLRQ 5
    #define STALLRQ_BIT 5
    #define STALLRQ_MASK 32

    sfrb UPCONX = 0xa9;
    #define PEN 0
    #define PEN_BIT 0
    #define PEN_MASK 1
    #define RSTDT 3
    #define RSTDT_BIT 3
    #define RSTDT_MASK 8
    #define INMODE 5
    #define INMODE_BIT 5
    #define INMODE_MASK 32
    #define PFREEZE 6
    #define PFREEZE_BIT 6
    #define PFREEZE_MASK 64

    sfrb UERST = 0xea;
    #define EPRST0 0
    #define EPRST0_BIT 0
    #define EPRST0_MASK 1
    #define EPRST1 1
    #define EPRST1_BIT 1
    #define EPRST1_MASK 2
    #define EPRST2 2
    #define EPRST2_BIT 2
    #define EPRST2_MASK 4
    #define EPRST3 3
    #define EPRST3_BIT 3
    #define EPRST3_MASK 8
    #define EPRST4 4
    #define EPRST4_BIT 4
    #define EPRST4_MASK 16
    #define EPRST5 5
    #define EPRST5_BIT 5
    #define EPRST5_MASK 32
    #define EPRST6 6
    #define EPRST6_BIT 6
    #define EPRST6_MASK 64

    sfrb UPRST = 0xa8;
    #define PRST0 0
    #define PRST0_BIT 0
    #define PRST0_MASK 1
    #define PRST1 1
    #define PRST1_BIT 1
    #define PRST1_MASK 2
    #define PRST2 2
    #define PRST2_BIT 2
    #define PRST2_MASK 4
    #define PRST3 3
    #define PRST3_BIT 3
    #define PRST3_MASK 8
    #define PRST4 4
    #define PRST4_BIT 4
    #define PRST4_MASK 16
    #define PRST5 5
    #define PRST5_BIT 5
    #define PRST5_MASK 32
    #define PRST6 6
    #define PRST6_BIT 6
    #define PRST6_MASK 64

    sfrb UENUM = 0xe9;
    #define UENUM_0 0
    #define UENUM_0_BIT 0
    #define UENUM_0_MASK 1
    #define UENUM_1 1
    #define UENUM_1_BIT 1
    #define UENUM_1_MASK 2
    #define UENUM_2 2
    #define UENUM_2_BIT 2
    #define UENUM_2_MASK 4

    sfrb UPNUM = 0xa7;
    #define PNUM0 0
    #define PNUM0_BIT 0
    #define PNUM0_MASK 1
    #define PNUM1 1
    #define PNUM1_BIT 1
    #define PNUM1_MASK 2
    #define PNUM2 2
    #define PNUM2_BIT 2
    #define PNUM2_MASK 4

    sfrb UEINTX = 0xe8;
    #define TXINI 0
    #define TXINI_BIT 0
    #define TXINI_MASK 1
    #define STALLEDI 1
    #define STALLEDI_BIT 1
    #define STALLEDI_MASK 2
    #define RXOUTI 2
    #define RXOUTI_BIT 2
    #define RXOUTI_MASK 4
    #define RXSTPI 3
    #define RXSTPI_BIT 3
    #define RXSTPI_MASK 8
    #define NAKOUTI 4
    #define NAKOUTI_BIT 4
    #define NAKOUTI_MASK 16
    #define RWAL 5
    #define RWAL_BIT 5
    #define RWAL_MASK 32
    #define NAKINI 6
    #define NAKINI_BIT 6
    #define NAKINI_MASK 64
    #define FIFOCON 7
    #define FIFOCON_BIT 7
    #define FIFOCON_MASK 128

    sfrb UPINTX = 0xa6;
    #define RXINI 0
    #define RXINI_BIT 0
    #define RXINI_MASK 1
    #define RXSTALLI 1
    #define RXSTALLI_BIT 1
    #define RXSTALLI_MASK 2
    #define TXOUTI 2
    #define TXOUTI_BIT 2
    #define TXOUTI_MASK 4
    #define TXSTPI 3
    #define TXSTPI_BIT 3
    #define TXSTPI_MASK 8
    #define PERRI 4
    #define PERRI_BIT 4
    #define PERRI_MASK 16
    #define RWAL 5
    #define RWAL_BIT 5
    #define RWAL_MASK 32
    #define NAKEDI 6
    #define NAKEDI_BIT 6
    #define NAKEDI_MASK 64
    #define FIFOCON 7
    #define FIFOCON_BIT 7
    #define FIFOCON_MASK 128

    sfrb UDTST = 0xe7;

    sfrb UPINRQX = 0xa5;
    #define INRQ0 0
    #define INRQ0_BIT 0
    #define INRQ0_MASK 1
    #define INRQ1 1
    #define INRQ1_BIT 1
    #define INRQ1_MASK 2
    #define INRQ2 2
    #define INRQ2_BIT 2
    #define INRQ2_MASK 4
    #define INRQ3 3
    #define INRQ3_BIT 3
    #define INRQ3_MASK 8
    #define INRQ4 4
    #define INRQ4_BIT 4
    #define INRQ4_MASK 16
    #define INRQ5 5
    #define INRQ5_BIT 5
    #define INRQ5_MASK 32
    #define INRQ6 6
    #define INRQ6_BIT 6
    #define INRQ6_MASK 64
    #define INRQ7 7
    #define INRQ7_BIT 7
    #define INRQ7_MASK 128

    sfrb UDMFN = 0xe6;
    #define FNCERR 4
    #define FNCERR_BIT 4
    #define FNCERR_MASK 16

    sfrb UHFLEN = 0xa4;
    #define UHFLEN_0 0
    #define UHFLEN_0_BIT 0
    #define UHFLEN_0_MASK 1
    #define UHFLEN_1 1
    #define UHFLEN_1_BIT 1
    #define UHFLEN_1_MASK 2
    #define UHFLEN_2 2
    #define UHFLEN_2_BIT 2
    #define UHFLEN_2_MASK 4
    #define UHFLEN_3 3
    #define UHFLEN_3_BIT 3
    #define UHFLEN_3_MASK 8
    #define UHFLEN_4 4
    #define UHFLEN_4_BIT 4
    #define UHFLEN_4_MASK 16
    #define UHFLEN_5 5
    #define UHFLEN_5_BIT 5
    #define UHFLEN_5_MASK 32
    #define UHFLEN_6 6
    #define UHFLEN_6_BIT 6
    #define UHFLEN_6_MASK 64
    #define UHFLEN_7 7
    #define UHFLEN_7_BIT 7
    #define UHFLEN_7_MASK 128

    sfrb UDFNUMH = 0xe5;
    #define UDFNUMH_0 0
    #define UDFNUMH_0_BIT 0
    #define UDFNUMH_0_MASK 1
    #define UDFNUMH_1 1
    #define UDFNUMH_1_BIT 1
    #define UDFNUMH_1_MASK 2
    #define UDFNUMH_2 2
    #define UDFNUMH_2_BIT 2
    #define UDFNUMH_2_MASK 4

    sfrb UHFNUMH = 0xa3;
    #define UHFNUMH_0 0
    #define UHFNUMH_0_BIT 0
    #define UHFNUMH_0_MASK 1
    #define UHFNUMH_1 1
    #define UHFNUMH_1_BIT 1
    #define UHFNUMH_1_MASK 2
    #define UHFNUMH_2 2
    #define UHFNUMH_2_BIT 2
    #define UHFNUMH_2_MASK 4

    sfrb UDFNUML = 0xe4;
    #define UDFNUML_0 0
    #define UDFNUML_0_BIT 0
    #define UDFNUML_0_MASK 1
    #define UDFNUML_1 1
    #define UDFNUML_1_BIT 1
    #define UDFNUML_1_MASK 2
    #define UDFNUML_2 2
    #define UDFNUML_2_BIT 2
    #define UDFNUML_2_MASK 4
    #define UDFNUML_3 3
    #define UDFNUML_3_BIT 3
    #define UDFNUML_3_MASK 8
    #define UDFNUML_4 4
    #define UDFNUML_4_BIT 4
    #define UDFNUML_4_MASK 16
    #define UDFNUML_5 5
    #define UDFNUML_5_BIT 5
    #define UDFNUML_5_MASK 32
    #define UDFNUML_6 6
    #define UDFNUML_6_BIT 6
    #define UDFNUML_6_MASK 64
    #define UDFNUML_7 7
    #define UDFNUML_7_BIT 7
    #define UDFNUML_7_MASK 128

    sfrb UHFNUML = 0xa2;
    #define UHFNUML_0 0
    #define UHFNUML_0_BIT 0
    #define UHFNUML_0_MASK 1
    #define UHFNUML_1 1
    #define UHFNUML_1_BIT 1
    #define UHFNUML_1_MASK 2
    #define UHFNUML_2 2
    #define UHFNUML_2_BIT 2
    #define UHFNUML_2_MASK 4
    #define UHFNUML_3 3
    #define UHFNUML_3_BIT 3
    #define UHFNUML_3_MASK 8
    #define UHFNUML_4 4
    #define UHFNUML_4_BIT 4
    #define UHFNUML_4_MASK 16
    #define UHFNUML_5 5
    #define UHFNUML_5_BIT 5
    #define UHFNUML_5_MASK 32
    #define UHFNUML_6 6
    #define UHFNUML_6_BIT 6
    #define UHFNUML_6_MASK 64
    #define UHFNUML_7 7
    #define UHFNUML_7_BIT 7
    #define UHFNUML_7_MASK 128

    sfrb UDADDR = 0xe3;
    #define UDADDR0 0
    #define UDADDR0_BIT 0
    #define UDADDR0_MASK 1
    #define UDADDR1 1
    #define UDADDR1_BIT 1
    #define UDADDR1_MASK 2
    #define UDADDR2 2
    #define UDADDR2_BIT 2
    #define UDADDR2_MASK 4
    #define UDADDR3 3
    #define UDADDR3_BIT 3
    #define UDADDR3_MASK 8
    #define UDADDR4 4
    #define UDADDR4_BIT 4
    #define UDADDR4_MASK 16
    #define UDADDR5 5
    #define UDADDR5_BIT 5
    #define UDADDR5_MASK 32
    #define UDADDR6 6
    #define UDADDR6_BIT 6
    #define UDADDR6_MASK 64
    #define ADDEN 7
    #define ADDEN_BIT 7
    #define ADDEN_MASK 128

    sfrb UHADDR = 0xa1;
    #define UHADDR_0 0
    #define UHADDR_0_BIT 0
    #define UHADDR_0_MASK 1
    #define UHADDR_1 1
    #define UHADDR_1_BIT 1
    #define UHADDR_1_MASK 2
    #define UHADDR_2 2
    #define UHADDR_2_BIT 2
    #define UHADDR_2_MASK 4
    #define UHADDR_3 3
    #define UHADDR_3_BIT 3
    #define UHADDR_3_MASK 8
    #define UHADDR_4 4
    #define UHADDR_4_BIT 4
    #define UHADDR_4_MASK 16
    #define UHADDR_5 5
    #define UHADDR_5_BIT 5
    #define UHADDR_5_MASK 32
    #define UHADDR_6 6
    #define UHADDR_6_BIT 6
    #define UHADDR_6_MASK 64

    sfrb UDIEN = 0xe2;
    #define SUSPE 0
    #define SUSPE_BIT 0
    #define SUSPE_MASK 1
    #define MSOFE 1
    #define MSOFE_BIT 1
    #define MSOFE_MASK 2
    #define SOFE 2
    #define SOFE_BIT 2
    #define SOFE_MASK 4
    #define EORSTE 3
    #define EORSTE_BIT 3
    #define EORSTE_MASK 8
    #define WAKEUPE 4
    #define WAKEUPE_BIT 4
    #define WAKEUPE_MASK 16
    #define EORSME 5
    #define EORSME_BIT 5
    #define EORSME_MASK 32
    #define UPRSME 6
    #define UPRSME_BIT 6
    #define UPRSME_MASK 64

    sfrb UHIEN = 0xa0;
    #define DCONNE 0
    #define DCONNE_BIT 0
    #define DCONNE_MASK 1
    #define DDISCE 1
    #define DDISCE_BIT 1
    #define DDISCE_MASK 2
    #define RSTE 2
    #define RSTE_BIT 2
    #define RSTE_MASK 4
    #define RSMEDE 3
    #define RSMEDE_BIT 3
    #define RSMEDE_MASK 8
    #define RXRSME 4
    #define RXRSME_BIT 4
    #define RXRSME_MASK 16
    #define HSOFE 5
    #define HSOFE_BIT 5
    #define HSOFE_MASK 32
    #define HWUPE 6
    #define HWUPE_BIT 6
    #define HWUPE_MASK 64

    sfrb UDINT = 0xe1;
    #define SUSPI 0
    #define SUSPI_BIT 0
    #define SUSPI_MASK 1
    #define MSOFI 1
    #define MSOFI_BIT 1
    #define MSOFI_MASK 2
    #define SOFI 2
    #define SOFI_BIT 2
    #define SOFI_MASK 4
    #define EORSTI 3
    #define EORSTI_BIT 3
    #define EORSTI_MASK 8
    #define WAKEUPI 4
    #define WAKEUPI_BIT 4
    #define WAKEUPI_MASK 16
    #define EORSMI 5
    #define EORSMI_BIT 5
    #define EORSMI_MASK 32
    #define UPRSMI 6
    #define UPRSMI_BIT 6
    #define UPRSMI_MASK 64

    sfrb UHINT = 0x9f;
    #define DCONNI 0
    #define DCONNI_BIT 0
    #define DCONNI_MASK 1
    #define DDISCI 1
    #define DDISCI_BIT 1
    #define DDISCI_MASK 2
    #define RSTI 2
    #define RSTI_BIT 2
    #define RSTI_MASK 4
    #define RSMEDI 3
    #define RSMEDI_BIT 3
    #define RSMEDI_MASK 8
    #define RXRSMI 4
    #define RXRSMI_BIT 4
    #define RXRSMI_MASK 16
    #define HSOFI 5
    #define HSOFI_BIT 5
    #define HSOFI_MASK 32
    #define UHUPI 6
    #define UHUPI_BIT 6
    #define UHUPI_MASK 64

    sfrb UDCON = 0xe0;
    #define DETACH 0
    #define DETACH_BIT 0
    #define DETACH_MASK 1
    #define RMWKUP 1
    #define RMWKUP_BIT 1
    #define RMWKUP_MASK 2
    #define LSM 2
    #define LSM_BIT 2
    #define LSM_MASK 4

    sfrb UHCON = 0x9e;
    #define SOFEN 0
    #define SOFEN_BIT 0
    #define SOFEN_MASK 1
    #define RESET 1
    #define RESET_BIT 1
    #define RESET_MASK 2
    #define RESUME 2
    #define RESUME_BIT 2
    #define RESUME_MASK 4

    sfrb OTGINT = 0xdf;
    #define SRPI 0
    #define SRPI_BIT 0
    #define SRPI_MASK 1
    #define VBERRI 1
    #define VBERRI_BIT 1
    #define VBERRI_MASK 2
    #define BCERRI 2
    #define BCERRI_BIT 2
    #define BCERRI_MASK 4
    #define ROLEEXI 3
    #define ROLEEXI_BIT 3
    #define ROLEEXI_MASK 8
    #define HNPERRI 4
    #define HNPERRI_BIT 4
    #define HNPERRI_MASK 16
    #define STOI 5
    #define STOI_BIT 5
    #define STOI_MASK 32

    sfrb OTGIEN = 0xde;
    #define SRPE 0
    #define SRPE_BIT 0
    #define SRPE_MASK 1
    #define VBERRE 1
    #define VBERRE_BIT 1
    #define VBERRE_MASK 2
    #define BCERRE 2
    #define BCERRE_BIT 2
    #define BCERRE_MASK 4
    #define ROLEEXE 3
    #define ROLEEXE_BIT 3
    #define ROLEEXE_MASK 8
    #define HNPERRE 4
    #define HNPERRE_BIT 4
    #define HNPERRE_MASK 16
    #define STOE 5
    #define STOE_BIT 5
    #define STOE_MASK 32

    sfrb OTGCON = 0xdd;
    #define VBUSRQC 0
    #define VBUSRQC_BIT 0
    #define VBUSRQC_MASK 1
    #define VBUSREQ 1
    #define VBUSREQ_BIT 1
    #define VBUSREQ_MASK 2
    #define VBUSHWC 2
    #define VBUSHWC_BIT 2
    #define VBUSHWC_MASK 4
    #define SRPSEL 3
    #define SRPSEL_BIT 3
    #define SRPSEL_MASK 8
    #define SRPREQ 4
    #define SRPREQ_BIT 4
    #define SRPREQ_MASK 16
    #define HNPREQ 5
    #define HNPREQ_BIT 5
    #define HNPREQ_MASK 32

    sfrb OTGTCON = 0xf9;
    #define VALUE_2_0 0
    #define VALUE_2_0_BIT 0
    #define VALUE_2_0_MASK 1
    #define VALUE_2_1 1
    #define VALUE_2_1_BIT 1
    #define VALUE_2_1_MASK 2
    #define VALUE_2 2
    #define VALUE_2_BIT 2
    #define VALUE_2_MASK 4
    #define PAGE0 5
    #define PAGE0_BIT 5
    #define PAGE0_MASK 32
    #define PAGE1 6
    #define PAGE1_BIT 6
    #define PAGE1_MASK 64
    #define OTGTCON_7 7
    #define OTGTCON_7_BIT 7
    #define OTGTCON_7_MASK 128

    sfrb UDPADDH = 0xdc;

    sfrb UDPADDL = 0xdb;

    sfrw UDPADDW = 0xdb;

    sfrb USBINT = 0xda;
    #define VBUSTI 0
    #define VBUSTI_BIT 0
    #define VBUSTI_MASK 1
    #define IDTI 1
    #define IDTI_BIT 1
    #define IDTI_MASK 2

    sfrb USBSTA = 0xd9;
    #define VBUS 0
    #define VBUS_BIT 0
    #define VBUS_MASK 1
    #define ID 1
    #define ID_BIT 1
    #define ID_MASK 2
    #define SPEED 3
    #define SPEED_BIT 3
    #define SPEED_MASK 8

    sfrb USBCON = 0xd8;
    #define VBUSTE 0
    #define VBUSTE_BIT 0
    #define VBUSTE_MASK 1
    #define IDTE 1
    #define IDTE_BIT 1
    #define IDTE_MASK 2
    #define OTGPADE 4
    #define OTGPADE_BIT 4
    #define OTGPADE_MASK 16
    #define FRZCLK 5
    #define FRZCLK_BIT 5
    #define FRZCLK_MASK 32
    #define HOST 6
    #define HOST_BIT 6
    #define HOST_MASK 64
    #define USBE 7
    #define USBE_BIT 7
    #define USBE_MASK 128

    sfrb UHWCON = 0xd7;
    #define UVREGE 0
    #define UVREGE_BIT 0
    #define UVREGE_MASK 1
    #define UVCONE 4
    #define UVCONE_BIT 4
    #define UVCONE_MASK 16
    #define UIDE 6
    #define UIDE_BIT 6
    #define UIDE_MASK 64
    #define UIMOD 7
    #define UIMOD_BIT 7
    #define UIMOD_MASK 128

    sfrb UDR1 = 0xce;
    #define UDR1_0 0
    #define UDR1_0_BIT 0
    #define UDR1_0_MASK 1
    #define UDR1_1 1
    #define UDR1_1_BIT 1
    #define UDR1_1_MASK 2
    #define UDR1_2 2
    #define UDR1_2_BIT 2
    #define UDR1_2_MASK 4
    #define UDR1_3 3
    #define UDR1_3_BIT 3
    #define UDR1_3_MASK 8
    #define UDR1_4 4
    #define UDR1_4_BIT 4
    #define UDR1_4_MASK 16
    #define UDR1_5 5
    #define UDR1_5_BIT 5
    #define UDR1_5_MASK 32
    #define UDR1_6 6
    #define UDR1_6_BIT 6
    #define UDR1_6_MASK 64
    #define UDR1_7 7
    #define UDR1_7_BIT 7
    #define UDR1_7_MASK 128

    sfrb UBRR1H = 0xcd;
    #define UBRR8 0
    #define UBRR8_BIT 0
    #define UBRR8_MASK 1
    #define UBRR9 1
    #define UBRR9_BIT 1
    #define UBRR9_MASK 2
    #define UBRR10 2
    #define UBRR10_BIT 2
    #define UBRR10_MASK 4
    #define UBRR11 3
    #define UBRR11_BIT 3
    #define UBRR11_MASK 8

    sfrb UBRR1L = 0xcc;
    #define UBRR0 0
    #define UBRR0_BIT 0
    #define UBRR0_MASK 1
    #define UBRR1 1
    #define UBRR1_BIT 1
    #define UBRR1_MASK 2
    #define UBRR2 2
    #define UBRR2_BIT 2
    #define UBRR2_MASK 4
    #define UBRR3 3
    #define UBRR3_BIT 3
    #define UBRR3_MASK 8
    #define UBRR4 4
    #define UBRR4_BIT 4
    #define UBRR4_MASK 16
    #define UBRR5 5
    #define UBRR5_BIT 5
    #define UBRR5_MASK 32
    #define UBRR6 6
    #define UBRR6_BIT 6
    #define UBRR6_MASK 64
    #define UBRR7 7
    #define UBRR7_BIT 7
    #define UBRR7_MASK 128

    sfrw UBRR1W = 0xcc;

    sfrb UCSR1C = 0xca;
    #define UCPOL1 0
    #define UCPOL1_BIT 0
    #define UCPOL1_MASK 1
    #define UCSZ10 1
    #define UCSZ10_BIT 1
    #define UCSZ10_MASK 2
    #define UCSZ11 2
    #define UCSZ11_BIT 2
    #define UCSZ11_MASK 4
    #define USBS1 3
    #define USBS1_BIT 3
    #define USBS1_MASK 8
    #define UPM10 4
    #define UPM10_BIT 4
    #define UPM10_MASK 16
    #define UPM11 5
    #define UPM11_BIT 5
    #define UPM11_MASK 32
    #define UMSEL10 6
    #define UMSEL10_BIT 6
    #define UMSEL10_MASK 64
    #define UMSEL11 7
    #define UMSEL11_BIT 7
    #define UMSEL11_MASK 128

    sfrb UCSR1B = 0xc9;
    #define TXB81 0
    #define TXB81_BIT 0
    #define TXB81_MASK 1
    #define RXB81 1
    #define RXB81_BIT 1
    #define RXB81_MASK 2
    #define UCSZ12 2
    #define UCSZ12_BIT 2
    #define UCSZ12_MASK 4
    #define TXEN1 3
    #define TXEN1_BIT 3
    #define TXEN1_MASK 8
    #define RXEN1 4
    #define RXEN1_BIT 4
    #define RXEN1_MASK 16
    #define UDRIE1 5
    #define UDRIE1_BIT 5
    #define UDRIE1_MASK 32
    #define TXCIE1 6
    #define TXCIE1_BIT 6
    #define TXCIE1_MASK 64
    #define RXCIE1 7
    #define RXCIE1_BIT 7
    #define RXCIE1_MASK 128

    sfrb UCSR1A = 0xc8;
    #define MPCM1 0
    #define MPCM1_BIT 0
    #define MPCM1_MASK 1
    #define U2X1 1
    #define U2X1_BIT 1
    #define U2X1_MASK 2
    #define UPE1 2
    #define UPE1_BIT 2
    #define UPE1_MASK 4
    #define DOR1 3
    #define DOR1_BIT 3
    #define DOR1_MASK 8
    #define FE1 4
    #define FE1_BIT 4
    #define FE1_MASK 16
    #define UDRE1 5
    #define UDRE1_BIT 5
    #define UDRE1_MASK 32
    #define TXC1 6
    #define TXC1_BIT 6
    #define TXC1_MASK 64
    #define RXC1 7
    #define RXC1_BIT 7
    #define RXC1_MASK 128

    sfrb TWAMR = 0xbd;
    #define TWAM0 1
    #define TWAM0_BIT 1
    #define TWAM0_MASK 2
    #define TWAM1 2
    #define TWAM1_BIT 2
    #define TWAM1_MASK 4
    #define TWAM2 3
    #define TWAM2_BIT 3
    #define TWAM2_MASK 8
    #define TWAM3 4
    #define TWAM3_BIT 4
    #define TWAM3_MASK 16
    #define TWAM4 5
    #define TWAM4_BIT 5
    #define TWAM4_MASK 32
    #define TWAM5 6
    #define TWAM5_BIT 6
    #define TWAM5_MASK 64
    #define TWAM6 7
    #define TWAM6_BIT 7
    #define TWAM6_MASK 128

    sfrb TWCR = 0xbc;
    #define TWIE 0
    #define TWIE_BIT 0
    #define TWIE_MASK 1
    #define TWEN 2
    #define TWEN_BIT 2
    #define TWEN_MASK 4
    #define TWWC 3
    #define TWWC_BIT 3
    #define TWWC_MASK 8
    #define TWSTO 4
    #define TWSTO_BIT 4
    #define TWSTO_MASK 16
    #define TWSTA 5
    #define TWSTA_BIT 5
    #define TWSTA_MASK 32
    #define TWEA 6
    #define TWEA_BIT 6
    #define TWEA_MASK 64
    #define TWINT 7
    #define TWINT_BIT 7
    #define TWINT_MASK 128

    sfrb TWDR = 0xbb;
    #define TWD0 0
    #define TWD0_BIT 0
    #define TWD0_MASK 1
    #define TWD1 1
    #define TWD1_BIT 1
    #define TWD1_MASK 2
    #define TWD2 2
    #define TWD2_BIT 2
    #define TWD2_MASK 4
    #define TWD3 3
    #define TWD3_BIT 3
    #define TWD3_MASK 8
    #define TWD4 4
    #define TWD4_BIT 4
    #define TWD4_MASK 16
    #define TWD5 5
    #define TWD5_BIT 5
    #define TWD5_MASK 32
    #define TWD6 6
    #define TWD6_BIT 6
    #define TWD6_MASK 64
    #define TWD7 7
    #define TWD7_BIT 7
    #define TWD7_MASK 128

    sfrb TWAR = 0xba;
    #define TWGCE 0
    #define TWGCE_BIT 0
    #define TWGCE_MASK 1
    #define TWA0 1
    #define TWA0_BIT 1
    #define TWA0_MASK 2
    #define TWA1 2
    #define TWA1_BIT 2
    #define TWA1_MASK 4
    #define TWA2 3
    #define TWA2_BIT 3
    #define TWA2_MASK 8
    #define TWA3 4
    #define TWA3_BIT 4
    #define TWA3_MASK 16
    #define TWA4 5
    #define TWA4_BIT 5
    #define TWA4_MASK 32
    #define TWA5 6
    #define TWA5_BIT 6
    #define TWA5_MASK 64
    #define TWA6 7
    #define TWA6_BIT 7
    #define TWA6_MASK 128

    sfrb TWSR = 0xb9;
    #define TWPS0 0
    #define TWPS0_BIT 0
    #define TWPS0_MASK 1
    #define TWPS1 1
    #define TWPS1_BIT 1
    #define TWPS1_MASK 2
    #define TWS3 3
    #define TWS3_BIT 3
    #define TWS3_MASK 8
    #define TWS4 4
    #define TWS4_BIT 4
    #define TWS4_MASK 16
    #define TWS5 5
    #define TWS5_BIT 5
    #define TWS5_MASK 32
    #define TWS6 6
    #define TWS6_BIT 6
    #define TWS6_MASK 64
    #define TWS7 7
    #define TWS7_BIT 7
    #define TWS7_MASK 128

    sfrb TWBR = 0xb8;
    #define TWBR0 0
    #define TWBR0_BIT 0
    #define TWBR0_MASK 1
    #define TWBR1 1
    #define TWBR1_BIT 1
    #define TWBR1_MASK 2
    #define TWBR2 2
    #define TWBR2_BIT 2
    #define TWBR2_MASK 4
    #define TWBR3 3
    #define TWBR3_BIT 3
    #define TWBR3_MASK 8
    #define TWBR4 4
    #define TWBR4_BIT 4
    #define TWBR4_MASK 16
    #define TWBR5 5
    #define TWBR5_BIT 5
    #define TWBR5_MASK 32
    #define TWBR6 6
    #define TWBR6_BIT 6
    #define TWBR6_MASK 64
    #define TWBR7 7
    #define TWBR7_BIT 7
    #define TWBR7_MASK 128

    sfrb ASSR = 0xb6;
    #define TCR2BUB 0
    #define TCR2BUB_BIT 0
    #define TCR2BUB_MASK 1
    #define TCR2AUB 1
    #define TCR2AUB_BIT 1
    #define TCR2AUB_MASK 2
    #define OCR2BUB 2
    #define OCR2BUB_BIT 2
    #define OCR2BUB_MASK 4
    #define OCR2AUB 3
    #define OCR2AUB_BIT 3
    #define OCR2AUB_MASK 8
    #define TCN2UB 4
    #define TCN2UB_BIT 4
    #define TCN2UB_MASK 16
    #define AS2 5
    #define AS2_BIT 5
    #define AS2_MASK 32
    #define EXCLK 6
    #define EXCLK_BIT 6
    #define EXCLK_MASK 64

    sfrb OCR2B = 0xb4;
    #define OCR2_0 0
    #define OCR2_0_BIT 0
    #define OCR2_0_MASK 1
    #define OCR2_1 1
    #define OCR2_1_BIT 1
    #define OCR2_1_MASK 2
    #define OCR2_2 2
    #define OCR2_2_BIT 2
    #define OCR2_2_MASK 4
    #define OCR2_3 3
    #define OCR2_3_BIT 3
    #define OCR2_3_MASK 8
    #define OCR2_4 4
    #define OCR2_4_BIT 4
    #define OCR2_4_MASK 16
    #define OCR2_5 5
    #define OCR2_5_BIT 5
    #define OCR2_5_MASK 32
    #define OCR2_6 6
    #define OCR2_6_BIT 6
    #define OCR2_6_MASK 64
    #define OCR2_7 7
    #define OCR2_7_BIT 7
    #define OCR2_7_MASK 128

    sfrb OCR2A = 0xb3;
    #define OCR2_0 0
    #define OCR2_0_BIT 0
    #define OCR2_0_MASK 1
    #define OCR2_1 1
    #define OCR2_1_BIT 1
    #define OCR2_1_MASK 2
    #define OCR2_2 2
    #define OCR2_2_BIT 2
    #define OCR2_2_MASK 4
    #define OCR2_3 3
    #define OCR2_3_BIT 3
    #define OCR2_3_MASK 8
    #define OCR2_4 4
    #define OCR2_4_BIT 4
    #define OCR2_4_MASK 16
    #define OCR2_5 5
    #define OCR2_5_BIT 5
    #define OCR2_5_MASK 32
    #define OCR2_6 6
    #define OCR2_6_BIT 6
    #define OCR2_6_MASK 64
    #define OCR2_7 7
    #define OCR2_7_BIT 7
    #define OCR2_7_MASK 128

    sfrb TCNT2 = 0xb2;
    #define TCNT2_0 0
    #define TCNT2_0_BIT 0
    #define TCNT2_0_MASK 1
    #define TCNT2_1 1
    #define TCNT2_1_BIT 1
    #define TCNT2_1_MASK 2
    #define TCNT2_2 2
    #define TCNT2_2_BIT 2
    #define TCNT2_2_MASK 4
    #define TCNT2_3 3
    #define TCNT2_3_BIT 3
    #define TCNT2_3_MASK 8
    #define TCNT2_4 4
    #define TCNT2_4_BIT 4
    #define TCNT2_4_MASK 16
    #define TCNT2_5 5
    #define TCNT2_5_BIT 5
    #define TCNT2_5_MASK 32
    #define TCNT2_6 6
    #define TCNT2_6_BIT 6
    #define TCNT2_6_MASK 64
    #define TCNT2_7 7
    #define TCNT2_7_BIT 7
    #define TCNT2_7_MASK 128

    sfrb TCCR2B = 0xb1;
    #define CS20 0
    #define CS20_BIT 0
    #define CS20_MASK 1
    #define CS21 1
    #define CS21_BIT 1
    #define CS21_MASK 2
    #define CS22 2
    #define CS22_BIT 2
    #define CS22_MASK 4
    #define WGM22 3
    #define WGM22_BIT 3
    #define WGM22_MASK 8
    #define FOC2B 6
    #define FOC2B_BIT 6
    #define FOC2B_MASK 64
    #define FOC2A 7
    #define FOC2A_BIT 7
    #define FOC2A_MASK 128

    sfrb TCCR2A = 0xb0;
    #define WGM20 0
    #define WGM20_BIT 0
    #define WGM20_MASK 1
    #define WGM21 1
    #define WGM21_BIT 1
    #define WGM21_MASK 2
    #define COM2B0 4
    #define COM2B0_BIT 4
    #define COM2B0_MASK 16
    #define COM2B1 5
    #define COM2B1_BIT 5
    #define COM2B1_MASK 32
    #define COM2A0 6
    #define COM2A0_BIT 6
    #define COM2A0_MASK 64
    #define COM2A1 7
    #define COM2A1_BIT 7
    #define COM2A1_MASK 128

    sfrb OCR3CH = 0x9d;
    #define OCR3CH0 0
    #define OCR3CH0_BIT 0
    #define OCR3CH0_MASK 1
    #define OCR3CH1 1
    #define OCR3CH1_BIT 1
    #define OCR3CH1_MASK 2
    #define OCR3CH2 2
    #define OCR3CH2_BIT 2
    #define OCR3CH2_MASK 4
    #define OCR3CH3 3
    #define OCR3CH3_BIT 3
    #define OCR3CH3_MASK 8
    #define OCR3CH4 4
    #define OCR3CH4_BIT 4
    #define OCR3CH4_MASK 16
    #define OCR3CH5 5
    #define OCR3CH5_BIT 5
    #define OCR3CH5_MASK 32
    #define OCR3CH6 6
    #define OCR3CH6_BIT 6
    #define OCR3CH6_MASK 64
    #define OCR3CH7 7
    #define OCR3CH7_BIT 7
    #define OCR3CH7_MASK 128

    sfrb OCR3CL = 0x9c;
    #define OCR3CL0 0
    #define OCR3CL0_BIT 0
    #define OCR3CL0_MASK 1
    #define OCR3CL1 1
    #define OCR3CL1_BIT 1
    #define OCR3CL1_MASK 2
    #define OCR3CL2 2
    #define OCR3CL2_BIT 2
    #define OCR3CL2_MASK 4
    #define OCR3CL3 3
    #define OCR3CL3_BIT 3
    #define OCR3CL3_MASK 8
    #define OCR3CL4 4
    #define OCR3CL4_BIT 4
    #define OCR3CL4_MASK 16
    #define OCR3CL5 5
    #define OCR3CL5_BIT 5
    #define OCR3CL5_MASK 32
    #define OCR3CL6 6
    #define OCR3CL6_BIT 6
    #define OCR3CL6_MASK 64
    #define OCR3CL7 7
    #define OCR3CL7_BIT 7
    #define OCR3CL7_MASK 128

    sfrw OCR3CW = 0x9c;

    sfrb OCR3BH = 0x9b;
    #define OCR3BH0 0
    #define OCR3BH0_BIT 0
    #define OCR3BH0_MASK 1
    #define OCR3BH1 1
    #define OCR3BH1_BIT 1
    #define OCR3BH1_MASK 2
    #define OCR3BH2 2
    #define OCR3BH2_BIT 2
    #define OCR3BH2_MASK 4
    #define OCR3BH3 3
    #define OCR3BH3_BIT 3
    #define OCR3BH3_MASK 8
    #define OCR3BH4 4
    #define OCR3BH4_BIT 4
    #define OCR3BH4_MASK 16
    #define OCR3BH5 5
    #define OCR3BH5_BIT 5
    #define OCR3BH5_MASK 32
    #define OCR3BH6 6
    #define OCR3BH6_BIT 6
    #define OCR3BH6_MASK 64
    #define OCR3BH7 7
    #define OCR3BH7_BIT 7
    #define OCR3BH7_MASK 128

    sfrb OCR3BL = 0x9a;
    #define OCR3BL0 0
    #define OCR3BL0_BIT 0
    #define OCR3BL0_MASK 1
    #define OCR3BL1 1
    #define OCR3BL1_BIT 1
    #define OCR3BL1_MASK 2
    #define OCR3BL2 2
    #define OCR3BL2_BIT 2
    #define OCR3BL2_MASK 4
    #define OCR3BL3 3
    #define OCR3BL3_BIT 3
    #define OCR3BL3_MASK 8
    #define OCR3BL4 4
    #define OCR3BL4_BIT 4
    #define OCR3BL4_MASK 16
    #define OCR3BL5 5
    #define OCR3BL5_BIT 5
    #define OCR3BL5_MASK 32
    #define OCR3BL6 6
    #define OCR3BL6_BIT 6
    #define OCR3BL6_MASK 64
    #define OCR3BL7 7
    #define OCR3BL7_BIT 7
    #define OCR3BL7_MASK 128

    sfrw OCR3BW = 0x9a;

    sfrb OCR3AH = 0x99;
    #define OCR3AH0 0
    #define OCR3AH0_BIT 0
    #define OCR3AH0_MASK 1
    #define OCR3AH1 1
    #define OCR3AH1_BIT 1
    #define OCR3AH1_MASK 2
    #define OCR3AH2 2
    #define OCR3AH2_BIT 2
    #define OCR3AH2_MASK 4
    #define OCR3AH3 3
    #define OCR3AH3_BIT 3
    #define OCR3AH3_MASK 8
    #define OCR3AH4 4
    #define OCR3AH4_BIT 4
    #define OCR3AH4_MASK 16
    #define OCR3AH5 5
    #define OCR3AH5_BIT 5
    #define OCR3AH5_MASK 32
    #define OCR3AH6 6
    #define OCR3AH6_BIT 6
    #define OCR3AH6_MASK 64
    #define OCR3AH7 7
    #define OCR3AH7_BIT 7
    #define OCR3AH7_MASK 128

    sfrb OCR3AL = 0x98;
    #define OCR3AL0 0
    #define OCR3AL0_BIT 0
    #define OCR3AL0_MASK 1
    #define OCR3AL1 1
    #define OCR3AL1_BIT 1
    #define OCR3AL1_MASK 2
    #define OCR3AL2 2
    #define OCR3AL2_BIT 2
    #define OCR3AL2_MASK 4
    #define OCR3AL3 3
    #define OCR3AL3_BIT 3
    #define OCR3AL3_MASK 8
    #define OCR3AL4 4
    #define OCR3AL4_BIT 4
    #define OCR3AL4_MASK 16
    #define OCR3AL5 5
    #define OCR3AL5_BIT 5
    #define OCR3AL5_MASK 32
    #define OCR3AL6 6
    #define OCR3AL6_BIT 6
    #define OCR3AL6_MASK 64
    #define OCR3AL7 7
    #define OCR3AL7_BIT 7
    #define OCR3AL7_MASK 128

    sfrw OCR3AW = 0x98;

    sfrb ICR3H = 0x97;
    #define ICR3H0 0
    #define ICR3H0_BIT 0
    #define ICR3H0_MASK 1
    #define ICR3H1 1
    #define ICR3H1_BIT 1
    #define ICR3H1_MASK 2
    #define ICR3H2 2
    #define ICR3H2_BIT 2
    #define ICR3H2_MASK 4
    #define ICR3H3 3
    #define ICR3H3_BIT 3
    #define ICR3H3_MASK 8
    #define ICR3H4 4
    #define ICR3H4_BIT 4
    #define ICR3H4_MASK 16
    #define ICR3H5 5
    #define ICR3H5_BIT 5
    #define ICR3H5_MASK 32
    #define ICR3H6 6
    #define ICR3H6_BIT 6
    #define ICR3H6_MASK 64
    #define ICR3H7 7
    #define ICR3H7_BIT 7
    #define ICR3H7_MASK 128

    sfrb ICR3L = 0x96;
    #define ICR3L0 0
    #define ICR3L0_BIT 0
    #define ICR3L0_MASK 1
    #define ICR3L1 1
    #define ICR3L1_BIT 1
    #define ICR3L1_MASK 2
    #define ICR3L2 2
    #define ICR3L2_BIT 2
    #define ICR3L2_MASK 4
    #define ICR3L3 3
    #define ICR3L3_BIT 3
    #define ICR3L3_MASK 8
    #define ICR3L4 4
    #define ICR3L4_BIT 4
    #define ICR3L4_MASK 16
    #define ICR3L5 5
    #define ICR3L5_BIT 5
    #define ICR3L5_MASK 32
    #define ICR3L6 6
    #define ICR3L6_BIT 6
    #define ICR3L6_MASK 64
    #define ICR3L7 7
    #define ICR3L7_BIT 7
    #define ICR3L7_MASK 128

    sfrw ICR3W = 0x96;

    sfrb TCNT3H = 0x95;
    #define TCNT3H0 0
    #define TCNT3H0_BIT 0
    #define TCNT3H0_MASK 1
    #define TCNT3H1 1
    #define TCNT3H1_BIT 1
    #define TCNT3H1_MASK 2
    #define TCNT3H2 2
    #define TCNT3H2_BIT 2
    #define TCNT3H2_MASK 4
    #define TCNT3H3 3
    #define TCNT3H3_BIT 3
    #define TCNT3H3_MASK 8
    #define TCNT3H4 4
    #define TCNT3H4_BIT 4
    #define TCNT3H4_MASK 16
    #define TCNT3H5 5
    #define TCNT3H5_BIT 5
    #define TCNT3H5_MASK 32
    #define TCNT3H6 6
    #define TCNT3H6_BIT 6
    #define TCNT3H6_MASK 64
    #define TCNT3H7 7
    #define TCNT3H7_BIT 7
    #define TCNT3H7_MASK 128

    sfrb TCNT3L = 0x94;
    #define TCNT3L0 0
    #define TCNT3L0_BIT 0
    #define TCNT3L0_MASK 1
    #define TCNT3L1 1
    #define TCNT3L1_BIT 1
    #define TCNT3L1_MASK 2
    #define TCNT3L2 2
    #define TCNT3L2_BIT 2
    #define TCNT3L2_MASK 4
    #define TCNT3L3 3
    #define TCNT3L3_BIT 3
    #define TCNT3L3_MASK 8
    #define TCNT3L4 4
    #define TCNT3L4_BIT 4
    #define TCNT3L4_MASK 16
    #define TCNT3L5 5
    #define TCNT3L5_BIT 5
    #define TCNT3L5_MASK 32
    #define TCNT3L6 6
    #define TCNT3L6_BIT 6
    #define TCNT3L6_MASK 64
    #define TCNT3L7 7
    #define TCNT3L7_BIT 7
    #define TCNT3L7_MASK 128

    sfrw TCNT3W = 0x94;

    sfrb TCCR3C = 0x92;
    #define FOC3C 5
    #define FOC3C_BIT 5
    #define FOC3C_MASK 32
    #define FOC3B 6
    #define FOC3B_BIT 6
    #define FOC3B_MASK 64
    #define FOC3A 7
    #define FOC3A_BIT 7
    #define FOC3A_MASK 128

    sfrb TCCR3B = 0x91;
    #define CS30 0
    #define CS30_BIT 0
    #define CS30_MASK 1
    #define CS31 1
    #define CS31_BIT 1
    #define CS31_MASK 2
    #define CS32 2
    #define CS32_BIT 2
    #define CS32_MASK 4
    #define WGM32 3
    #define WGM32_BIT 3
    #define WGM32_MASK 8
    #define WGM33 4
    #define WGM33_BIT 4
    #define WGM33_MASK 16
    #define ICES3 6
    #define ICES3_BIT 6
    #define ICES3_MASK 64
    #define ICNC3 7
    #define ICNC3_BIT 7
    #define ICNC3_MASK 128

    sfrb TCCR3A = 0x90;
    #define WGM30 0
    #define WGM30_BIT 0
    #define WGM30_MASK 1
    #define WGM31 1
    #define WGM31_BIT 1
    #define WGM31_MASK 2
    #define COM3C0 2
    #define COM3C0_BIT 2
    #define COM3C0_MASK 4
    #define COM3C1 3
    #define COM3C1_BIT 3
    #define COM3C1_MASK 8
    #define COM3B0 4
    #define COM3B0_BIT 4
    #define COM3B0_MASK 16
    #define COM3B1 5
    #define COM3B1_BIT 5
    #define COM3B1_MASK 32
    #define COM3A0 6
    #define COM3A0_BIT 6
    #define COM3A0_MASK 64
    #define COM3A1 7
    #define COM3A1_BIT 7
    #define COM3A1_MASK 128

    sfrb OCR1CH = 0x8d;
    #define OCR1CH0 0
    #define OCR1CH0_BIT 0
    #define OCR1CH0_MASK 1
    #define OCR1CH1 1
    #define OCR1CH1_BIT 1
    #define OCR1CH1_MASK 2
    #define OCR1CH2 2
    #define OCR1CH2_BIT 2
    #define OCR1CH2_MASK 4
    #define OCR1CH3 3
    #define OCR1CH3_BIT 3
    #define OCR1CH3_MASK 8
    #define OCR1CH4 4
    #define OCR1CH4_BIT 4
    #define OCR1CH4_MASK 16
    #define OCR1CH5 5
    #define OCR1CH5_BIT 5
    #define OCR1CH5_MASK 32
    #define OCR1CH6 6
    #define OCR1CH6_BIT 6
    #define OCR1CH6_MASK 64
    #define OCR1CH7 7
    #define OCR1CH7_BIT 7
    #define OCR1CH7_MASK 128

    sfrb OCR1CL = 0x8c;
    #define OCR1CL0 0
    #define OCR1CL0_BIT 0
    #define OCR1CL0_MASK 1
    #define OCR1CL1 1
    #define OCR1CL1_BIT 1
    #define OCR1CL1_MASK 2
    #define OCR1CL2 2
    #define OCR1CL2_BIT 2
    #define OCR1CL2_MASK 4
    #define OCR1CL3 3
    #define OCR1CL3_BIT 3
    #define OCR1CL3_MASK 8
    #define OCR1CL4 4
    #define OCR1CL4_BIT 4
    #define OCR1CL4_MASK 16
    #define OCR1CL5 5
    #define OCR1CL5_BIT 5
    #define OCR1CL5_MASK 32
    #define OCR1CL6 6
    #define OCR1CL6_BIT 6
    #define OCR1CL6_MASK 64
    #define OCR1CL7 7
    #define OCR1CL7_BIT 7
    #define OCR1CL7_MASK 128

    sfrw OCR1CW = 0x8c;

    sfrb OCR1BH = 0x8b;
    #define OCR1BH0 0
    #define OCR1BH0_BIT 0
    #define OCR1BH0_MASK 1
    #define OCR1BH1 1
    #define OCR1BH1_BIT 1
    #define OCR1BH1_MASK 2
    #define OCR1BH2 2
    #define OCR1BH2_BIT 2
    #define OCR1BH2_MASK 4
    #define OCR1BH3 3
    #define OCR1BH3_BIT 3
    #define OCR1BH3_MASK 8
    #define OCR1BH4 4
    #define OCR1BH4_BIT 4
    #define OCR1BH4_MASK 16
    #define OCR1BH5 5
    #define OCR1BH5_BIT 5
    #define OCR1BH5_MASK 32
    #define OCR1BH6 6
    #define OCR1BH6_BIT 6
    #define OCR1BH6_MASK 64
    #define OCR1BH7 7
    #define OCR1BH7_BIT 7
    #define OCR1BH7_MASK 128

    sfrb OCR1BL = 0x8a;
    #define OCR1BL0 0
    #define OCR1BL0_BIT 0
    #define OCR1BL0_MASK 1
    #define OCR1BL1 1
    #define OCR1BL1_BIT 1
    #define OCR1BL1_MASK 2
    #define OCR1BL2 2
    #define OCR1BL2_BIT 2
    #define OCR1BL2_MASK 4
    #define OCR1BL3 3
    #define OCR1BL3_BIT 3
    #define OCR1BL3_MASK 8
    #define OCR1BL4 4
    #define OCR1BL4_BIT 4
    #define OCR1BL4_MASK 16
    #define OCR1BL5 5
    #define OCR1BL5_BIT 5
    #define OCR1BL5_MASK 32
    #define OCR1BL6 6
    #define OCR1BL6_BIT 6
    #define OCR1BL6_MASK 64
    #define OCR1BL7 7
    #define OCR1BL7_BIT 7
    #define OCR1BL7_MASK 128

    sfrw OCR1BW = 0x8a;

    sfrb OCR1AH = 0x89;
    #define OCR1AH0 0
    #define OCR1AH0_BIT 0
    #define OCR1AH0_MASK 1
    #define OCR1AH1 1
    #define OCR1AH1_BIT 1
    #define OCR1AH1_MASK 2
    #define OCR1AH2 2
    #define OCR1AH2_BIT 2
    #define OCR1AH2_MASK 4
    #define OCR1AH3 3
    #define OCR1AH3_BIT 3
    #define OCR1AH3_MASK 8
    #define OCR1AH4 4
    #define OCR1AH4_BIT 4
    #define OCR1AH4_MASK 16
    #define OCR1AH5 5
    #define OCR1AH5_BIT 5
    #define OCR1AH5_MASK 32
    #define OCR1AH6 6
    #define OCR1AH6_BIT 6
    #define OCR1AH6_MASK 64
    #define OCR1AH7 7
    #define OCR1AH7_BIT 7
    #define OCR1AH7_MASK 128

    sfrb OCR1AL = 0x88;
    #define OCR1AL0 0
    #define OCR1AL0_BIT 0
    #define OCR1AL0_MASK 1
    #define OCR1AL1 1
    #define OCR1AL1_BIT 1
    #define OCR1AL1_MASK 2
    #define OCR1AL2 2
    #define OCR1AL2_BIT 2
    #define OCR1AL2_MASK 4
    #define OCR1AL3 3
    #define OCR1AL3_BIT 3
    #define OCR1AL3_MASK 8
    #define OCR1AL4 4
    #define OCR1AL4_BIT 4
    #define OCR1AL4_MASK 16
    #define OCR1AL5 5
    #define OCR1AL5_BIT 5
    #define OCR1AL5_MASK 32
    #define OCR1AL6 6
    #define OCR1AL6_BIT 6
    #define OCR1AL6_MASK 64
    #define OCR1AL7 7
    #define OCR1AL7_BIT 7
    #define OCR1AL7_MASK 128

    sfrw OCR1AW = 0x88;

    sfrb ICR1H = 0x87;
    #define ICR1H0 0
    #define ICR1H0_BIT 0
    #define ICR1H0_MASK 1
    #define ICR1H1 1
    #define ICR1H1_BIT 1
    #define ICR1H1_MASK 2
    #define ICR1H2 2
    #define ICR1H2_BIT 2
    #define ICR1H2_MASK 4
    #define ICR1H3 3
    #define ICR1H3_BIT 3
    #define ICR1H3_MASK 8
    #define ICR1H4 4
    #define ICR1H4_BIT 4
    #define ICR1H4_MASK 16
    #define ICR1H5 5
    #define ICR1H5_BIT 5
    #define ICR1H5_MASK 32
    #define ICR1H6 6
    #define ICR1H6_BIT 6
    #define ICR1H6_MASK 64
    #define ICR1H7 7
    #define ICR1H7_BIT 7
    #define ICR1H7_MASK 128

    sfrb ICR1L = 0x86;
    #define ICR1L0 0
    #define ICR1L0_BIT 0
    #define ICR1L0_MASK 1
    #define ICR1L1 1
    #define ICR1L1_BIT 1
    #define ICR1L1_MASK 2
    #define ICR1L2 2
    #define ICR1L2_BIT 2
    #define ICR1L2_MASK 4
    #define ICR1L3 3
    #define ICR1L3_BIT 3
    #define ICR1L3_MASK 8
    #define ICR1L4 4
    #define ICR1L4_BIT 4
    #define ICR1L4_MASK 16
    #define ICR1L5 5
    #define ICR1L5_BIT 5
    #define ICR1L5_MASK 32
    #define ICR1L6 6
    #define ICR1L6_BIT 6
    #define ICR1L6_MASK 64
    #define ICR1L7 7
    #define ICR1L7_BIT 7
    #define ICR1L7_MASK 128

    sfrw ICR1W = 0x86;

    sfrb TCNT1H = 0x85;
    #define TCNT1H0 0
    #define TCNT1H0_BIT 0
    #define TCNT1H0_MASK 1
    #define TCNT1H1 1
    #define TCNT1H1_BIT 1
    #define TCNT1H1_MASK 2
    #define TCNT1H2 2
    #define TCNT1H2_BIT 2
    #define TCNT1H2_MASK 4
    #define TCNT1H3 3
    #define TCNT1H3_BIT 3
    #define TCNT1H3_MASK 8
    #define TCNT1H4 4
    #define TCNT1H4_BIT 4
    #define TCNT1H4_MASK 16
    #define TCNT1H5 5
    #define TCNT1H5_BIT 5
    #define TCNT1H5_MASK 32
    #define TCNT1H6 6
    #define TCNT1H6_BIT 6
    #define TCNT1H6_MASK 64
    #define TCNT1H7 7
    #define TCNT1H7_BIT 7
    #define TCNT1H7_MASK 128

    sfrb TCNT1L = 0x84;
    #define TCNT1L0 0
    #define TCNT1L0_BIT 0
    #define TCNT1L0_MASK 1
    #define TCNT1L1 1
    #define TCNT1L1_BIT 1
    #define TCNT1L1_MASK 2
    #define TCNT1L2 2
    #define TCNT1L2_BIT 2
    #define TCNT1L2_MASK 4
    #define TCNT1L3 3
    #define TCNT1L3_BIT 3
    #define TCNT1L3_MASK 8
    #define TCNT1L4 4
    #define TCNT1L4_BIT 4
    #define TCNT1L4_MASK 16
    #define TCNT1L5 5
    #define TCNT1L5_BIT 5
    #define TCNT1L5_MASK 32
    #define TCNT1L6 6
    #define TCNT1L6_BIT 6
    #define TCNT1L6_MASK 64
    #define TCNT1L7 7
    #define TCNT1L7_BIT 7
    #define TCNT1L7_MASK 128

    sfrw TCNT1W = 0x84;

    sfrb TCCR1C = 0x82;
    #define FOC1C 5
    #define FOC1C_BIT 5
    #define FOC1C_MASK 32
    #define FOC1B 6
    #define FOC1B_BIT 6
    #define FOC1B_MASK 64
    #define FOC1A 7
    #define FOC1A_BIT 7
    #define FOC1A_MASK 128

    sfrb TCCR1B = 0x81;
    #define CS10 0
    #define CS10_BIT 0
    #define CS10_MASK 1
    #define CS11 1
    #define CS11_BIT 1
    #define CS11_MASK 2
    #define CS12 2
    #define CS12_BIT 2
    #define CS12_MASK 4
    #define WGM12 3
    #define WGM12_BIT 3
    #define WGM12_MASK 8
    #define WGM13 4
    #define WGM13_BIT 4
    #define WGM13_MASK 16
    #define ICES1 6
    #define ICES1_BIT 6
    #define ICES1_MASK 64
    #define ICNC1 7
    #define ICNC1_BIT 7
    #define ICNC1_MASK 128

    sfrb TCCR1A = 0x80;
    #define WGM10 0
    #define WGM10_BIT 0
    #define WGM10_MASK 1
    #define WGM11 1
    #define WGM11_BIT 1
    #define WGM11_MASK 2
    #define COM1C0 2
    #define COM1C0_BIT 2
    #define COM1C0_MASK 4
    #define COM1C1 3
    #define COM1C1_BIT 3
    #define COM1C1_MASK 8
    #define COM1B0 4
    #define COM1B0_BIT 4
    #define COM1B0_MASK 16
    #define COM1B1 5
    #define COM1B1_BIT 5
    #define COM1B1_MASK 32
    #define COM1A0 6
    #define COM1A0_BIT 6
    #define COM1A0_MASK 64
    #define COM1A1 7
    #define COM1A1_BIT 7
    #define COM1A1_MASK 128

    sfrb DIDR1 = 0x7f;
    #define AIN0D 0
    #define AIN0D_BIT 0
    #define AIN0D_MASK 1
    #define AIN1D 1
    #define AIN1D_BIT 1
    #define AIN1D_MASK 2

    sfrb DIDR0 = 0x7e;
    #define ADC0D 0
    #define ADC0D_BIT 0
    #define ADC0D_MASK 1
    #define ADC1D 1
    #define ADC1D_BIT 1
    #define ADC1D_MASK 2
    #define ADC2D 2
    #define ADC2D_BIT 2
    #define ADC2D_MASK 4
    #define ADC3D 3
    #define ADC3D_BIT 3
    #define ADC3D_MASK 8
    #define ADC4D 4
    #define ADC4D_BIT 4
    #define ADC4D_MASK 16
    #define ADC5D 5
    #define ADC5D_BIT 5
    #define ADC5D_MASK 32
    #define ADC6D 6
    #define ADC6D_BIT 6
    #define ADC6D_MASK 64
    #define ADC7D 7
    #define ADC7D_BIT 7
    #define ADC7D_MASK 128

    sfrb DIDR2 = 0x7d;

    sfrb ADMUX = 0x7c;
    #define MUX0 0
    #define MUX0_BIT 0
    #define MUX0_MASK 1
    #define MUX1 1
    #define MUX1_BIT 1
    #define MUX1_MASK 2
    #define MUX2 2
    #define MUX2_BIT 2
    #define MUX2_MASK 4
    #define MUX3 3
    #define MUX3_BIT 3
    #define MUX3_MASK 8
    #define MUX4 4
    #define MUX4_BIT 4
    #define MUX4_MASK 16
    #define ADLAR 5
    #define ADLAR_BIT 5
    #define ADLAR_MASK 32
    #define REFS0 6
    #define REFS0_BIT 6
    #define REFS0_MASK 64
    #define REFS1 7
    #define REFS1_BIT 7
    #define REFS1_MASK 128

    sfrb ADCSRB = 0x7b;
    #define ADTS0 0
    #define ADTS0_BIT 0
    #define ADTS0_MASK 1
    #define ADTS1 1
    #define ADTS1_BIT 1
    #define ADTS1_MASK 2
    #define ADTS2 2
    #define ADTS2_BIT 2
    #define ADTS2_MASK 4
    #define ACME 6
    #define ACME_BIT 6
    #define ACME_MASK 64
    #define ADHSM 7
    #define ADHSM_BIT 7
    #define ADHSM_MASK 128

    sfrb ADCSRA = 0x7a;
    #define ADPS0 0
    #define ADPS0_BIT 0
    #define ADPS0_MASK 1
    #define ADPS1 1
    #define ADPS1_BIT 1
    #define ADPS1_MASK 2
    #define ADPS2 2
    #define ADPS2_BIT 2
    #define ADPS2_MASK 4
    #define ADIE 3
    #define ADIE_BIT 3
    #define ADIE_MASK 8
    #define ADIF 4
    #define ADIF_BIT 4
    #define ADIF_MASK 16
    #define ADATE 5
    #define ADATE_BIT 5
    #define ADATE_MASK 32
    #define ADSC 6
    #define ADSC_BIT 6
    #define ADSC_MASK 64
    #define ADEN 7
    #define ADEN_BIT 7
    #define ADEN_MASK 128

    sfrb ADCH = 0x79;
    #define ADCH0 0
    #define ADCH0_BIT 0
    #define ADCH0_MASK 1
    #define ADCH1 1
    #define ADCH1_BIT 1
    #define ADCH1_MASK 2
    #define ADCH2 2
    #define ADCH2_BIT 2
    #define ADCH2_MASK 4
    #define ADCH3 3
    #define ADCH3_BIT 3
    #define ADCH3_MASK 8
    #define ADCH4 4
    #define ADCH4_BIT 4
    #define ADCH4_MASK 16
    #define ADCH5 5
    #define ADCH5_BIT 5
    #define ADCH5_MASK 32
    #define ADCH6 6
    #define ADCH6_BIT 6
    #define ADCH6_MASK 64
    #define ADCH7 7
    #define ADCH7_BIT 7
    #define ADCH7_MASK 128

    sfrb ADCL = 0x78;
    #define ADCL0 0
    #define ADCL0_BIT 0
    #define ADCL0_MASK 1
    #define ADCL1 1
    #define ADCL1_BIT 1
    #define ADCL1_MASK 2
    #define ADCL2 2
    #define ADCL2_BIT 2
    #define ADCL2_MASK 4
    #define ADCL3 3
    #define ADCL3_BIT 3
    #define ADCL3_MASK 8
    #define ADCL4 4
    #define ADCL4_BIT 4
    #define ADCL4_MASK 16
    #define ADCL5 5
    #define ADCL5_BIT 5
    #define ADCL5_MASK 32
    #define ADCL6 6
    #define ADCL6_BIT 6
    #define ADCL6_MASK 64
    #define ADCL7 7
    #define ADCL7_BIT 7
    #define ADCL7_MASK 128

    sfrw ADCW = 0x78;

    sfrb XMCRB = 0x75;
    #define XMM0 0
    #define XMM0_BIT 0
    #define XMM0_MASK 1
    #define XMM1 1
    #define XMM1_BIT 1
    #define XMM1_MASK 2
    #define XMM2 2
    #define XMM2_BIT 2
    #define XMM2_MASK 4
    #define XMBK 7
    #define XMBK_BIT 7
    #define XMBK_MASK 128

    sfrb XMCRA = 0x74;
    #define SRW00 0
    #define SRW00_BIT 0
    #define SRW00_MASK 1
    #define SRW01 1
    #define SRW01_BIT 1
    #define SRW01_MASK 2
    #define SRW10 2
    #define SRW10_BIT 2
    #define SRW10_MASK 4
    #define SRW11 3
    #define SRW11_BIT 3
    #define SRW11_MASK 8
    #define SRL0 4
    #define SRL0_BIT 4
    #define SRL0_MASK 16
    #define SRL1 5
    #define SRL1_BIT 5
    #define SRL1_MASK 32
    #define SRL2 6
    #define SRL2_BIT 6
    #define SRL2_MASK 64
    #define SRE 7
    #define SRE_BIT 7
    #define SRE_MASK 128

    sfrb TIMSK5 = 0x73;

    sfrb TIMSK4 = 0x72;

    sfrb TIMSK3 = 0x71;
    #define TOIE3 0
    #define TOIE3_BIT 0
    #define TOIE3_MASK 1
    #define OCIE3A 1
    #define OCIE3A_BIT 1
    #define OCIE3A_MASK 2
    #define OCIE3B 2
    #define OCIE3B_BIT 2
    #define OCIE3B_MASK 4
    #define OCIE3C 3
    #define OCIE3C_BIT 3
    #define OCIE3C_MASK 8
    #define ICIE3 5
    #define ICIE3_BIT 5
    #define ICIE3_MASK 32

    sfrb TIMSK2 = 0x70;
    #define TOIE2 0
    #define TOIE2_BIT 0
    #define TOIE2_MASK 1
    #define OCIE2A 1
    #define OCIE2A_BIT 1
    #define OCIE2A_MASK 2
    #define OCIE2B 2
    #define OCIE2B_BIT 2
    #define OCIE2B_MASK 4

    sfrb TIMSK1 = 0x6f;
    #define TOIE1 0
    #define TOIE1_BIT 0
    #define TOIE1_MASK 1
    #define OCIE1A 1
    #define OCIE1A_BIT 1
    #define OCIE1A_MASK 2
    #define OCIE1B 2
    #define OCIE1B_BIT 2
    #define OCIE1B_MASK 4
    #define OCIE1C 3
    #define OCIE1C_BIT 3
    #define OCIE1C_MASK 8
    #define ICIE1 5
    #define ICIE1_BIT 5
    #define ICIE1_MASK 32

    sfrb TIMSK0 = 0x6e;
    #define TOIE0 0
    #define TOIE0_BIT 0
    #define TOIE0_MASK 1
    #define OCIE0A 1
    #define OCIE0A_BIT 1
    #define OCIE0A_MASK 2
    #define OCIE0B 2
    #define OCIE0B_BIT 2
    #define OCIE0B_MASK 4

    sfrb PCMSK2 = 0x6d;

    sfrb PCMSK1 = 0x6c;

    sfrb PCMSK0 = 0x6b;
    #define PCINT0 0
    #define PCINT0_BIT 0
    #define PCINT0_MASK 1
    #define PCINT1 1
    #define PCINT1_BIT 1
    #define PCINT1_MASK 2
    #define PCINT2 2
    #define PCINT2_BIT 2
    #define PCINT2_MASK 4
    #define PCINT3 3
    #define PCINT3_BIT 3
    #define PCINT3_MASK 8
    #define PCINT4 4
    #define PCINT4_BIT 4
    #define PCINT4_MASK 16
    #define PCINT5 5
    #define PCINT5_BIT 5
    #define PCINT5_MASK 32
    #define PCINT6 6
    #define PCINT6_BIT 6
    #define PCINT6_MASK 64
    #define PCINT7 7
    #define PCINT7_BIT 7
    #define PCINT7_MASK 128

    sfrb EICRB = 0x6a;
    #define ISC40 0
    #define ISC40_BIT 0
    #define ISC40_MASK 1
    #define ISC41 1
    #define ISC41_BIT 1
    #define ISC41_MASK 2
    #define ISC50 2
    #define ISC50_BIT 2
    #define ISC50_MASK 4
    #define ISC51 3
    #define ISC51_BIT 3
    #define ISC51_MASK 8
    #define ISC60 4
    #define ISC60_BIT 4
    #define ISC60_MASK 16
    #define ISC61 5
    #define ISC61_BIT 5
    #define ISC61_MASK 32
    #define ISC70 6
    #define ISC70_BIT 6
    #define ISC70_MASK 64
    #define ISC71 7
    #define ISC71_BIT 7
    #define ISC71_MASK 128

    sfrb EICRA = 0x69;
    #define ISC00 0
    #define ISC00_BIT 0
    #define ISC00_MASK 1
    #define ISC01 1
    #define ISC01_BIT 1
    #define ISC01_MASK 2
    #define ISC10 2
    #define ISC10_BIT 2
    #define ISC10_MASK 4
    #define ISC11 3
    #define ISC11_BIT 3
    #define ISC11_MASK 8
    #define ISC20 4
    #define ISC20_BIT 4
    #define ISC20_MASK 16
    #define ISC21 5
    #define ISC21_BIT 5
    #define ISC21_MASK 32
    #define ISC30 6
    #define ISC30_BIT 6
    #define ISC30_MASK 64
    #define ISC31 7
    #define ISC31_BIT 7
    #define ISC31_MASK 128

    sfrb PCICR = 0x68;
    #define PCIE0 0
    #define PCIE0_BIT 0
    #define PCIE0_MASK 1
    #define PCIE1 1
    #define PCIE1_BIT 1
    #define PCIE1_MASK 2
    #define PCIE2 2
    #define PCIE2_BIT 2
    #define PCIE2_MASK 4

    sfrb OSCCAL = 0x66;
    #define CAL0 0
    #define CAL0_BIT 0
    #define CAL0_MASK 1
    #define CAL1 1
    #define CAL1_BIT 1
    #define CAL1_MASK 2
    #define CAL2 2
    #define CAL2_BIT 2
    #define CAL2_MASK 4
    #define CAL3 3
    #define CAL3_BIT 3
    #define CAL3_MASK 8
    #define CAL4 4
    #define CAL4_BIT 4
    #define CAL4_MASK 16
    #define CAL5 5
    #define CAL5_BIT 5
    #define CAL5_MASK 32
    #define CAL6 6
    #define CAL6_BIT 6
    #define CAL6_MASK 64
    #define CAL7 7
    #define CAL7_BIT 7
    #define CAL7_MASK 128

    sfrb PRR1 = 0x65;
    #define PRUSART1 0
    #define PRUSART1_BIT 0
    #define PRUSART1_MASK 1
    #define PRUSART2 1
    #define PRUSART2_BIT 1
    #define PRUSART2_MASK 2
    #define PRUSART3 2
    #define PRUSART3_BIT 2
    #define PRUSART3_MASK 4
    #define PRTIM3 3
    #define PRTIM3_BIT 3
    #define PRTIM3_MASK 8
    #define PRTIM4 4
    #define PRTIM4_BIT 4
    #define PRTIM4_MASK 16
    #define PRTIM5 5
    #define PRTIM5_BIT 5
    #define PRTIM5_MASK 32

    sfrb PRR0 = 0x64;
    #define PRADC 0
    #define PRADC_BIT 0
    #define PRADC_MASK 1
    #define PRUSART0 1
    #define PRUSART0_BIT 1
    #define PRUSART0_MASK 2
    #define PRSPI 2
    #define PRSPI_BIT 2
    #define PRSPI_MASK 4
    #define PRTIM1 3
    #define PRTIM1_BIT 3
    #define PRTIM1_MASK 8
    #define PRTIM0 5
    #define PRTIM0_BIT 5
    #define PRTIM0_MASK 32
    #define PRTIM2 6
    #define PRTIM2_BIT 6
    #define PRTIM2_MASK 64
    #define PRTWI 7
    #define PRTWI_BIT 7
    #define PRTWI_MASK 128

    sfrb CLKPR = 0x61;
    #define CLKPS0 0
    #define CLKPS0_BIT 0
    #define CLKPS0_MASK 1
    #define CLKPS1 1
    #define CLKPS1_BIT 1
    #define CLKPS1_MASK 2
    #define CLKPS2 2
    #define CLKPS2_BIT 2
    #define CLKPS2_MASK 4
    #define CLKPS3 3
    #define CLKPS3_BIT 3
    #define CLKPS3_MASK 8
    #define CLKPCE 7
    #define CLKPCE_BIT 7
    #define CLKPCE_MASK 128

    sfrb WDTCSR = 0x60;
    #define WDP0 0
    #define WDP0_BIT 0
    #define WDP0_MASK 1
    #define WDP1 1
    #define WDP1_BIT 1
    #define WDP1_MASK 2
    #define WDP2 2
    #define WDP2_BIT 2
    #define WDP2_MASK 4
    #define WDE 3
    #define WDE_BIT 3
    #define WDE_MASK 8
    #define WDCE 4
    #define WDCE_BIT 4
    #define WDCE_MASK 16
    #define WDP3 5
    #define WDP3_BIT 5
    #define WDP3_MASK 32
    #define WDIE 6
    #define WDIE_BIT 6
    #define WDIE_MASK 64
    #define WDIF 7
    #define WDIF_BIT 7
    #define WDIF_MASK 128

    sfrb SREG = 0x5f;

    sfrb SPH = 0x5e;
    #define SP8 0
    #define SP8_BIT 0
    #define SP8_MASK 1
    #define SP9 1
    #define SP9_BIT 1
    #define SP9_MASK 2
    #define SP10 2
    #define SP10_BIT 2
    #define SP10_MASK 4
    #define SP11 3
    #define SP11_BIT 3
    #define SP11_MASK 8
    #define SP12 4
    #define SP12_BIT 4
    #define SP12_MASK 16
    #define SP13 5
    #define SP13_BIT 5
    #define SP13_MASK 32
    #define SP14 6
    #define SP14_BIT 6
    #define SP14_MASK 64
    #define SP15 7
    #define SP15_BIT 7
    #define SP15_MASK 128

    sfrb SPL = 0x5d;
    #define SP0 0
    #define SP0_BIT 0
    #define SP0_MASK 1
    #define SP1 1
    #define SP1_BIT 1
    #define SP1_MASK 2
    #define SP2 2
    #define SP2_BIT 2
    #define SP2_MASK 4
    #define SP3 3
    #define SP3_BIT 3
    #define SP3_MASK 8
    #define SP4 4
    #define SP4_BIT 4
    #define SP4_MASK 16
    #define SP5 5
    #define SP5_BIT 5
    #define SP5_MASK 32
    #define SP6 6
    #define SP6_BIT 6
    #define SP6_MASK 64
    #define SP7 7
    #define SP7_BIT 7
    #define SP7_MASK 128

    sfrw SPW = 0x5d;

    sfrb EIND = 0x5c;
    #define EIND0 0
    #define EIND0_BIT 0
    #define EIND0_MASK 1

    sfrb RAMPZ = 0x5b;
    #define RAMPZ0 0
    #define RAMPZ0_BIT 0
    #define RAMPZ0_MASK 1

    sfrb SPMCSR = 0x57;
    #define SPMEN 0
    #define SPMEN_BIT 0
    #define SPMEN_MASK 1
    #define PGERS 1
    #define PGERS_BIT 1
    #define PGERS_MASK 2
    #define PGWRT 2
    #define PGWRT_BIT 2
    #define PGWRT_MASK 4
    #define BLBSET 3
    #define BLBSET_BIT 3
    #define BLBSET_MASK 8
    #define RWWSRE 4
    #define RWWSRE_BIT 4
    #define RWWSRE_MASK 16
    #define SIGRD 5
    #define SIGRD_BIT 5
    #define SIGRD_MASK 32
    #define RWWSB 6
    #define RWWSB_BIT 6
    #define RWWSB_MASK 64
    #define SPMIE 7
    #define SPMIE_BIT 7
    #define SPMIE_MASK 128

    sfrb MCUCR = 0x55;
    #define IVCE 0
    #define IVCE_BIT 0
    #define IVCE_MASK 1
    #define IVSEL 1
    #define IVSEL_BIT 1
    #define IVSEL_MASK 2
    #define PUD 4
    #define PUD_BIT 4
    #define PUD_MASK 16
    #define JTD 7
    #define JTD_BIT 7
    #define JTD_MASK 128

    sfrb MCUSR = 0x54;
    #define PORF 0
    #define PORF_BIT 0
    #define PORF_MASK 1
    #define EXTRF 1
    #define EXTRF_BIT 1
    #define EXTRF_MASK 2
    #define BORF 2
    #define BORF_BIT 2
    #define BORF_MASK 4
    #define WDRF 3
    #define WDRF_BIT 3
    #define WDRF_MASK 8
    #define JTRF 4
    #define JTRF_BIT 4
    #define JTRF_MASK 16

    sfrb SMCR = 0x53;
    #define SE 0
    #define SE_BIT 0
    #define SE_MASK 1
    #define SM0 1
    #define SM0_BIT 1
    #define SM0_MASK 2
    #define SM1 2
    #define SM1_BIT 2
    #define SM1_MASK 4
    #define SM2 3
    #define SM2_BIT 3
    #define SM2_MASK 8

    sfrb OCDR = 0x51;
    #define OCDR0 0
    #define OCDR0_BIT 0
    #define OCDR0_MASK 1
    #define OCDR1 1
    #define OCDR1_BIT 1
    #define OCDR1_MASK 2
    #define OCDR2 2
    #define OCDR2_BIT 2
    #define OCDR2_MASK 4
    #define OCDR3 3
    #define OCDR3_BIT 3
    #define OCDR3_MASK 8
    #define OCDR4 4
    #define OCDR4_BIT 4
    #define OCDR4_MASK 16
    #define OCDR5 5
    #define OCDR5_BIT 5
    #define OCDR5_MASK 32
    #define OCDR6 6
    #define OCDR6_BIT 6
    #define OCDR6_MASK 64
    #define OCDR7 7
    #define OCDR7_BIT 7
    #define OCDR7_MASK 128

    sfrb ACSR = 0x50;
    #define ACIS0 0
    #define ACIS0_BIT 0
    #define ACIS0_MASK 1
    #define ACIS1 1
    #define ACIS1_BIT 1
    #define ACIS1_MASK 2
    #define ACIC 2
    #define ACIC_BIT 2
    #define ACIC_MASK 4
    #define ACIE 3
    #define ACIE_BIT 3
    #define ACIE_MASK 8
    #define ACI 4
    #define ACI_BIT 4
    #define ACI_MASK 16
    #define ACO 5
    #define ACO_BIT 5
    #define ACO_MASK 32
    #define ACBG 6
    #define ACBG_BIT 6
    #define ACBG_MASK 64
    #define ACD 7
    #define ACD_BIT 7
    #define ACD_MASK 128

    sfrb SPDR = 0x4e;
    #define SPDR0 0
    #define SPDR0_BIT 0
    #define SPDR0_MASK 1
    #define SPDR1 1
    #define SPDR1_BIT 1
    #define SPDR1_MASK 2
    #define SPDR2 2
    #define SPDR2_BIT 2
    #define SPDR2_MASK 4
    #define SPDR3 3
    #define SPDR3_BIT 3
    #define SPDR3_MASK 8
    #define SPDR4 4
    #define SPDR4_BIT 4
    #define SPDR4_MASK 16
    #define SPDR5 5
    #define SPDR5_BIT 5
    #define SPDR5_MASK 32
    #define SPDR6 6
    #define SPDR6_BIT 6
    #define SPDR6_MASK 64
    #define SPDR7 7
    #define SPDR7_BIT 7
    #define SPDR7_MASK 128

    sfrb SPSR = 0x4d;
    #define SPI2X 0
    #define SPI2X_BIT 0
    #define SPI2X_MASK 1
    #define WCOL 6
    #define WCOL_BIT 6
    #define WCOL_MASK 64
    #define SPIF 7
    #define SPIF_BIT 7
    #define SPIF_MASK 128

    sfrb SPCR = 0x4c;
    #define SPR0 0
    #define SPR0_BIT 0
    #define SPR0_MASK 1
    #define SPR1 1
    #define SPR1_BIT 1
    #define SPR1_MASK 2
    #define CPHA 2
    #define CPHA_BIT 2
    #define CPHA_MASK 4
    #define CPOL 3
    #define CPOL_BIT 3
    #define CPOL_MASK 8
    #define MSTR 4
    #define MSTR_BIT 4
    #define MSTR_MASK 16
    #define DORD 5
    #define DORD_BIT 5
    #define DORD_MASK 32
    #define SPE 6
    #define SPE_BIT 6
    #define SPE_MASK 64
    #define SPIE 7
    #define SPIE_BIT 7
    #define SPIE_MASK 128

    sfrb GPIOR2 = 0x4b;
    #define GPIOR20 0
    #define GPIOR20_BIT 0
    #define GPIOR20_MASK 1
    #define GPIOR21 1
    #define GPIOR21_BIT 1
    #define GPIOR21_MASK 2
    #define GPIOR22 2
    #define GPIOR22_BIT 2
    #define GPIOR22_MASK 4
    #define GPIOR23 3
    #define GPIOR23_BIT 3
    #define GPIOR23_MASK 8
    #define GPIOR24 4
    #define GPIOR24_BIT 4
    #define GPIOR24_MASK 16
    #define GPIOR25 5
    #define GPIOR25_BIT 5
    #define GPIOR25_MASK 32
    #define GPIOR26 6
    #define GPIOR26_BIT 6
    #define GPIOR26_MASK 64
    #define GPIOR27 7
    #define GPIOR27_BIT 7
    #define GPIOR27_MASK 128

    sfrb GPIOR1 = 0x4a;
    #define GPIOR10 0
    #define GPIOR10_BIT 0
    #define GPIOR10_MASK 1
    #define GPIOR11 1
    #define GPIOR11_BIT 1
    #define GPIOR11_MASK 2
    #define GPIOR12 2
    #define GPIOR12_BIT 2
    #define GPIOR12_MASK 4
    #define GPIOR13 3
    #define GPIOR13_BIT 3
    #define GPIOR13_MASK 8
    #define GPIOR14 4
    #define GPIOR14_BIT 4
    #define GPIOR14_MASK 16
    #define GPIOR15 5
    #define GPIOR15_BIT 5
    #define GPIOR15_MASK 32
    #define GPIOR16 6
    #define GPIOR16_BIT 6
    #define GPIOR16_MASK 64
    #define GPIOR17 7
    #define GPIOR17_BIT 7
    #define GPIOR17_MASK 128

    sfrb OCR0B = 0x48;
    #define OCR0B_0 0
    #define OCR0B_0_BIT 0
    #define OCR0B_0_MASK 1
    #define OCR0B_1 1
    #define OCR0B_1_BIT 1
    #define OCR0B_1_MASK 2
    #define OCR0B_2 2
    #define OCR0B_2_BIT 2
    #define OCR0B_2_MASK 4
    #define OCR0B_3 3
    #define OCR0B_3_BIT 3
    #define OCR0B_3_MASK 8
    #define OCR0B_4 4
    #define OCR0B_4_BIT 4
    #define OCR0B_4_MASK 16
    #define OCR0B_5 5
    #define OCR0B_5_BIT 5
    #define OCR0B_5_MASK 32
    #define OCR0B_6 6
    #define OCR0B_6_BIT 6
    #define OCR0B_6_MASK 64
    #define OCR0B_7 7
    #define OCR0B_7_BIT 7
    #define OCR0B_7_MASK 128

    sfrb OCR0A = 0x47;
    #define OCROA_0 0
    #define OCROA_0_BIT 0
    #define OCROA_0_MASK 1
    #define OCROA_1 1
    #define OCROA_1_BIT 1
    #define OCROA_1_MASK 2
    #define OCROA_2 2
    #define OCROA_2_BIT 2
    #define OCROA_2_MASK 4
    #define OCROA_3 3
    #define OCROA_3_BIT 3
    #define OCROA_3_MASK 8
    #define OCROA_4 4
    #define OCROA_4_BIT 4
    #define OCROA_4_MASK 16
    #define OCROA_5 5
    #define OCROA_5_BIT 5
    #define OCROA_5_MASK 32
    #define OCROA_6 6
    #define OCROA_6_BIT 6
    #define OCROA_6_MASK 64
    #define OCROA_7 7
    #define OCROA_7_BIT 7
    #define OCROA_7_MASK 128

    sfrb TCNT0 = 0x46;
    #define TCNT0_0 0
    #define TCNT0_0_BIT 0
    #define TCNT0_0_MASK 1
    #define TCNT0_1 1
    #define TCNT0_1_BIT 1
    #define TCNT0_1_MASK 2
    #define TCNT0_2 2
    #define TCNT0_2_BIT 2
    #define TCNT0_2_MASK 4
    #define TCNT0_3 3
    #define TCNT0_3_BIT 3
    #define TCNT0_3_MASK 8
    #define TCNT0_4 4
    #define TCNT0_4_BIT 4
    #define TCNT0_4_MASK 16
    #define TCNT0_5 5
    #define TCNT0_5_BIT 5
    #define TCNT0_5_MASK 32
    #define TCNT0_6 6
    #define TCNT0_6_BIT 6
    #define TCNT0_6_MASK 64
    #define TCNT0_7 7
    #define TCNT0_7_BIT 7
    #define TCNT0_7_MASK 128

    sfrb TCCR0B = 0x45;
    #define CS00 0
    #define CS00_BIT 0
    #define CS00_MASK 1
    #define CS01 1
    #define CS01_BIT 1
    #define CS01_MASK 2
    #define CS02 2
    #define CS02_BIT 2
    #define CS02_MASK 4
    #define WGM02 3
    #define WGM02_BIT 3
    #define WGM02_MASK 8
    #define FOC0B 6
    #define FOC0B_BIT 6
    #define FOC0B_MASK 64
    #define FOC0A 7
    #define FOC0A_BIT 7
    #define FOC0A_MASK 128

    sfrb TCCR0A = 0x44;
    #define WGM00 0
    #define WGM00_BIT 0
    #define WGM00_MASK 1
    #define WGM01 1
    #define WGM01_BIT 1
    #define WGM01_MASK 2
    #define COM0B0 4
    #define COM0B0_BIT 4
    #define COM0B0_MASK 16
    #define COM0B1 5
    #define COM0B1_BIT 5
    #define COM0B1_MASK 32
    #define COM0A0 6
    #define COM0A0_BIT 6
    #define COM0A0_MASK 64
    #define COM0A1 7
    #define COM0A1_BIT 7
    #define COM0A1_MASK 128

    sfrb GTCCR = 0x43;
    #define PSRSYNC 0
    #define PSRSYNC_BIT 0
    #define PSRSYNC_MASK 1
    #define PSRASY 1
    #define PSRASY_BIT 1
    #define PSRASY_MASK 2
    #define TSM 7
    #define TSM_BIT 7
    #define TSM_MASK 128

    sfrb EEARH = 0x42;
    #define EEAR8 0
    #define EEAR8_BIT 0
    #define EEAR8_MASK 1
    #define EEAR9 1
    #define EEAR9_BIT 1
    #define EEAR9_MASK 2
    #define EEAR10 2
    #define EEAR10_BIT 2
    #define EEAR10_MASK 4
    #define EEAR11 3
    #define EEAR11_BIT 3
    #define EEAR11_MASK 8

    sfrb EEARL = 0x41;
    #define EEAR0 0
    #define EEAR0_BIT 0
    #define EEAR0_MASK 1
    #define EEAR1 1
    #define EEAR1_BIT 1
    #define EEAR1_MASK 2
    #define EEAR2 2
    #define EEAR2_BIT 2
    #define EEAR2_MASK 4
    #define EEAR3 3
    #define EEAR3_BIT 3
    #define EEAR3_MASK 8
    #define EEAR4 4
    #define EEAR4_BIT 4
    #define EEAR4_MASK 16
    #define EEAR5 5
    #define EEAR5_BIT 5
    #define EEAR5_MASK 32
    #define EEAR6 6
    #define EEAR6_BIT 6
    #define EEAR6_MASK 64
    #define EEAR7 7
    #define EEAR7_BIT 7
    #define EEAR7_MASK 128

    sfrw EEARW = 0x41;

    sfrb EEDR = 0x40;
    #define EEDR0 0
    #define EEDR0_BIT 0
    #define EEDR0_MASK 1
    #define EEDR1 1
    #define EEDR1_BIT 1
    #define EEDR1_MASK 2
    #define EEDR2 2
    #define EEDR2_BIT 2
    #define EEDR2_MASK 4
    #define EEDR3 3
    #define EEDR3_BIT 3
    #define EEDR3_MASK 8
    #define EEDR4 4
    #define EEDR4_BIT 4
    #define EEDR4_MASK 16
    #define EEDR5 5
    #define EEDR5_BIT 5
    #define EEDR5_MASK 32
    #define EEDR6 6
    #define EEDR6_BIT 6
    #define EEDR6_MASK 64
    #define EEDR7 7
    #define EEDR7_BIT 7
    #define EEDR7_MASK 128

    sfrb EECR = 0x3f;
    #define EERE 0
    #define EERE_BIT 0
    #define EERE_MASK 1
    #define EEPE 1
    #define EEPE_BIT 1
    #define EEPE_MASK 2
    #define EEMPE 2
    #define EEMPE_BIT 2
    #define EEMPE_MASK 4
    #define EERIE 3
    #define EERIE_BIT 3
    #define EERIE_MASK 8
    #define EEPM0 4
    #define EEPM0_BIT 4
    #define EEPM0_MASK 16
    #define EEPM1 5
    #define EEPM1_BIT 5
    #define EEPM1_MASK 32

    sfrb GPIOR0 = 0x3e;
    #define GPIOR00 0
    #define GPIOR00_BIT 0
    #define GPIOR00_MASK 1
    #define GPIOR01 1
    #define GPIOR01_BIT 1
    #define GPIOR01_MASK 2
    #define GPIOR02 2
    #define GPIOR02_BIT 2
    #define GPIOR02_MASK 4
    #define GPIOR03 3
    #define GPIOR03_BIT 3
    #define GPIOR03_MASK 8
    #define GPIOR04 4
    #define GPIOR04_BIT 4
    #define GPIOR04_MASK 16
    #define GPIOR05 5
    #define GPIOR05_BIT 5
    #define GPIOR05_MASK 32
    #define GPIOR06 6
    #define GPIOR06_BIT 6
    #define GPIOR06_MASK 64
    #define GPIOR07 7
    #define GPIOR07_BIT 7
    #define GPIOR07_MASK 128

    sfrb EIMSK = 0x3d;
    #define INT0 0
    #define INT0_BIT 0
    #define INT0_MASK 1
    #define INT1 1
    #define INT1_BIT 1
    #define INT1_MASK 2
    #define INT2 2
    #define INT2_BIT 2
    #define INT2_MASK 4
    #define INT3 3
    #define INT3_BIT 3
    #define INT3_MASK 8
    #define INT4 4
    #define INT4_BIT 4
    #define INT4_MASK 16
    #define INT5 5
    #define INT5_BIT 5
    #define INT5_MASK 32
    #define INT6 6
    #define INT6_BIT 6
    #define INT6_MASK 64
    #define INT7 7
    #define INT7_BIT 7
    #define INT7_MASK 128

    sfrb EIFR = 0x3c;
    #define INTF0 0
    #define INTF0_BIT 0
    #define INTF0_MASK 1
    #define INTF1 1
    #define INTF1_BIT 1
    #define INTF1_MASK 2
    #define INTF2 2
    #define INTF2_BIT 2
    #define INTF2_MASK 4
    #define INTF3 3
    #define INTF3_BIT 3
    #define INTF3_MASK 8
    #define INTF4 4
    #define INTF4_BIT 4
    #define INTF4_MASK 16
    #define INTF5 5
    #define INTF5_BIT 5
    #define INTF5_MASK 32
    #define INTF6 6
    #define INTF6_BIT 6
    #define INTF6_MASK 64
    #define INTF7 7
    #define INTF7_BIT 7
    #define INTF7_MASK 128

    sfrb PCIFR = 0x3b;
    #define PCIF0 0
    #define PCIF0_BIT 0
    #define PCIF0_MASK 1
    #define PCIF1 1
    #define PCIF1_BIT 1
    #define PCIF1_MASK 2
    #define PCIF2 2
    #define PCIF2_BIT 2
    #define PCIF2_MASK 4

    sfrb TIFR5 = 0x3a;

    sfrb TIFR4 = 0x39;

    sfrb TIFR3 = 0x38;
    #define TOV3 0
    #define TOV3_BIT 0
    #define TOV3_MASK 1
    #define OCF3A 1
    #define OCF3A_BIT 1
    #define OCF3A_MASK 2
    #define OCF3B 2
    #define OCF3B_BIT 2
    #define OCF3B_MASK 4
    #define OCF3C 3
    #define OCF3C_BIT 3
    #define OCF3C_MASK 8
    #define ICF3 5
    #define ICF3_BIT 5
    #define ICF3_MASK 32

    sfrb TIFR2 = 0x37;
    #define TOV2 0
    #define TOV2_BIT 0
    #define TOV2_MASK 1
    #define OCF2A 1
    #define OCF2A_BIT 1
    #define OCF2A_MASK 2
    #define OCF2B 2
    #define OCF2B_BIT 2
    #define OCF2B_MASK 4

    sfrb TIFR1 = 0x36;
    #define TOV1 0
    #define TOV1_BIT 0
    #define TOV1_MASK 1
    #define OCF1A 1
    #define OCF1A_BIT 1
    #define OCF1A_MASK 2
    #define OCF1B 2
    #define OCF1B_BIT 2
    #define OCF1B_MASK 4
    #define OCF1C 3
    #define OCF1C_BIT 3
    #define OCF1C_MASK 8
    #define ICF1 5
    #define ICF1_BIT 5
    #define ICF1_MASK 32

    sfrb TIFR0 = 0x35;
    #define TOV0 0
    #define TOV0_BIT 0
    #define TOV0_MASK 1
    #define OCF0A 1
    #define OCF0A_BIT 1
    #define OCF0A_MASK 2
    #define OCF0B 2
    #define OCF0B_BIT 2
    #define OCF0B_MASK 4

    sfrb PORTF = 0x31;
    #define PORTF0 0
    #define PORTF0_BIT 0
    #define PORTF0_MASK 1
    #define PORTF1 1
    #define PORTF1_BIT 1
    #define PORTF1_MASK 2
    #define PORTF2 2
    #define PORTF2_BIT 2
    #define PORTF2_MASK 4
    #define PORTF3 3
    #define PORTF3_BIT 3
    #define PORTF3_MASK 8
    #define PORTF4 4
    #define PORTF4_BIT 4
    #define PORTF4_MASK 16
    #define PORTF5 5
    #define PORTF5_BIT 5
    #define PORTF5_MASK 32
    #define PORTF6 6
    #define PORTF6_BIT 6
    #define PORTF6_MASK 64
    #define PORTF7 7
    #define PORTF7_BIT 7
    #define PORTF7_MASK 128

    sfrb DDRF = 0x30;
    #define DDF0 0
    #define DDF0_BIT 0
    #define DDF0_MASK 1
    #define DDF1 1
    #define DDF1_BIT 1
    #define DDF1_MASK 2
    #define DDF2 2
    #define DDF2_BIT 2
    #define DDF2_MASK 4
    #define DDF3 3
    #define DDF3_BIT 3
    #define DDF3_MASK 8
    #define DDF4 4
    #define DDF4_BIT 4
    #define DDF4_MASK 16
    #define DDF5 5
    #define DDF5_BIT 5
    #define DDF5_MASK 32
    #define DDF6 6
    #define DDF6_BIT 6
    #define DDF6_MASK 64
    #define DDF7 7
    #define DDF7_BIT 7
    #define DDF7_MASK 128

    sfrb PINF = 0x2f;
    #define PINF0 0
    #define PINF0_BIT 0
    #define PINF0_MASK 1
    #define PINF1 1
    #define PINF1_BIT 1
    #define PINF1_MASK 2
    #define PINF2 2
    #define PINF2_BIT 2
    #define PINF2_MASK 4
    #define PINF3 3
    #define PINF3_BIT 3
    #define PINF3_MASK 8
    #define PINF4 4
    #define PINF4_BIT 4
    #define PINF4_MASK 16
    #define PINF5 5
    #define PINF5_BIT 5
    #define PINF5_MASK 32
    #define PINF6 6
    #define PINF6_BIT 6
    #define PINF6_MASK 64
    #define PINF7 7
    #define PINF7_BIT 7
    #define PINF7_MASK 128

    sfrb PORTE = 0x2e;
    #define PORTE0 0
    #define PORTE0_BIT 0
    #define PORTE0_MASK 1
    #define PORTE1 1
    #define PORTE1_BIT 1
    #define PORTE1_MASK 2
    #define PORTE2 2
    #define PORTE2_BIT 2
    #define PORTE2_MASK 4
    #define PORTE3 3
    #define PORTE3_BIT 3
    #define PORTE3_MASK 8
    #define PORTE4 4
    #define PORTE4_BIT 4
    #define PORTE4_MASK 16
    #define PORTE5 5
    #define PORTE5_BIT 5
    #define PORTE5_MASK 32
    #define PORTE6 6
    #define PORTE6_BIT 6
    #define PORTE6_MASK 64
    #define PORTE7 7
    #define PORTE7_BIT 7
    #define PORTE7_MASK 128

    sfrb DDRE = 0x2d;
    #define DDE0 0
    #define DDE0_BIT 0
    #define DDE0_MASK 1
    #define DDE1 1
    #define DDE1_BIT 1
    #define DDE1_MASK 2
    #define DDE2 2
    #define DDE2_BIT 2
    #define DDE2_MASK 4
    #define DDE3 3
    #define DDE3_BIT 3
    #define DDE3_MASK 8
    #define DDE4 4
    #define DDE4_BIT 4
    #define DDE4_MASK 16
    #define DDE5 5
    #define DDE5_BIT 5
    #define DDE5_MASK 32
    #define DDE6 6
    #define DDE6_BIT 6
    #define DDE6_MASK 64
    #define DDE7 7
    #define DDE7_BIT 7
    #define DDE7_MASK 128

    sfrb PINE = 0x2c;
    #define PINE0 0
    #define PINE0_BIT 0
    #define PINE0_MASK 1
    #define PINE1 1
    #define PINE1_BIT 1
    #define PINE1_MASK 2
    #define PINE2 2
    #define PINE2_BIT 2
    #define PINE2_MASK 4
    #define PINE3 3
    #define PINE3_BIT 3
    #define PINE3_MASK 8
    #define PINE4 4
    #define PINE4_BIT 4
    #define PINE4_MASK 16
    #define PINE5 5
    #define PINE5_BIT 5
    #define PINE5_MASK 32
    #define PINE6 6
    #define PINE6_BIT 6
    #define PINE6_MASK 64
    #define PINE7 7
    #define PINE7_BIT 7
    #define PINE7_MASK 128

    sfrb PORTD = 0x2b;
    #define PORTD0 0
    #define PORTD0_BIT 0
    #define PORTD0_MASK 1
    #define PORTD1 1
    #define PORTD1_BIT 1
    #define PORTD1_MASK 2
    #define PORTD2 2
    #define PORTD2_BIT 2
    #define PORTD2_MASK 4
    #define PORTD3 3
    #define PORTD3_BIT 3
    #define PORTD3_MASK 8
    #define PORTD4 4
    #define PORTD4_BIT 4
    #define PORTD4_MASK 16
    #define PORTD5 5
    #define PORTD5_BIT 5
    #define PORTD5_MASK 32
    #define PORTD6 6
    #define PORTD6_BIT 6
    #define PORTD6_MASK 64
    #define PORTD7 7
    #define PORTD7_BIT 7
    #define PORTD7_MASK 128

    sfrb DDRD = 0x2a;
    #define DDD0 0
    #define DDD0_BIT 0
    #define DDD0_MASK 1
    #define DDD1 1
    #define DDD1_BIT 1
    #define DDD1_MASK 2
    #define DDD2 2
    #define DDD2_BIT 2
    #define DDD2_MASK 4
    #define DDD3 3
    #define DDD3_BIT 3
    #define DDD3_MASK 8
    #define DDD4 4
    #define DDD4_BIT 4
    #define DDD4_MASK 16
    #define DDD5 5
    #define DDD5_BIT 5
    #define DDD5_MASK 32
    #define DDD6 6
    #define DDD6_BIT 6
    #define DDD6_MASK 64
    #define DDD7 7
    #define DDD7_BIT 7
    #define DDD7_MASK 128

    sfrb PIND = 0x29;
    #define PIND0 0
    #define PIND0_BIT 0
    #define PIND0_MASK 1
    #define PIND1 1
    #define PIND1_BIT 1
    #define PIND1_MASK 2
    #define PIND2 2
    #define PIND2_BIT 2
    #define PIND2_MASK 4
    #define PIND3 3
    #define PIND3_BIT 3
    #define PIND3_MASK 8
    #define PIND4 4
    #define PIND4_BIT 4
    #define PIND4_MASK 16
    #define PIND5 5
    #define PIND5_BIT 5
    #define PIND5_MASK 32
    #define PIND6 6
    #define PIND6_BIT 6
    #define PIND6_MASK 64
    #define PIND7 7
    #define PIND7_BIT 7
    #define PIND7_MASK 128

    sfrb PORTC = 0x28;
    #define PORTC0 0
    #define PORTC0_BIT 0
    #define PORTC0_MASK 1
    #define PORTC1 1
    #define PORTC1_BIT 1
    #define PORTC1_MASK 2
    #define PORTC2 2
    #define PORTC2_BIT 2
    #define PORTC2_MASK 4
    #define PORTC3 3
    #define PORTC3_BIT 3
    #define PORTC3_MASK 8
    #define PORTC4 4
    #define PORTC4_BIT 4
    #define PORTC4_MASK 16
    #define PORTC5 5
    #define PORTC5_BIT 5
    #define PORTC5_MASK 32
    #define PORTC6 6
    #define PORTC6_BIT 6
    #define PORTC6_MASK 64
    #define PORTC7 7
    #define PORTC7_BIT 7
    #define PORTC7_MASK 128

    sfrb DDRC = 0x27;
    #define DDC0 0
    #define DDC0_BIT 0
    #define DDC0_MASK 1
    #define DDC1 1
    #define DDC1_BIT 1
    #define DDC1_MASK 2
    #define DDC2 2
    #define DDC2_BIT 2
    #define DDC2_MASK 4
    #define DDC3 3
    #define DDC3_BIT 3
    #define DDC3_MASK 8
    #define DDC4 4
    #define DDC4_BIT 4
    #define DDC4_MASK 16
    #define DDC5 5
    #define DDC5_BIT 5
    #define DDC5_MASK 32
    #define DDC6 6
    #define DDC6_BIT 6
    #define DDC6_MASK 64
    #define DDC7 7
    #define DDC7_BIT 7
    #define DDC7_MASK 128

    sfrb PINC = 0x26;
    #define PINC0 0
    #define PINC0_BIT 0
    #define PINC0_MASK 1
    #define PINC1 1
    #define PINC1_BIT 1
    #define PINC1_MASK 2
    #define PINC2 2
    #define PINC2_BIT 2
    #define PINC2_MASK 4
    #define PINC3 3
    #define PINC3_BIT 3
    #define PINC3_MASK 8
    #define PINC4 4
    #define PINC4_BIT 4
    #define PINC4_MASK 16
    #define PINC5 5
    #define PINC5_BIT 5
    #define PINC5_MASK 32
    #define PINC6 6
    #define PINC6_BIT 6
    #define PINC6_MASK 64
    #define PINC7 7
    #define PINC7_BIT 7
    #define PINC7_MASK 128

    sfrb PORTB = 0x25;
    #define PORTB0 0
    #define PORTB0_BIT 0
    #define PORTB0_MASK 1
    #define PORTB1 1
    #define PORTB1_BIT 1
    #define PORTB1_MASK 2
    #define PORTB2 2
    #define PORTB2_BIT 2
    #define PORTB2_MASK 4
    #define PORTB3 3
    #define PORTB3_BIT 3
    #define PORTB3_MASK 8
    #define PORTB4 4
    #define PORTB4_BIT 4
    #define PORTB4_MASK 16
    #define PORTB5 5
    #define PORTB5_BIT 5
    #define PORTB5_MASK 32
    #define PORTB6 6
    #define PORTB6_BIT 6
    #define PORTB6_MASK 64
    #define PORTB7 7
    #define PORTB7_BIT 7
    #define PORTB7_MASK 128

    sfrb DDRB = 0x24;
    #define DDB0 0
    #define DDB0_BIT 0
    #define DDB0_MASK 1
    #define DDB1 1
    #define DDB1_BIT 1
    #define DDB1_MASK 2
    #define DDB2 2
    #define DDB2_BIT 2
    #define DDB2_MASK 4
    #define DDB3 3
    #define DDB3_BIT 3
    #define DDB3_MASK 8
    #define DDB4 4
    #define DDB4_BIT 4
    #define DDB4_MASK 16
    #define DDB5 5
    #define DDB5_BIT 5
    #define DDB5_MASK 32
    #define DDB6 6
    #define DDB6_BIT 6
    #define DDB6_MASK 64
    #define DDB7 7
    #define DDB7_BIT 7
    #define DDB7_MASK 128

    sfrb PINB = 0x23;
    #define PINB0 0
    #define PINB0_BIT 0
    #define PINB0_MASK 1
    #define PINB1 1
    #define PINB1_BIT 1
    #define PINB1_MASK 2
    #define PINB2 2
    #define PINB2_BIT 2
    #define PINB2_MASK 4
    #define PINB3 3
    #define PINB3_BIT 3
    #define PINB3_MASK 8
    #define PINB4 4
    #define PINB4_BIT 4
    #define PINB4_MASK 16
    #define PINB5 5
    #define PINB5_BIT 5
    #define PINB5_MASK 32
    #define PINB6 6
    #define PINB6_BIT 6
    #define PINB6_MASK 64
    #define PINB7 7
    #define PINB7_BIT 7
    #define PINB7_MASK 128

    sfrb PORTA = 0x22;
    #define PORTA0 0
    #define PORTA0_BIT 0
    #define PORTA0_MASK 1
    #define PORTA1 1
    #define PORTA1_BIT 1
    #define PORTA1_MASK 2
    #define PORTA2 2
    #define PORTA2_BIT 2
    #define PORTA2_MASK 4
    #define PORTA3 3
    #define PORTA3_BIT 3
    #define PORTA3_MASK 8
    #define PORTA4 4
    #define PORTA4_BIT 4
    #define PORTA4_MASK 16
    #define PORTA5 5
    #define PORTA5_BIT 5
    #define PORTA5_MASK 32
    #define PORTA6 6
    #define PORTA6_BIT 6
    #define PORTA6_MASK 64
    #define PORTA7 7
    #define PORTA7_BIT 7
    #define PORTA7_MASK 128

    sfrb DDRA = 0x21;
    #define DDA0 0
    #define DDA0_BIT 0
    #define DDA0_MASK 1
    #define DDA1 1
    #define DDA1_BIT 1
    #define DDA1_MASK 2
    #define DDA2 2
    #define DDA2_BIT 2
    #define DDA2_MASK 4
    #define DDA3 3
    #define DDA3_BIT 3
    #define DDA3_MASK 8
    #define DDA4 4
    #define DDA4_BIT 4
    #define DDA4_MASK 16
    #define DDA5 5
    #define DDA5_BIT 5
    #define DDA5_MASK 32
    #define DDA6 6
    #define DDA6_BIT 6
    #define DDA6_MASK 64
    #define DDA7 7
    #define DDA7_BIT 7
    #define DDA7_MASK 128

    sfrb PINA = 0x20;
    #define PINA0 0
    #define PINA0_BIT 0
    #define PINA0_MASK 1
    #define PINA1 1
    #define PINA1_BIT 1
    #define PINA1_MASK 2
    #define PINA2 2
    #define PINA2_BIT 2
    #define PINA2_MASK 4
    #define PINA3 3
    #define PINA3_BIT 3
    #define PINA3_MASK 8
    #define PINA4 4
    #define PINA4_BIT 4
    #define PINA4_MASK 16
    #define PINA5 5
    #define PINA5_BIT 5
    #define PINA5_MASK 32
    #define PINA6 6
    #define PINA6_BIT 6
    #define PINA6_MASK 64
    #define PINA7 7
    #define PINA7_BIT 7
    #define PINA7_MASK 128

    #endif