##### Synopsis

    #include <inmaxq.h>
    unsigned __restore_interrupt(unsigned state);

##### Description

__restore_interrupt restores the state of the IGE bit in the interrupt control register IC to the value saved in state.

The value of state is returned from the __disable_interrupt, __enable_interrupt, and __save_interrupt intrinsic functions and is simply the previous value of the interrupt control register.

__restore_interrupt is an intrinsic function and produces inline code.

##### Portability

__restore_interrupt can be used on any MAXQ device.

##### See Also

__disable_interrupt, __enable_interrupt, __save_interrupt