##### Synopsis

    #include <inmaxq.h>
    unsigned __save_interrupt(void);

##### Description

__save_interrupt returns the current value of the interrupt control register IC, including the IGE bit, without changing the status register. You can restore the state of the interrupt flag using the __restore_interrupt intrinsic function.

__save_interrupt is an intrinsic function and produces inline code.

##### Portability

__save_interrupt can be used on any MAXQ device.

##### See Also

__restore_interrupt