The MAXQ Serial To JTAG Interface target interface provides access to Dallas Semiconductor’s MAXQJTAG interface board. This target interface supports program loading and debugging. When debugging with this target interface you will have access to four program breakpoints and two data breakpoints. Note that one of the program breakpoints will be needed for single stepping and one of the data breakpoints will be needed for the debug io library.

###### Connection property group

Port Name
  The name of the serial port.