<solution version="1" Name="msp430p140" >
  <configuration Target="MSP430F149" linker_memory_map_file="$(StudioDir)/targets/MSP430F149.xml" link_include_standard_libraries="Yes" link_include_startup_code="Yes" Name="Common" build_use_hardware_multiplier="Yes" />
  <project Name="Software Toggle P1.0 " >
    <folder Name="Source Files" >
      <file file_name="fet140_1.c" Name="fet140_1.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_1.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="ADC12 Sample A0, AVcc " >
    <folder Name="Source Files" >
      <file file_name="fet140_adc12_00.c" Name="fet140_adc12_00.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_adc12_00.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="ADC12 Using 10 External Channels for Conversion " >
    <folder Name="Source Files" >
      <file file_name="fet140_adc12_01.c" Name="fet140_adc12_01.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_adc12_01.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="ADC12 Using an External Reference " >
    <folder Name="Source Files" >
      <file file_name="fet140_adc12_02.c" Name="fet140_adc12_02.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_adc12_02.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="ADC12 Extended sampling " >
    <folder Name="Source Files" >
      <file file_name="fet140_adc12_03.c" Name="fet140_adc12_03.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_adc12_03.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="ADC12 Using the Internal Reference " >
    <folder Name="Source Files" >
      <file file_name="fet140_adc12_04.c" Name="fet140_adc12_04.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_adc12_04.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="ADC12 Repeated Sequence of Conversions " >
    <folder Name="Source Files" >
      <file file_name="fet140_adc12_05.c" Name="fet140_adc12_05.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_adc12_05.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="ADC12 Repeated Single Channel Conversions " >
    <folder Name="Source Files" >
      <file file_name="fet140_adc12_06.c" Name="fet140_adc12_06.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_adc12_06.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="ADC12 Single Conversion on Single Channel " >
    <folder Name="Source Files" >
      <file file_name="fet140_adc12_07.c" Name="fet140_adc12_07.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_adc12_07.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="ADC12 Sequence of Conversions (non-repeated) " >
    <folder Name="Source Files" >
      <file file_name="fet140_adc12_08.c" Name="fet140_adc12_08.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_adc12_08.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="ADC12 Using the temperature diode " >
    <folder Name="Source Files" >
      <file file_name="fet140_adc12_09.c" Name="fet140_adc12_09.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_adc12_09.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="ADC12, Trigger Conversion With Timer_A " >
    <folder Name="Source Files" >
      <file file_name="fet140_adc12_10.c" Name="fet140_adc12_10.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_adc12_10.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="BasicClock MCLK configured with HF XTAL XT2 " >
    <folder Name="Source Files" >
      <file file_name="fet140_hfxt2.c" Name="fet140_hfxt2.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_hfxt2.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="BasicClock MCLK configured with HF XTAL " >
    <folder Name="Source Files" >
      <file file_name="fet140_hfxtal.c" Name="fet140_hfxtal.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_hfxtal.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="BasicClock LPM3 Using WDT ISR, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_lpm3.c" Name="fet140_lpm3.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_lpm3.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="USART0 SPI Interface with HC165/164 Shift Registers " >
    <folder Name="Source Files" >
      <file file_name="fet140_spi0_016x.c" Name="fet140_spi0_016x.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_spi0_016x.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0, CCR0 Contmode ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_ta01.c" Name="fet140_ta01.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_ta01.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0, CCR0 upmode ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_ta02.c" Name="fet140_ta02.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_ta02.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0, overflow ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_ta03.c" Name="fet140_ta03.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_ta03.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0, overflow ISR, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_ta04.c" Name="fet140_ta04.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_ta04.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0, CCR0 upmode ISR, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_ta05.c" Name="fet140_ta05.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_ta05.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0, CCR1 Contmode ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_ta06.c" Name="fet140_ta06.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_ta06.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0-3 CCRx Contmode ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_ta07.c" Name="fet140_ta07.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_ta07.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0-3 CCRx Contmode ISR, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_ta08.c" Name="fet140_ta08.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_ta08.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0-3 CCRx Contmode ISR, HF XTAL ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_ta09.c" Name="fet140_ta09.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_ta09.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.1 With TA0 upmode, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_ta10.c" Name="fet140_ta10.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_ta10.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.1 With TA0 upmode, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_ta11.c" Name="fet140_ta11.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_ta11.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.1 With TA0 upmode, HF XTAL ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_ta12.c" Name="fet140_ta12.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_ta12.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.1 With TA0 up-downmode, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_ta13.c" Name="fet140_ta13.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_ta13.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.1 With TA0 up-downmode, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_ta14.c" Name="fet140_ta14.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_ta14.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.1 With TA0 up-downmode, HF XTAL ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_ta15.c" Name="fet140_ta15.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_ta15.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A PWM TA1-2 upmode, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_ta_pwm01.c" Name="fet140_ta_pwm01.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_ta_pwm01.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A PWM TA1-2 upmode, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_ta_pwm02.c" Name="fet140_ta_pwm02.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_ta_pwm02.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A PWM TA1-2 upmode, HFTAL ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_ta_pwm03.c" Name="fet140_ta_pwm03.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_ta_pwm03.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A PWM TA1-2 up-downmode, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_ta_pwm04.c" Name="fet140_ta_pwm04.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_ta_pwm04.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A PWM TA1-2 up-downmode, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_ta_pwm05.c" Name="fet140_ta_pwm05.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_ta_pwm05.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A PWM TA1-2 up-downmode, HFTAL ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_ta_pwm06.c" Name="fet140_ta_pwm06.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_ta_pwm06.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_B Toggle P1.0, TBCCR0 Contmode ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_tb01.c" Name="fet140_tb01.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_tb01.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_B Toggle P1.0, CCR0 upmode ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_tb02.c" Name="fet140_tb02.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_tb02.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_B Toggle P1.0, overflow ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_tb03.c" Name="fet140_tb03.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_tb03.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_B Toggle P1.0, overflow ISR, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_tb04.c" Name="fet140_tb04.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_tb04.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_B Toggle P1.0, CCR0 upmode ISR, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_tb05.c" Name="fet140_tb05.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_tb05.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="USART0 UART 2400 Ultra-low Power Echo ISR, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_uart01_02400.c" Name="fet140_uart01_02400.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_uart01_02400.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="USART0 UART 9600 Echo ISR, HF XTAL ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_uart01_09600.c" Name="fet140_uart01_09600.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_uart01_09600.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="USART0 UART 19200 Echo ISR, HF XTAL ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_uart01_19200.c" Name="fet140_uart01_19200.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_uart01_19200.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="USART0 UART 115200 Echo ISR, HF XTAL ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_uart01_0115k.c" Name="fet140_uart01_0115k.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_uart01_0115k.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="USART1 UART 2400 Ultra-low Power Echo ISR, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_uart11_02400.c" Name="fet140_uart11_02400.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_uart11_02400.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="USART1 UART 19200 Echo ISR, XT2 HF XTAL SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_uart11_19200_2.c" Name="fet140_uart11_19200_2.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_uart11_19200_2.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="USART1 UART 115200 Echo ISR, XT2 HF XTAL SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_uart11_0115k_2.c" Name="fet140_uart11_0115k_2.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_uart11_0115k_2.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="WDT Toggle P1.0 Interval overflow ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet140_wdt01.c" Name="fet140_wdt01.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_wdt01.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="WDT Toggle P1.0 Interval overflow ISR, 32kHz ACLK   " >
    <folder Name="Source Files" >
      <file file_name="fet140_wdt02.c" Name="fet140_wdt02.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet140_wdt02.hzx" project_type="Executable" Name="Common" />
  </project>
  <configuration Name="Debug" />
  <configuration build_debug_information="No" Name="Release" build_optimize_output="Yes" />
</solution>
