<solution version="1" Name="msp430p120" >
  <configuration Target="MSP430F1232" linker_memory_map_file="$(StudioDir)/targets/MSP430F1232.xml" link_include_standard_libraries="Yes" link_include_startup_code="Yes" Name="Common" build_use_hardware_multiplier="No" />
  <project Name="Software Toggle P1.0 " >
    <folder Name="Source Files" >
      <file file_name="fet120_1.c" Name="fet120_1.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_1.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="ADC10 Sample A0, AVcc, Set P1.0 if > 0.5*AVcc " >
    <folder Name="Source Files" >
      <file file_name="fet120_ADC10_01.c" Name="fet120_ADC10_01.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_ADC10_01.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="ADC10 Sample A0, 1.5V, Set P1.0 if > 0.2V " >
    <folder Name="Source Files" >
      <file file_name="fet120_ADC10_02.c" Name="fet120_ADC10_02.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_ADC10_02.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="ADC10 Sample A10 Temp Set P1.0 if temp > ~ 29c " >
    <folder Name="Source Files" >
      <file file_name="fet120_ADC10_03.c" Name="fet120_ADC10_03.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_ADC10_03.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="ADC10 Sample A0 Signed AVcc Set P1.0 if > 0.5*AVcc " >
    <folder Name="Source Files" >
      <file file_name="fet120_ADC10_04.c" Name="fet120_ADC10_04.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_ADC10_04.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="ADC10 Sample A11 lo_Batt Set P1.0 if &lt; 2.3V " >
    <folder Name="Source Files" >
      <file file_name="fet120_ADC10_05.c" Name="fet120_ADC10_05.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_ADC10_05.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="ADC10 Output Internal Vref on P2.4 and Osc. on P1.0 " >
    <folder Name="Source Files" >
      <file file_name="fet120_ADC10_06.c" Name="fet120_ADC10_06.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_ADC10_06.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="ADC10 Sample A0 64x, AVcc, Repeat Single DTC DCO " >
    <folder Name="Source Files" >
      <file file_name="fet120_ADC10_07.c" Name="fet120_ADC10_07.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_ADC10_07.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="ADC10 Sample A0 64x, 1.5V, Repeat Single DTC DCO " >
    <folder Name="Source Files" >
      <file file_name="fet120_ADC10_08.c" Name="fet120_ADC10_08.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_ADC10_08.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="ADC10 Sample A10 64x, 1.5v, Repeat Single DTC DCO " >
    <folder Name="Source Files" >
      <file file_name="fet120_ADC10_09.c" Name="fet120_ADC10_09.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_ADC10_09.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="ADC10 Sample A2-0, AVcc, SIngle Sequence DTC DCO " >
    <folder Name="Source Files" >
      <file file_name="fet120_ADC10_10.c" Name="fet120_ADC10_10.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_ADC10_10.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="ADC10 Sample A10Temp and Convert to oC and oF " >
    <folder Name="Source Files" >
      <file file_name="fet120_ADC10_temp.c" Name="fet120_ADC10_temp.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_ADC10_temp.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="BasicClock Output buffered SMCLK, ACLK and MCLK/12 " >
    <folder Name="Source Files" >
      <file file_name="fet120_clks.c" Name="fet120_clks.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_clks.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Flash In-System Programming " >
    <folder Name="Source Files" >
      <file file_name="fet120_flash_write.c" Name="fet120_flash_write.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_flash_write.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="BasicClock MCLK configured with HF XTAL " >
    <folder Name="Source Files" >
      <file file_name="fet120_hfxtal.c" Name="fet120_hfxtal.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_hfxtal.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="BasicClock LPM3 Using WDT ISR, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet120_lpm3.c" Name="fet120_lpm3.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_lpm3.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="USART0 SPI Interface with HC165/164 Shift Registers " >
    <folder Name="Source Files" >
      <file file_name="fet120_spi0_016x.c" Name="fet120_spi0_016x.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_spi0_016x.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0, CCR0 Contmode ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet120_ta01.c" Name="fet120_ta01.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_ta01.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0, CCR0 upmode ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet120_ta02.c" Name="fet120_ta02.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_ta02.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0, overflow ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet120_ta03.c" Name="fet120_ta03.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_ta03.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0, overflow ISR, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet120_ta04.c" Name="fet120_ta04.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_ta04.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0, CCR0 upmode ISR, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet120_ta05.c" Name="fet120_ta05.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_ta05.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0, CCR1 Contmode ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet120_ta06.c" Name="fet120_ta06.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_ta06.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0-3 CCRx Contmode ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet120_ta07.c" Name="fet120_ta07.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_ta07.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0-3 CCRx Contmode ISR, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet120_ta08.c" Name="fet120_ta08.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_ta08.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0-3 CCRx Contmode ISR, HF XTAL ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet120_ta09.c" Name="fet120_ta09.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_ta09.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.1 With TA0 upmode, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet120_ta10.c" Name="fet120_ta10.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_ta10.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.1 With TA0 upmode, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet120_ta11.c" Name="fet120_ta11.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_ta11.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.1 With TA0 upmode, HF XTAL ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet120_ta12.c" Name="fet120_ta12.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_ta12.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.1 With TA0 up-downmode, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet120_ta13.c" Name="fet120_ta13.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_ta13.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.1 With TA0 up-downmode, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet120_ta14.c" Name="fet120_ta14.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_ta14.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.1 With TA0 up-downmode, HF XTAL ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet120_ta15.c" Name="fet120_ta15.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_ta15.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A PWM TA1-2 upmode, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet120_ta_pwm01.c" Name="fet120_ta_pwm01.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_ta_pwm01.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A PWM TA1-2 upmode, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet120_ta_pwm02.c" Name="fet120_ta_pwm02.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_ta_pwm02.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A PWM TA1-2 upmode, HFTAL ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet120_ta_pwm03.c" Name="fet120_ta_pwm03.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_ta_pwm03.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A PWM TA1-2 up-downmode, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet120_ta_pwm04.c" Name="fet120_ta_pwm04.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_ta_pwm04.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A PWM TA1-2 up-downmode, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet120_ta_pwm05.c" Name="fet120_ta_pwm05.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_ta_pwm05.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A PWM TA1-2 up-downmode, HFTAL ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet120_ta_pwm06.c" Name="fet120_ta_pwm06.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_ta_pwm06.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="USART0 UART 2400 Ultra-low Power Echo ISR, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet120_uart01_02400.c" Name="fet120_uart01_02400.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_uart01_02400.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="USART0 UART 9600 Echo ISR, HF XTAL ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet120_uart01_09600.c" Name="fet120_uart01_09600.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_uart01_09600.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="USART0 UART 19200 Echo ISR, HF XTAL ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet120_uart01_19200.c" Name="fet120_uart01_19200.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_uart01_19200.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="USART0 UART 115200 Echo ISR, HF XTAL ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet120_uart01_0115k.c" Name="fet120_uart01_0115k.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_uart01_0115k.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="WDT Toggle P1.0 Interval overflow ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet120_wdt01.c" Name="fet120_wdt01.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_wdt01.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="WDT Toggle P1.0 Interval overflow ISR, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet120_wdt02.c" Name="fet120_wdt02.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_wdt02.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="WDT Toggle P1.0 Interval overflow ISR, HF XTAL ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet120_wdt03.c" Name="fet120_wdt03.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet120_wdt03.hzx" project_type="Executable" Name="Common" />
  </project>
  <configuration Name="Debug" />
  <configuration build_debug_information="No" Name="Release" build_optimize_output="Yes" />
</solution>
