<solution Name="msp430p410" version="1" >
  <configuration Target="MSP430F413" linker_memory_map_file="$(StudioDir)/targets/MSP430F413.xml" link_include_standard_libraries="No" link_include_startup_code="No" Name="Common" build_use_hardware_multiplier="No" />
  <project Name="Software Toggle P5.1 " >
    <folder Name="Source Files" >
      <file file_name="fet410_1.s43" Name="fet410_1.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet410_1.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="FLL+ Output MCLK, ACLK Using 32k XTAL and DCO " >
    <folder Name="Source Files" >
      <file file_name="fet410_clks.s43" Name="fet410_clks.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet410_clks.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="FLL+ clock Runs internal DCO at 2.45Mhz " >
    <folder Name="Source Files" >
      <file file_name="fet410_fll01.s43" Name="fet410_fll01.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet410_fll01.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="FLL+ clock runs internal DCO at 8 Mhz " >
    <folder Name="Source Files" >
      <file file_name="fet410_fll02.s43" Name="fet410_fll02.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet410_fll02.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="FLL+ LPM3 Using BasicTimer ISR, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet410_lpm3.s43" Name="fet410_lpm3.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet410_lpm3.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="LCD Put &quot;6543210&quot; on STK/EVK LCD " >
    <folder Name="Source Files" >
      <file file_name="fet410_lcd01.s43" Name="fet410_lcd01.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet410_lcd01.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="LCD Displays numbers on statc LCD " >
    <folder Name="Source Files" >
      <file file_name="fet410_lcd02.s43" Name="fet410_lcd02.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet410_lcd02.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="LCD displays numbers on 4 multiplex rate LCD " >
    <folder Name="Source Files" >
      <file file_name="fet410_lcd03.s43" Name="fet410_lcd03.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet410_lcd03.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="LCD Displays numbers on 3 multiplex rate LCD " >
    <folder Name="Source Files" >
      <file file_name="fet410_lcd04.s43" Name="fet410_lcd04.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet410_lcd04.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="LCD Displays a real time clock on a static LCD " >
    <folder Name="Source Files" >
      <file file_name="fet410_lcd05.s43" Name="fet410_lcd05.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet410_lcd05.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="LCD Displays numbers on 14 segment 4 multiplex rate " >
    <folder Name="Source Files" >
      <file file_name="fet410_lcd06.s43" Name="fet410_lcd06.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet410_lcd06.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="BasicTimer Toggle P5.1 using ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet410_bt01.s43" Name="fet410_bt01.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet410_bt01.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="BasicTimer Toggle P5.1 using ISR, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet410_bt02.s43" Name="fet410_bt02.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet410_bt02.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Flash In-System Program memory " >
    <folder Name="Source Files" >
      <file file_name="fet410_isp.s43" Name="fet410_isp.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet410_isp.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P5.1, CCR0 Contmode ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet410_ta01.s43" Name="fet410_ta01.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet410_ta01.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P5.1, CCR0 upmode ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet410_ta02.s43" Name="fet410_ta02.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet410_ta02.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P5.1, overflow ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet410_ta03.s43" Name="fet410_ta03.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet410_ta03.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P5.1, overflow ISR, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet410_ta04.s43" Name="fet410_ta04.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet410_ta04.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P5.1, CCR0 upmode ISR, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet410_ta05.s43" Name="fet410_ta05.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet410_ta05.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Output 40khz square wave, UpMode SMCLK DCO " >
    <folder Name="Source Files" >
      <file file_name="fet410_ta_40k.s43" Name="fet410_ta_40k.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet410_ta_40k.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A PWM TA1-2 upmode, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet410_ta_pwm01.s43" Name="fet410_ta_pwm01.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet410_ta_pwm01.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A PWM TA1-2 upmode, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet410_ta_pwm02.s43" Name="fet410_ta_pwm02.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet410_ta_pwm02.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A used to generate DTMF using UpMode, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet410_ta_dtmf.s43" Name="fet410_ta_dtmf.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet410_ta_dtmf.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A UART 2400 Ultra-low Power Echo, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet410_ta_uart2400.s43" Name="fet410_ta_uart2400.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet410_ta_uart2400.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A UART 9600 Echo, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet410_ta_uart9600.s43" Name="fet410_ta_uart9600.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet410_ta_uart9600.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A UART 115200 Echo, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet410_ta_uart115k.s43" Name="fet410_ta_uart115k.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet410_ta_uart115k.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="WDT Toggle P5.1 Interval overflow ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet410_wdt01.s43" Name="fet410_wdt01.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet410_wdt01.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="WDT Toggle P5.1 Interval overflow ISR, 32kHz ACLK       " >
    <folder Name="Source Files" >
      <file file_name="fet410_wdt02.s43" Name="fet410_wdt02.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet410_wdt02.hzx" project_type="Executable" Name="Common" />
  </project>
  <configuration Name="Debug" />
  <configuration build_debug_information="No" Name="Release" build_optimize_output="Yes" />
</solution>
