<solution version="1" Name="msp430p440" >
  <configuration Target="MSP430F449" linker_memory_map_file="$(StudioDir)/targets/MSP430F449.xml" link_include_standard_libraries="No" link_include_startup_code="No" Name="Common" build_use_hardware_multiplier="Yes" />
  <project Name="Software Toggle P5.1 " >
    <folder Name="Source Files" >
      <file file_name="fet440_1.s43" Name="fet440_1.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_1.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="ADC12 Sample A0, AVcc " >
    <folder Name="Source Files" >
      <file file_name="fet440_adc12_00.s43" Name="fet440_adc12_00.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_adc12_00.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="ADC12 Using 10 External Channels for Conversion " >
    <folder Name="Source Files" >
      <file file_name="fet440_adc12_01.s43" Name="fet440_adc12_01.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_adc12_01.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="ADC12 Using an External Reference " >
    <folder Name="Source Files" >
      <file file_name="fet440_adc12_02.s43" Name="fet440_adc12_02.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_adc12_02.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="ADC12 Extended sampling " >
    <folder Name="Source Files" >
      <file file_name="fet440_adc12_03.s43" Name="fet440_adc12_03.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_adc12_03.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="ADC12 Using the Internal Reference " >
    <folder Name="Source Files" >
      <file file_name="fet440_adc12_04.s43" Name="fet440_adc12_04.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_adc12_04.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="ADC12 Repeated Sequence of Conversions " >
    <folder Name="Source Files" >
      <file file_name="fet440_adc12_05.s43" Name="fet440_adc12_05.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_adc12_05.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="ADC12 Repeated Single Channel Conversions " >
    <folder Name="Source Files" >
      <file file_name="fet440_adc12_06.s43" Name="fet440_adc12_06.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_adc12_06.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="ADC12 Single Conversion on Single Channel " >
    <folder Name="Source Files" >
      <file file_name="fet440_adc12_07.s43" Name="fet440_adc12_07.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_adc12_07.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="ADC12 Sequence of Conversions (non-repeated) " >
    <folder Name="Source Files" >
      <file file_name="fet440_adc12_08.s43" Name="fet440_adc12_08.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_adc12_08.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="ADC12 Using the temperature diode " >
    <folder Name="Source Files" >
      <file file_name="fet440_adc12_09.s43" Name="fet440_adc12_09.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_adc12_09.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="ADC12, Trigger Conversion With Timer_A " >
    <folder Name="Source Files" >
      <file file_name="fet440_adc12_10.s43" Name="fet440_adc12_10.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_adc12_10.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="BasicTimer Toggle P5.1 using ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet440_bt01.c" Name="fet440_bt01.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_bt01.hzx" project_type="Executable" build_exclude_from_build="Yes" Name="Common" />
  </project>
  <project Name="BasicTimer Toggle P5.1 using ISR, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet440_bt02.c" Name="fet440_bt02.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_bt02.hzx" project_type="Executable" build_exclude_from_build="Yes" Name="Common" />
  </project>
  <project Name="FLL+ Output MCLK, SMCLK, ACLK Using 32k XTAL " >
    <folder Name="Source Files" >
      <file file_name="fet440_clks1.s43" Name="fet440_clks1.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_clks1.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="FLL+ Output 32k xtal + HF xtal + internal DCO " >
    <folder Name="Source Files" >
      <file file_name="fet440_clks2.s43" Name="fet440_clks2.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_clks2.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="FLL+ clock Runs internal DCO at 2.45Mhz " >
    <folder Name="Source Files" >
      <file file_name="fet440_fll01.s43" Name="fet440_fll01.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_fll01.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="FLL+ clock runs internal DCO at 8 Mhz " >
    <folder Name="Source Files" >
      <file file_name="fet440_fll02.s43" Name="fet440_fll02.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_fll02.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="FLL+ MCLK configured to operate from XT2 HF XTAL " >
    <folder Name="Source Files" >
      <file file_name="fet440_hfxt2.s43" Name="fet440_hfxt2.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_hfxt2.hzx" project_type="Executable" build_exclude_from_build="Yes" Name="Common" />
  </project>
  <project Name="Flash In-System Program memory " >
    <folder Name="Source Files" >
      <file file_name="fet440_isp.s43" Name="fet440_isp.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_isp.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="LCD Put &quot;6543210&quot; on STK/EVK LCD " >
    <folder Name="Source Files" >
      <file file_name="fet440_lcd01.s43" Name="fet440_lcd01.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_lcd01.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="LCD displays numbers on static LCD " >
    <folder Name="Source Files" >
      <file file_name="fet440_lcd02.s43" Name="fet440_lcd02.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_lcd02.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="LCD displays numbers on 4 multiplex rate LCD " >
    <folder Name="Source Files" >
      <file file_name="fet440_lcd03.s43" Name="fet440_lcd03.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_lcd03.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="LCD Displays numbers on 3 multiplex rate LCD " >
    <folder Name="Source Files" >
      <file file_name="fet440_lcd04.s43" Name="fet440_lcd04.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_lcd04.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="FLL+ LPM3 Using BasicTimer ISR, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet440_lpm3.s43" Name="fet440_lpm3.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_lpm3.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P5.1, CCR0 Contmode ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet440_ta01.s43" Name="fet440_ta01.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_ta01.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P5.1, CCR0 upmode ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet440_ta02.s43" Name="fet440_ta02.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_ta02.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P5.1, overflow ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet440_ta03.s43" Name="fet440_ta03.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_ta03.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P5.1, overflow ISR, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet440_ta04.s43" Name="fet440_ta04.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_ta04.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P5.1, CCR0 upmode ISR, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet440_ta05.s43" Name="fet440_ta05.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_ta05.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A PWM TA1-2 upmode, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet440_ta_pwm01.s43" Name="fet440_ta_pwm01.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_ta_pwm01.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A PWM TA1-2 upmode, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet440_ta_pwm02.s43" Name="fet440_ta_pwm02.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_ta_pwm02.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_B Toggle P5.1, TBCCR0 Contmode ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet440_tb01.s43" Name="fet440_tb01.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_tb01.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_B Toggle P5.1, TBCCR0 upmode ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet440_tb02.s43" Name="fet440_tb02.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_tb02.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_B Toggle P5.1, overflow ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet440_tb03.s43" Name="fet440_tb03.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_tb03.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_B Toggle P5.1, overflow ISR, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet440_tb04.s43" Name="fet440_tb04.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_tb04.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_B Toggle P5.1, TBCCR0 upmode ISR, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet440_tb05.s43" Name="fet440_tb05.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_tb05.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="USART0 SPI Interface to HC165/164 Shift Registers " >
    <folder Name="Source Files" >
      <file file_name="fet440_spi0_016x.s43" Name="fet440_spi0_016x.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_spi0_016x.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="USART0 UART 2400 Ultra-low Power Echo ISR, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet440_uart01_02400.s43" Name="fet440_uart01_02400.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_uart01_02400.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="USART0 UART 9600 Echo ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet440_uart01_09600.s43" Name="fet440_uart01_09600.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_uart01_09600.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="USART0 UART 19200 Echo ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet440_uart01_19200.s43" Name="fet440_uart01_19200.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_uart01_19200.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="USART0 UART 115200 Echo ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet440_uart01_0115k.s43" Name="fet440_uart01_0115k.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_uart01_0115k.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="USART1 UART 19200 Echo ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet440_uart11_19200.s43" Name="fet440_uart11_19200.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_uart11_19200.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="USART1 UART 38400 Echo ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet440_uart11_38400.s43" Name="fet440_uart11_38400.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_uart11_38400.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="WDT Toggle P5.1 Interval overflow ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet440_wdt01.s43" Name="fet440_wdt01.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_wdt01.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="WDT Toggle P5.1 Interval overflow ISR, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet440_wdt02.s43" Name="fet440_wdt02.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet440_wdt02.hzx" project_type="Executable" Name="Common" />
  </project>
  <configuration Name="Debug" />
  <configuration build_debug_information="No" Name="Release" build_optimize_output="Yes" />
</solution>
