<solution Name="msp430x110" version="1" >
  <configuration Target="MSP430F1121A" linker_memory_map_file="$(StudioDir)/targets/MSP430F1121A.xml" link_include_standard_libraries="Yes" link_include_startup_code="Yes" Name="Common" build_use_hardware_multiplier="No" />
  <project Name="Software Toggle P1.0 " >
    <folder Name="Source Files" >
      <file file_name="fet_1.c" Name="fet_1.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration Target="MSP430F1121A" linker_memory_map_file="$(StudioDir)/targets/MSP430F1121A.xml" build_output_file_name="$(OutDir)/fet_1.hzx" project_type="Executable" Name="Common" build_use_hardware_multiplier="No" />
    <configuration build_debug_information="No" Name="Release" build_optimize_output="Yes" />
  </project>
  <project Name="Software SPI Interface TLC549 Set P1.0 if > 0.5*Vcc " >
    <folder Name="Source Files" >
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
      <file file_name="fet110_549.c" Name="fet110_549.c" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_549" project_type="Executable" Name="Common" />
  </project>
  <project Name="Comp_A Output Comparator_A reference voltages on P2.3 " >
    <folder Name="Source Files" >
      <file file_name="fet110_ca01.c" Name="fet110_ca01.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ca01.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Comp_A Detect theashold, Set P1.0 if P2.3 > 0.25*Vcc " >
    <folder Name="Source Files" >
      <file file_name="fet110_ca02.c" Name="fet110_ca02.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ca02.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="BasicClock Output buffered SMCLK, ACLK and MCLK/12 " >
    <folder Name="Source Files" >
      <file file_name="fet110_clks.c" Name="fet110_clks.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_clks.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Flash In-System Programming " >
    <folder Name="Source Files" >
      <file file_name="fet110_flash_write.c" Name="fet110_flash_write.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_flash_write.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="BasicClock Implement Auto RSEL SW FLL " >
    <folder Name="Source Files" >
      <file file_name="fet110_fll.c" Name="fet110_fll.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_fll.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="BasicClock MCLK configured with HF XTAL " >
    <folder Name="Source Files" >
      <file file_name="fet110_hfxtal.c" Name="fet110_hfxtal.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_hfxtal.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="BasicClock LPM3 Using WDT ISR, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_lpm3.c" Name="fet110_lpm3.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_lpm3.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0, CCR0 Contmode ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta01.c" Name="fet110_ta01.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta01.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0, CCR0 upmode ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta02.c" Name="fet110_ta02.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta02.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0, overflow ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta03.c" Name="fet110_ta03.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta03.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0, overflow ISR, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta04.c" Name="fet110_ta04.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta04.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0, CCR0 upmode ISR, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta05.c" Name="fet110_ta05.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta05.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0, CCR1 Contmode ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta06.c" Name="fet110_ta06.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta06.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0-3 CCRx Contmode ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta07.c" Name="fet110_ta07.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta07.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0-3 CCRx Contmode ISR, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta08.c" Name="fet110_ta08.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta08.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0-3 CCRx Contmode ISR, HF XTAL ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta09.c" Name="fet110_ta09.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta09.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.1 With TA0 upmode, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta10.c" Name="fet110_ta10.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta10.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.1 With TA0 upmode, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta11.c" Name="fet110_ta11.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta11.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.1 With TA0 upmode, HF XTAL ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta12.c" Name="fet110_ta12.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta12.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.1 With TA0 up-downmode, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta13.c" Name="fet110_ta13.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta13.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.1 With TA0 up-downmode, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta14.c" Name="fet110_ta14.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta14.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.1 With TA0 up-downmode, HF XTAL ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta15.c" Name="fet110_ta15.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta15.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A PWM TA1-2 upmode, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta_pwm01.c" Name="fet110_ta_pwm01.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta_pwm01.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A PWM TA1-2 upmode, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta_pwm02.c" Name="fet110_ta_pwm02.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta_pwm02.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A PWM TA1-2 upmode, HFTAL ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta_pwm03.c" Name="fet110_ta_pwm03.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta_pwm03.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A PWM TA1-2 up-downmode, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta_pwm04.c" Name="fet110_ta_pwm04.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta_pwm04.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A PWM TA1-2 up-downmode, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta_pwm05.c" Name="fet110_ta_pwm05.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta_pwm05.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A PWM TA1-2 up-downmode, HFTAL ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta_pwm06.c" Name="fet110_ta_pwm06.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta_pwm06.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A UART 2400 Ultra-low Power Echo, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta_uart2400.c" Name="fet110_ta_uart2400.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta_uart2400.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A UART 9600 Echo, HF XTAL ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta_uart9600.c" Name="fet110_ta_uart9600.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta_uart9600.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A UART 115200 Echo, HF XTAL ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta_uart115k.c" Name="fet110_ta_uart115k.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta_uart115k.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="WDT Toggle P1.0 Interval overflow ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_wdt01.c" Name="fet110_wdt01.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_wdt01.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="WDT Toggle P1.0 Interval overflow ISR, 32kHz ACLK    " >
    <folder Name="Source Files" >
      <file file_name="fet110_wdt02.c" Name="fet110_wdt02.c" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_wdt02.hzx" project_type="Executable" Name="Common" />
  </project>
  <configuration Name="Debug" />
  <configuration build_debug_information="No" Name="Release" build_optimize_output="Yes" />
</solution>
