<!DOCTYPE CrossStudio_Project_File>
<solution version="1" Name="msp430x110" >
  <configuration Target="MSP430F1121A" linker_memory_map_file="$(StudioDir)/targets/MSP430F1121A.xml" link_include_standard_libraries="No" link_include_startup_code="No" Name="Common" build_use_hardware_multiplier="No" />
  <project Name="Software Toggle P1.0 " >
    <folder Name="Source Files" >
      <file file_name="fet_1.s43" Name="fet_1.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet_1.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Software SPI Interface With TLV0831 " >
    <folder Name="Source Files" >
      <file file_name="fet110_0831.s43" Name="fet110_0831.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_0831.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Software SPI Interface TLC549 Set P1.0 if > 0.5*Vcc " >
    <folder Name="Source Files" >
      <file file_name="fet110_549.s43" Name="fet110_549.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_549.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Software SPI Interface to TLV5616 12-bit DAC " >
    <folder Name="Source Files" >
      <file file_name="fet110_5616.s43" Name="fet110_5616.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_5616.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="5Timers + 2 Clock Outputs 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_5timers.s43" Name="fet110_5timers.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_5timers.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Software Interface to Read ADS7822 " >
    <folder Name="Source Files" >
      <file file_name="fet110_7822.s43" Name="fet110_7822.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_7822.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Comp_A Output Comparator_A reference voltages on P2.3 " >
    <folder Name="Source Files" >
      <file file_name="fet110_ca01.s43" Name="fet110_ca01.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ca01.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Comp_A Detect Theashold, Set P1.0 if P2.3 > 0.25*Vcc " >
    <folder Name="Source Files" >
      <file file_name="fet110_ca02.s43" Name="fet110_ca02.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ca02.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Comp_A Slope ADC to Detect Temp Level Set P1.0 > 25c " >
    <folder Name="Source Files" >
      <file file_name="fet110_ca_temp1.s43" Name="fet110_ca_temp1.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ca_temp1.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Comp_A Thermometer 0 - 99 F " >
    <folder Name="Source Files" >
      <file file_name="fet110_ca_temp2.s43" Name="fet110_ca_temp2.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ca_temp2.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Software Interface with CD4511 7-Segment Decoder " >
    <folder Name="Source Files" >
      <file file_name="fet110_cd4511.s43" Name="fet110_cd4511.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_cd4511.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="BasicClock Output buffered SMCLK, ACLK and MCLK/12 " >
    <folder Name="Source Files" >
      <file file_name="fet110_clks.s43" Name="fet110_clks.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_clks.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Flash In-System Programming " >
    <folder Name="Source Files" >
      <file file_name="fet110_flash_write.s43" Name="fet110_flash_write.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_flash_write.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="BasicClock Implement Auto RSEL SW FLL " >
    <folder Name="Source Files" >
      <file file_name="fet110_fll.s43" Name="fet110_fll.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_fll.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Software Parellel Interface with HC138 " >
    <folder Name="Source Files" >
      <file file_name="fet110_hc138.s43" Name="fet110_hc138.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_hc138.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Software SPI Interface with HC164 Shift Register " >
    <folder Name="Source Files" >
      <file file_name="fet110_hc164.s43" Name="fet110_hc164.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_hc164.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Software SPI Interface with HC165 Shift Register " >
    <folder Name="Source Files" >
      <file file_name="fet110_hc165.s43" Name="fet110_hc165.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_hc165.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Software SPI Interface with HC595 Shift Register " >
    <folder Name="Source Files" >
      <file file_name="fet110_hc595.s43" Name="fet110_hc595.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_hc595.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="BasicClock MCLK configured with HF XTAL " >
    <folder Name="Source Files" >
      <file file_name="fet110_hfxtal.s43" Name="fet110_hfxtal.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_hfxtal.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Software Port Interrupt Service on P2.0 " >
    <folder Name="Source Files" >
      <file file_name="fet110_int_P2.s43" Name="fet110_int_P2.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_int_P2.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="BasicClock LPM3 Using WDT Interrupt, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_lpm3.s43" Name="fet110_lpm3.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_lpm3.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="BasicClock LPM4, Pulse P1.0 on P2.0_ISR " >
    <folder Name="Source Files" >
      <file file_name="fet110_lpm4.s43" Name="fet110_lpm4.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_lpm4.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Software Poll P2.0, Set P1.0 if P2.0 = 1 " >
    <folder Name="Source Files" >
      <file file_name="fet110_poll_P2.s43" Name="fet110_poll_P2.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_poll_P2.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Software Output 6-bit R2R DAC " >
    <folder Name="Source Files" >
      <file file_name="fet110_r2r.s43" Name="fet110_r2r.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_r2r.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Ultra-low Power 1200hz detect, ACLK +/- 5% " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta_cap01.s43" Name="fet110_ta_cap01.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta_cap01.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Ultra-low Power 1800hz detect, SMCLK +/- 1% " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta_cap02.s43" Name="fet110_ta_cap02.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta_cap02.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0, CCR0 Contmode ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta01.s43" Name="fet110_ta01.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta01.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0, CCR0 upmode ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta02.s43" Name="fet110_ta02.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta02.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0, overflow ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta03.s43" Name="fet110_ta03.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta03.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0, overflow ISR, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta04.s43" Name="fet110_ta04.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta04.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0, CCR0 upmode ISR, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta05.s43" Name="fet110_ta05.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta05.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0, CCR1 Contmode ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta06.s43" Name="fet110_ta06.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta06.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0-3, CCRx Contmode ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta07.s43" Name="fet110_ta07.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta07.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0-3, CCRx ISR Contmode, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta08.s43" Name="fet110_ta08.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta08.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.0-3, CCRx ISR Contmode, HF XTAL ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta09.s43" Name="fet110_ta09.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta09.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.1 With TA0 upmode, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta10.s43" Name="fet110_ta10.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta10.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.1 With TA0 upmode, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta11.s43" Name="fet110_ta11.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta11.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.1 With TA0 upmode, HF XTAL ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta12.s43" Name="fet110_ta12.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta12.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.1 With TA0 up-downmode, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta13.s43" Name="fet110_ta13.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta13.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.1 With TA0 up-downmode, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta14.s43" Name="fet110_ta14.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta14.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Toggle P1.1 With TA0 up-downmode, HF XTAL ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta15.s43" Name="fet110_ta15.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta15.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A Output 40khz square wave, UpMode SMCLK DCO " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta_40k.s43" Name="fet110_ta_40k.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta_40k.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A PWM TA1-2 upmode, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta_pwm01.s43" Name="fet110_ta_pwm01.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta_pwm01.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A PWM TA1-2 upmode, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta_pwm02.s43" Name="fet110_ta_pwm02.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta_pwm02.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A PWM TA1-2 upmode, HFTAL ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta_pwm03.s43" Name="fet110_ta_pwm03.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta_pwm03.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A PWM TA1-2 up-downmode, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta_pwm04.s43" Name="fet110_ta_pwm04.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta_pwm04.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A PWM TA1-2 up-downmode, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta_pwm05.s43" Name="fet110_ta_pwm05.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta_pwm05.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A PWM TA1-2 up-downmode, HFTAL ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta_pwm06.s43" Name="fet110_ta_pwm06.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta_pwm06.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A UART 2400 Ultra-low Power Echo, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta_uart2400.s43" Name="fet110_ta_uart2400.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta_uart2400.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A UART 9600 Echo, HF XTAL ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta_uart9600.s43" Name="fet110_ta_uart9600.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta_uart9600.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="Timer_A UART 115200 Echo, HF XTAL ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_ta_uart115k.s43" Name="fet110_ta_uart115k.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_ta_uart115k.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="WDT Toggle P1.0 Interval overflow ISR, DCO SMCLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_wdt01.s43" Name="fet110_wdt01.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_wdt01.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="WDT Toggle P1.0 Interval overflow ISR, 32kHz ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_wdt02.s43" Name="fet110_wdt02.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_wdt02.hzx" project_type="Executable" Name="Common" />
  </project>
  <project Name="WDT Toggle P1.0 Interval overflow ISR, HF XTAL ACLK " >
    <folder Name="Source Files" >
      <file file_name="fet110_wdt03.s43" Name="fet110_wdt03.s43" />
      <configuration filter="c;h;s;asm;inc;s43" Name="Common" />
    </folder>
    <configuration build_output_file_name="$(OutDir)/fet110_wdt03.hzx" project_type="Executable" Name="Common" />
  </project>
  <configuration Name="Debug" />
  <configuration build_debug_information="No" Name="Release" build_optimize_output="Yes" />
</solution>
