##### Synopsis

    #include <inmsp.h>
    unsigned long long __bcd_add_long_long(unsigned long long x, unsigned long long y);

##### Description

__bcd_add_long_long adds x to y using decimal arithmetic. Both x and y must be binary coded decimal numbers and the result is a binary coded decimal number.

__bcd_add_long_long is an intrinsic function and produces inline code.

##### Portability

__bcd_add_long_long can be used on any MSP430 device.