This section describes the steps needed to install your Elprotronic PE010X01-02 or PE010X01-04 JTAG or JTAG/BSL programming adapter so that CrossStudio can use it.

###### Installing the Drivers

Download and install the drivers necessary for the programming adapter from Elprotronics’s web site using this link:

http://www.elprotronic.com/Support.asp

Please note that the PE010X01-0x programming adapters are only supported on Windows operating systems. Once you have installed the drivers, you can integrate support for the PE010X01-0x adapter as described below.

###### Configuring CrossStudio for the PE010X01-0x

In this section we will assume that you have installed the PE010X01-0x software in the default directory “C:\Program Files\Elprotronic\USB MSP430 Flash Programmer”.

Set up the required files so CrossStudio can use them:

1. Copy the file MSP430DLL\MSP430.DLL from the Elprotronic installation directory into the CrossStudio bin directory as PEFPA.DLL so that it does not overwrite the existing MSP430.DLL file which is TI's parallel port FET driver.

Now that the files are copied, you can create a target interface that will use these DLLs.

1. Show the targets window using View > Targets.
2. In the Targets window, right click the empty part of the list view.
3. From the popup menu, click New Target Interface then Flash Emulation Tool (TI Driver).

You will see that a new Flash Emulation Tool target appears as the last entry in the target window. Next, rename the target interface to make it more easily recognizable:

1. Right click the new Flash Emulation Tool target interface
2. From the popup menu, select Rename.
3. Type “Elprotronic PE010X01-0x Programmer” into the text entry box.

Next, use the Elprotronic PE010X01-0x DLL rather than the TI parallel port DLL for this interface:

1. Right click the Elprotronic PE010X01-0x Programmer target interface.
2. From the popup menu, select Properties.
3. In the Properties window, select the Target Driver DLL Path property in the Connection group.
4. Change the property from “$(StudioDir)/bin/msp430.dll” to “$(StudioDir)/bin/pefpa.dll”.

You are now ready to use the Elprotronic PE010X01-0x target interface to program and debug your applications.

###### Useful web links

- Elprotronic's web site, s.