The USB CrossConnect target interface provides access to MSP430 targets through Rowley Associates' CrossConnect for MSP430 device. This target interface supports program loading and debugging.

###### Connection property group

Enable Regulator
  Specifies whether the regulator is enabled when the target is connected.
Identify
  If set the device will be identified on connect. If not set the Target project property setting of the current project in the current build configuration will be used.
Operating Voltage
  The operating voltage of the target.
Release JTAG
  Release the JTAG signals when Reset, Start Without Debugging or Stop Debugging is used.
Serial Number
  The serial number of the currently connected USB CrossConnect device.
Use Serial Number
  The serial number of the USB CrossConnect you want to connect to. If multiple USB CrossConnects are connected to your system, this property allows you to specify which one to use. If no serial number is specified, the first available CrossConnect will be used.

###### Current property group

Device Type
  The identified device type.

###### Emulation property group

Clock Control
  The level of debug clock control supported by the device.
Emulation Level
  The debug capabilities supported by the device.

###### Loader property group

Erase All
  If true erase all memory. If false just erase the pages that are to be programmed.
FLASH Block Write Enabled
  If set to Yes, the flash is programmed in block mode rather than word mode. Block mode flashing is approximately twice as fast as word mode programming.
Verify FLASH Erase
  If set to Yes, FLASH memory will be checked after an erase to determine if operation has succeeded.
Verify FLASH Writes
  If set to Yes, FLASH memory will be checked after a write to determine if operation has succeded.