Node:MN10200 Options, Next:MN10300 Options, Previous:ARM Options, Up:Submodel Options

#### MN10200 Options

These `-m` options are defined for Matsushita MN10200 architectures:

`-mrelax`
  Indicate to the linker that it should perform a relaxation optimization pass to shorten branches, calls and absolute memory addresses. This option only has an effect when used on the command line for the final link step.

  This option makes symbolic debugging impossible.