##### Synopsis

    #include <__armlib.h>
    void __ARMLIB_disableFIQ(void);

##### Description

__ARMLIB_disableFIQ globally disables the ARM's FIQ interrupts by setting the F bit of the CPSR register.

##### Portability

__ARMLIB_disableFIQ is an ARM specific extension provided by CrossWorks C.

##### See also

__ARMLIB_enableFIQ __ARMLIB_enableIRQ __ARMLIB_disableIRQ __ARMLIB_isrEnableIRQ __ARMLIB_isrDisableIRQ