##### Synopsis

    #include <__armlib.h>
    void __ARMLIB_isrDisableIRQ(void);

##### Description

__ARMLIB_isrDisableIRQ re-disables the ARM's global interrupts from within an ISR.

__ARMLIB_isrDisableIRQ should only be called after a previous call to __ARMLIB_isrEnableIRQ.

##### Portability

__ARMLIB_isrDisableIRQ is an ARM specific extension provided by CrossWorks C.

##### See also

__ARMLIB_enableIRQ __ARMLIB_disableIRQ __ARMLIB_isrEnableIRQ