Node: M68K-Directives, Next: M68K-opcodes, Previous: M68K-Float, Up: M68K-Dependent

### 680x0 Machine Directives

In order to be compatible with the Sun assembler the 680x0 assembler understands the following directives.

`.data1`
  This directive is identical to a `.data 1` directive.
`.data2`
  This directive is identical to a `.data 2` directive.
`.even`
  This directive is a special case of the `.align` directive; it aligns the output to an even byte boundary.
`.skip`
  This directive is identical to a `.space` directive.