The GCC used in this version of CrossStudio for ARM is made up of the following packages:

- binutils-2.13-021227
- gcc-3.3-021223 - The build of GCC used has been slightly modified from the standard arm-elf build so that software VFP floating point support is enabled by default. This is to allow the CrossWorks C floating point library to work as it expects floating point doubles to be in target endian format.

The packages were built for Windows using MinGW.

- AS Assembler Documentation
- GCC Compiler Documentation
- CPP C Preprocessor Documentation
- LD Linker Documentation
- BINUTILS Utilities Documentation