The Debug Control menu provides commands to control how you debug your program. The Debug Control menu is a submenu of the Debug menu.

###### The Debug Control menu

###### Debug Control commands

Menu command | Keystroke | Description
Source Mode | Ctrl+T, S | Switches the debugger into Source Debugging mode where code is stepped a statement at a time.
Interleaved Mode | Ctrl+T, I | Switches the debugger into Interleaved Debugging mode where code is stepped one instruction at a time and source code is intermixed with the generated assembly code.
Assembly Mode | Ctrl+T, A | Switches the debugger into Assembly Debugging mode where code is stepped one instruction at a time with a simple disassembly of memory.
Toggle Debug Mode | Ctrl+F11 | Toggles between Source Debugging and Interleaved Debugging modes.
Enable Interrupt Processing | Ctrl+T, N | Enables global interrupts in the processor by writing to the appropriate register.
Disable Interrupt Processing | Ctrl+T, X | Disables global interrupts in the processor by writing to the appropriate register.
Start Cycle Counter |  | Restarts the cycle counter after it has been paused.
Pause Cycle Counter |  | Pauses the cycle counter so that it does not incremement and count cycles even though code executes.
Reset Cycle Counter |  | Resets the cycle counter to zero.