##### Syntax

-F fmt

##### Description

The -F option sets the output format to fmt. The supported output formats are:

- -Fsrec Motorola S-record format
- -Fhex Intel extended hex format
- -Ftek Tektronix hex format
- -Ttxt Texas Instruments hex format
- -Flst Hexadecimal listing

##### Example

    hex app.hzx -Ftxt -o app

This reads the application file app.hzx and writes all sections in Texas Instruments hex format to app.txt.