##### Synopsis

    #include <inmsp.h>
    unsigned __bcd_subtract_short(unsigned x, unsigned y);

##### Description

__bcd_subtract_short subtracts y from x using decimal arithmetic. Both x and y must be binary coded decimal numbers and the result is a binary coded decimal number.

__bcd_subtract_short is an intrinsic function and produces inline code.

##### Portability

__bcd_subtract_short can be used on any MSP430 device.